Archive member included because of file (symbol)

c:/program files/microchip/mplab c30/bin/bin/../../lib\libpic30-coff.a(crt1.o)
                              (_resetALT)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libpic30-coff.a(crt0.o)
                              (_resetPRI)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(udivsi3.o)
                              ..\Microchip\MDD File System\Objects - PIC24F Starter Kit\FSIO.o (__udivsi3)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(malloc.o)
                              ..\Microchip\Usb\Objects - PIC24F Starter Kit\usb_host.o (malloc)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(free.o)
                              ..\Microchip\Usb\Objects - PIC24F Starter Kit\usb_host.o (free)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(tolower.os)
                              ..\Microchip\MDD File System\Objects - PIC24F Starter Kit\FSIO.o (tolower)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memset.o)
                              ..\Microchip\MDD File System\Objects - PIC24F Starter Kit\FSIO.o (memset)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strncpy.o)
                              ..\Microchip\MDD File System\Objects - PIC24F Starter Kit\FSIO.o (strncpy)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(toupper.os)
                              ..\Microchip\MDD File System\Objects - PIC24F Starter Kit\FSIO.o (toupper)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strlen.o)
                              ..\Microchip\MDD File System\Objects - PIC24F Starter Kit\FSIO.o (strlen)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strcpy.o)
                              ..\Microchip\MDD File System\Objects - PIC24F Starter Kit\FSIO.o (strcpy)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strchr.o)
                              ..\Microchip\MDD File System\Objects - PIC24F Starter Kit\FSIO.o (strchr)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strcat.o)
                              Objects - PIC24F Starter Kit\PIC24F Starter Kit.o (strcat)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strcmp.o)
                              Objects - PIC24F Starter Kit\PIC24F Starter Kit.o (strcmp)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(sprintf.io)
                              Objects - PIC24F Starter Kit\Demos.o (_isprintf)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strncmp.o)
                              Objects - PIC24F Starter Kit\Flash.o (strncmp)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(srand.o)
                              Objects - PIC24F Starter Kit\Games.o (srand)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(rand.o)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(srand.o) (_Tls_setup__Randseed)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xgetmem.o)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(malloc.o) (_Getmem)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memcpy.o)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(sprintf.io) (memcpy)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xprintf.io)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(sprintf.io) (__iPrintf)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xvacopy.o)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xprintf.io) (_Vacopy)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xputfld.io)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xprintf.io) (__iPutfld)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xputtxt.o)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xprintf.io) (_Puttxt)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xlitob.o)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xputfld.io) (_Litob)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memchr.o)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xputfld.io) (memchr)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libpic30-coff.a(sbrk.o)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xgetmem.o) (sbrk)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libpic30-coff.a(brk.o)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libpic30-coff.a(sbrk.o) (brk)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(mulsi3.o)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(rand.o) (__mulsi3)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(divmoddi3.o)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xlitob.o) (__udivdi3)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(muldi3.o)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xlitob.o) (__muldi3)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(umuldi3.o)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(muldi3.o) (__umuldi3)


Program Memory Usage

section                    address   length (PC units)   length (bytes) (dec)
-------                    -------   -----------------   --------------------
.reset                           0                 0x4             0x6  (6)
.ivt                           0x4                0xfc           0x17a  (378)
.aivt                        0x104                0xfc           0x17a  (378)
.text                        0x200               0xdea          0x14df  (5343)
.const                       0xfea               0xc0a          0x120f  (4623)
.text                       0x1bf4             0x132aa         0x1cbff  (117759)
C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn8   0x14e9e               0x40a           0x60f  (1551)
C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn9   0x152a8               0x40a           0x60f  (1551)
.text                      0x156b2               0x97a           0xe37  (3639)
.dinit                     0x1602c               0x1c0           0x2a0  (672)
C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn7   0x161ec                0x2a            0x3f  (63)
C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn6   0x16216                0x1e            0x2d  (45)
C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn1   0x16234                0x12            0x1b  (27)
C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn2   0x16246                0x12            0x1b  (27)
C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn3   0x16258                0x12            0x1b  (27)
C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn4   0x1626a                0x12            0x1b  (27)
C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn5   0x1627c                0x12            0x1b  (27)
C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn10   0x1628e                0x12            0x1b  (27)
C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn11   0x162a0                0x12            0x1b  (27)
C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn12   0x162b2                0x12            0x1b  (27)
__CONFIG2                  0x2abfc                 0x2             0x3  (3)
__CONFIG1                  0x2abfe                 0x2             0x3  (3)

                     Total program memory used (bytes):        0x21426  (136230) 51%


Data Memory Usage

section                    address      alignment gaps    total length  (dec)
-------                    -------      --------------    -------------------
.nbss                        0x800                   0           0x8ec  (2284)
_02b7193048f67891           0x10ec                   0           0x200  (512)
_02b71a8048f67891           0x12ec                   0           0x200  (512)
.nbss                       0x14ec                   0           0x24e  (590)
_0207177048f678a6           0x173a                   0            0x3a  (58)
.nbss                       0x1774                   0            0x6a  (106)
.ndata                      0x17de                   0            0x30  (48)
.nbss                       0x180e                   0            0x4c  (76)
.ndata                      0x185a                   0            0x1e  (30)
.nbss                       0x1878                   0            0x2c  (44)
.ndata                      0x18a4                   0            0x12  (18)
.ndata                      0x18b6                   0            0x38  (56)
.nbss                       0x18ee                   0            0x12  (18)
.ndata                      0x1900                   0            0x18  (24)
.nbss                       0x1918                   0             0xc  (12)
.ndata                      0x1924                   0             0xa  (10)
.nbss                       0x192e                   0            0x12  (18)
.ndata                      0x1940                   0             0x8  (8)
.nbss                       0x1948                   0            0x12  (18)
.ndata                      0x195a                   0             0x6  (6)
.nbss                       0x1960                   0             0x2  (2)
.ndata                      0x1962                   0             0x2  (2)
.nbss                       0x1964                   0             0x2  (2)
.bss                        0x1966                   0            0x88  (136)
.data                       0x19ee                   0            0x12  (18)
_02cdbaf048f67890           0x1a00                   0            0x10  (16)
.data                       0x1a10                   0            0x22  (34)
.data                       0x1a32                   0             0xa  (10)
.dconst                     0x1a3c                   0             0x8  (8)
.data                       0x1a44                   0             0x6  (6)

                        Total data memory used (bytes):         0x124a  (4682) 28%


Dynamic Memory Usage

region                     address                      maximum length  (dec)
------                     -------                      ---------------------
heap                        0x1a4a                               0x400  (1024)
stack                       0x1e4a                              0x29b6  (10678)

                        Maximum dynamic memory (bytes):         0x2db6  (11702)


External Symbols in Data Memory (by address):

                    0x0802                  _captureFile
                    0x0804                  _graphData
                    0x0882                  _graphDataHead
                    0x0884                  _graphDataTail
                    0x0886                  _graphOffset
                    0x0888                  _graphUpdateRate
                    0x088a                  _logBufferReading
                    0x088b                  _logBufferWriting
                    0x088c                  _logData
                    0x0c94                  _potADC
                    0x0c98                  _gamesGrid
                    0x0c9a                  _pScore
                    0x0c9c                  _score
                    0x0c9e                  _scoreText
                    0x0cb2                  _scoreInfo
                    0x0ccc                  _asteroid
                    0x0d0e                  _bullet
                    0x0d1c                  _pShip
                    0x0d1e                  _balls
                    0x0d2a                  _ballsRemoved
                    0x0d2c                  _columnsRemoved
                    0x0d2e                  _lastSelectedColumn
                    0x0d30                  _lastSelectedRow
                    0x0d32                  _lastBall
                    0x0d34                  _lastBallCount
                    0x0d36                  _selectionMarked
                    0x0d38                  _defaultDirection
                    0x0d3a                  _field
                    0x0e8a                  _snake
                    0x10ec                  _gDataBuffer
                    0x12ec                  _gFATBuffer
                    0x14ec                  _gFileArray
                    0x1558                  _gFileSlotOpen
                    0x155a                  _gTimeCrtMS
                    0x155c                  _gTimeCrtTime
                    0x155e                  _gTimeCrtDate
                    0x1560                  _gTimeAccDate
                    0x1562                  _gTimeWrtTime
                    0x1564                  _gTimeWrtDate
                    0x1566                  _FatRootDirClusterValue
                    0x156a                  _BytesPerSec
                    0x156c                  _FAT32_BkBootSector
                    0x156e                  _FAT32_FSInfo
                    0x1570                  _TempClusterCalc
                    0x1574                  _Index
                    0x1575                  _dirCleared
                    0x1576                  _dotdot
                    0x157a                  _tempCWDobj
                    0x15b0                  _gFileTemp
                    0x15e6                  _cwd
                    0x161c                  _gDiskData
                    0x163a                  _defaultString
                    0x1645                  _defaultArray
                    0x1654                  _pageInformation
                    0x16f0                  _displayChangeTime
                    0x16f4                  _previousSecond
                    0x16f6                  _pScheme
                    0x1728                  __lineType
                    0x172a                  __lineThickness
                    0x172c                  __cursorX
                    0x172e                  __cursorY
                    0x1730                  __fontOrientation
                    0x1732                  __font
                    0x1734                  __fontFirstChar
                    0x1736                  __fontLastChar
                    0x1738                  __fontHeight
                    0x173a                  _deviceInfoMSD
                    0x1774                  _buttons
                    0x1776                  _rawCTMU
                    0x1780                  _average
                    0x178a                  _trip
                    0x1794                  _hyst
                    0x179e                  _first
                    0x179f                  _buttonIndex
                    0x17a0                  _value
                    0x17a2                  _bigVal
                    0x17a4                  _smallAvg
                    0x17a6                  _AvgIndex
                    0x17a8                  _buttonsPrevious
                    0x17aa                  _calibrationState
                    0x17ac                  _countCTMU
                    0x17ae                  _currentTouchpad
                    0x17b0                  _stateTick
                    0x17b4                  _sumCTMUPressed
                    0x17c8                  _sumCTMUReleased
                    0x17dc                  _currentControlSet
                    0x17de                  _daysPerMonth
                    0x17ea                  _monthNames
                    0x180e                  _mediaPresent
                    0x1810                  _pFlashFiles
                    0x1812                  _pSlider
                    0x1814                  _usbErrorCode
                    0x1815                  _usbErrorText
                    0x182a                  _volume
                    0x1838                  _countConfigurations
                    0x1839                  _numCommandTries
                    0x183a                  _numEnumerationTries
                    0x183c                  _numTimerInterrupts
                    0x183e                  _pCurrentEndpoint
                    0x1840                  _usbBusInfo
                    0x1848                  _usbDeviceInfo
                    0x1854                  _usbHostState
                    0x1856                  _usbOverrideHostState
                    0x1858                  _usbRootHubInfo
                    0x185a                  _scoreSize
                    0x1860                  _scoreSpeed
                    0x1866                  _scoreTable
                    0x187e                  __rpnlX1
                    0x1880                  __rpnlY1
                    0x1882                  __rpnlX2
                    0x1884                  __rpnlY2
                    0x1886                  __rpnlR
                    0x1888                  __rpnlFaceColor
                    0x188a                  __rpnlEmbossLtColor
                    0x188c                  __rpnlEmbossDkColor
                    0x188e                  __rpnlEmbossSize
                    0x18a4                  _gLastFATSectorRead
                    0x18a8                  _gNeedFATWrite
                    0x18aa                  _gBufferOwner
                    0x18ac                  _gLastDataSectorRead
                    0x18b0                  _gNeedDataWrite
                    0x18b1                  _nextClusterIsLast
                    0x18b2                  _gBufferZeroed
                    0x18b3                  _recache
                    0x18b4                  _cwdptr
                    0x18b6                  __time_str
                    0x18c6                  __date_str
                    0x18d6                  _usbMediaInterfaceTable
                    0x18de                  _usbClientDrvTable
                    0x18e6                  _usbTPL
                    0x18ee                  __time
                    0x18f6                  __time_chk
                    0x18fe                  __rtcc_flag
                    0x1900                  _pConfigurationDescriptorList
                    0x1902                  _pCurrentConfigurationDescriptor
                    0x1904                  _pDeviceDescriptor
                    0x1906                  _pEndpointList
                    0x1908                  _pEP0Data
                    0x190a                  _pInterfaceList
                    0x190c                  __cosine
                    0x1918                  __color
                    0x191a                  __clipRgn
                    0x191c                  __clipLeft
                    0x191e                  __clipTop
                    0x1920                  __clipRight
                    0x1922                  __clipBottom
                    0x1924                  _previousTick
                    0x1928                  _screenState
                    0x192a                  _tick
                    0x1940                  __pGolObjects
                    0x1942                  __pDefaultGolScheme
                    0x1944                  __pObjectFocused
                    0x1946                  __pRpnlBitmap
                    0x195a                  _dCBWTagNext
                    0x1962                  _deviceAddress
                    0x1963                  _maxLUN
                    0x1964                  ___curbrk
                    0x1a00                  _BDT
                    0x1a32                  __Tls_setup__Randseed
                    0x1a34                  __Randseed
                    0x1a38                  __Tls_setup__Randinit
                    0x1a3a                  __Randinit
                    0x1a44                  __Size_block
                    0x1a46                  __Aldata

External Symbols in Data Memory (by name):

                    0x17a6                  _AvgIndex
                    0x1a00                  _BDT
                    0x156a                  _BytesPerSec
                    0x156c                  _FAT32_BkBootSector
                    0x156e                  _FAT32_FSInfo
                    0x1566                  _FatRootDirClusterValue
                    0x1574                  _Index
                    0x1570                  _TempClusterCalc
                    0x1a46                  __Aldata
                    0x1a3a                  __Randinit
                    0x1a34                  __Randseed
                    0x1a44                  __Size_block
                    0x1a38                  __Tls_setup__Randinit
                    0x1a32                  __Tls_setup__Randseed
                    0x1964                  ___curbrk
                    0x1922                  __clipBottom
                    0x191c                  __clipLeft
                    0x191a                  __clipRgn
                    0x1920                  __clipRight
                    0x191e                  __clipTop
                    0x1918                  __color
                    0x190c                  __cosine
                    0x172c                  __cursorX
                    0x172e                  __cursorY
                    0x18c6                  __date_str
                    0x1732                  __font
                    0x1734                  __fontFirstChar
                    0x1738                  __fontHeight
                    0x1736                  __fontLastChar
                    0x1730                  __fontOrientation
                    0x172a                  __lineThickness
                    0x1728                  __lineType
                    0x1942                  __pDefaultGolScheme
                    0x1940                  __pGolObjects
                    0x1944                  __pObjectFocused
                    0x1946                  __pRpnlBitmap
                    0x188c                  __rpnlEmbossDkColor
                    0x188a                  __rpnlEmbossLtColor
                    0x188e                  __rpnlEmbossSize
                    0x1888                  __rpnlFaceColor
                    0x1886                  __rpnlR
                    0x187e                  __rpnlX1
                    0x1882                  __rpnlX2
                    0x1880                  __rpnlY1
                    0x1884                  __rpnlY2
                    0x18fe                  __rtcc_flag
                    0x18ee                  __time
                    0x18f6                  __time_chk
                    0x18b6                  __time_str
                    0x0ccc                  _asteroid
                    0x1780                  _average
                    0x0d1e                  _balls
                    0x0d2a                  _ballsRemoved
                    0x17a2                  _bigVal
                    0x0d0e                  _bullet
                    0x179f                  _buttonIndex
                    0x1774                  _buttons
                    0x17a8                  _buttonsPrevious
                    0x17aa                  _calibrationState
                    0x0802                  _captureFile
                    0x0d2c                  _columnsRemoved
                    0x17ac                  _countCTMU
                    0x1838                  _countConfigurations
                    0x17dc                  _currentControlSet
                    0x17ae                  _currentTouchpad
                    0x15e6                  _cwd
                    0x18b4                  _cwdptr
                    0x195a                  _dCBWTagNext
                    0x17de                  _daysPerMonth
                    0x1645                  _defaultArray
                    0x0d38                  _defaultDirection
                    0x163a                  _defaultString
                    0x1962                  _deviceAddress
                    0x173a                  _deviceInfoMSD
                    0x1575                  _dirCleared
                    0x16f0                  _displayChangeTime
                    0x1576                  _dotdot
                    0x0d3a                  _field
                    0x179e                  _first
                    0x18aa                  _gBufferOwner
                    0x18b2                  _gBufferZeroed
                    0x10ec                  _gDataBuffer
                    0x161c                  _gDiskData
                    0x12ec                  _gFATBuffer
                    0x14ec                  _gFileArray
                    0x1558                  _gFileSlotOpen
                    0x15b0                  _gFileTemp
                    0x18ac                  _gLastDataSectorRead
                    0x18a4                  _gLastFATSectorRead
                    0x18b0                  _gNeedDataWrite
                    0x18a8                  _gNeedFATWrite
                    0x1560                  _gTimeAccDate
                    0x155e                  _gTimeCrtDate
                    0x155a                  _gTimeCrtMS
                    0x155c                  _gTimeCrtTime
                    0x1564                  _gTimeWrtDate
                    0x1562                  _gTimeWrtTime
                    0x0c98                  _gamesGrid
                    0x0804                  _graphData
                    0x0882                  _graphDataHead
                    0x0884                  _graphDataTail
                    0x0886                  _graphOffset
                    0x0888                  _graphUpdateRate
                    0x1794                  _hyst
                    0x0d32                  _lastBall
                    0x0d34                  _lastBallCount
                    0x0d2e                  _lastSelectedColumn
                    0x0d30                  _lastSelectedRow
                    0x088a                  _logBufferReading
                    0x088b                  _logBufferWriting
                    0x088c                  _logData
                    0x1963                  _maxLUN
                    0x180e                  _mediaPresent
                    0x17ea                  _monthNames
                    0x18b1                  _nextClusterIsLast
                    0x1839                  _numCommandTries
                    0x183a                  _numEnumerationTries
                    0x183c                  _numTimerInterrupts
                    0x1900                  _pConfigurationDescriptorList
                    0x1902                  _pCurrentConfigurationDescriptor
                    0x183e                  _pCurrentEndpoint
                    0x1904                  _pDeviceDescriptor
                    0x1908                  _pEP0Data
                    0x1906                  _pEndpointList
                    0x1810                  _pFlashFiles
                    0x190a                  _pInterfaceList
                    0x16f6                  _pScheme
                    0x0c9a                  _pScore
                    0x0d1c                  _pShip
                    0x1812                  _pSlider
                    0x1654                  _pageInformation
                    0x0c94                  _potADC
                    0x16f4                  _previousSecond
                    0x1924                  _previousTick
                    0x1776                  _rawCTMU
                    0x18b3                  _recache
                    0x0c9c                  _score
                    0x0cb2                  _scoreInfo
                    0x185a                  _scoreSize
                    0x1860                  _scoreSpeed
                    0x1866                  _scoreTable
                    0x0c9e                  _scoreText
                    0x1928                  _screenState
                    0x0d36                  _selectionMarked
                    0x17a4                  _smallAvg
                    0x0e8a                  _snake
                    0x17b0                  _stateTick
                    0x17b4                  _sumCTMUPressed
                    0x17c8                  _sumCTMUReleased
                    0x157a                  _tempCWDobj
                    0x192a                  _tick
                    0x178a                  _trip
                    0x1840                  _usbBusInfo
                    0x18de                  _usbClientDrvTable
                    0x1848                  _usbDeviceInfo
                    0x1814                  _usbErrorCode
                    0x1815                  _usbErrorText
                    0x1854                  _usbHostState
                    0x18d6                  _usbMediaInterfaceTable
                    0x1856                  _usbOverrideHostState
                    0x1858                  _usbRootHubInfo
                    0x18e6                  _usbTPL
                    0x17a0                  _value
                    0x182a                  _volume

External Symbols in Program Memory (by address):

                  0x000200                  __resetPRI
                  0x00021e                  __psv_init
                  0x00022e                  __data_init
                  0x00029c                  _malloc
                  0x000340                  _free
                  0x0003a8                  _tolower
                  0x0003b6                  _memset
                  0x0003c4                  _strncpy
                  0x0003ea                  _toupper
                  0x0003f8                  _strlen
                  0x000406                  _strcpy
                  0x000416                  _strchr
                  0x000428                  _strcat
                  0x000446                  _strcmp
                  0x00046a                  sprintf.io:_prout
                  0x000476                  __isprintf
                  0x000498                  _strncmp
                  0x0004bc                  _srand
                  0x0004de                  _rand
                  0x000588                  __Getmem
                  0x000596                  _memcpy
                  0x0005a4                  ___iPrintf
                  0x000716                  __Vacopy
                  0x000720                  ___iPutfld
                  0x0009a6                  __Puttxt
                  0x000b3a                  __Litob
                  0x000caa                  _memchr
                  0x000d08                  ___udivsi3
                  0x000d28                  ___mulsi3
                  0x000d5a                  ___udivmoddi3
                  0x000e28                  ___udivdi3
                  0x000e36                  ___umoddi3
                  0x000e3e                  ___divdi3
                  0x000e78                  ___moddi3
                  0x000f4a                  ___muldi3
                  0x000fa6                  ___umuldi3
                  0x000fea                  _GOLFontDefault
                  0x000fee                  _L13579
                  0x001a86                  _mediaRequest
                  0x001b72                  _ballCircle
                  0x001b78                  _ballCross
                  0x001b7e                  _ballMarking
                  0x001b84                  _ballSquare
                  0x001b8a                  _ballTriangle
                  0x001b90                  _iconFolderSmall
                  0x001b96                  _iconMicrochip
                  0x001b9c                  _intro
                  0x001ba2                  _introDevice
                  0x001ba8                  _snakeBody
                  0x001bae                  _snakeFood
                  0x001bb4                  _snakeHead
                  0x001bf4                  _FSInit
                  0x001c8c                  _FILEfind
                  0x001e76                  _FILEopen
                  0x001f9c                  _FILEget_next_cluster
                  0x002074                  _DISKmount
                  0x0020b6                  _LoadMBR
                  0x002258                  _LoadBootSector
                  0x002460                  _FSformat
                  0x002b2c                  _Write_File_Entry
                  0x002bce                  _FAT_erase_cluster_chain
                  0x002ce0                  _Cache_File_Entry
                  0x002ec2                  _CreateFileEntry
                  0x002f2c                  _CreateFirstCluster
                  0x002fb8                  _FindEmptyEntries
                  0x0030cc                  _PopulateEntries
                  0x0031b4                  _CacheTime
                  0x00330a                  _FILEallocate_new_cluster
                  0x0033b2                  _FATfindEmptyCluster
                  0x0034b0                  _FSfclose
                  0x00357a                  _Fill_File_Object
                  0x0036d4                  _LoadDirAttrib
                  0x00375a                  _FILEerase
                  0x003816                  _FSrename
                  0x003cce                  _FSfopen
                  0x003f0c                  _FSftell
                  0x003f1a                  _FSremove
                  0x003fbc                  _FSrewind
                  0x003ff0                  _FileObjectCopy
                  0x004030                  _FILECreateHeadCluster
                  0x0040dc                  _EraseCluster
                  0x004168                  _Cluster2Sector
                  0x004210                  _FSfwrite
                  0x004488                  _flushData
                  0x0044e2                  _FSfeof
                  0x004506                  _FSfread
                  0x0046b2                  _FormatFileName
                  0x0047c6                  _ValidateChars
                  0x00488e                  _isShort
                  0x004946                  _isDIR
                  0x0049f2                  _FSfseek
                  0x004c16                  _ReadFAT
                  0x004fc2                  _WriteFAT
                  0x005426                  _FSchdir
                  0x005436                  _chdirhelper
                  0x0057d2                  _FSgetcwd
                  0x005b36                  _GetPreviousEntry
                  0x005cc8                  _FSmkdir
                  0x005cd8                  _mkdirhelper
                  0x005f32                  _CreateDIR
                  0x00602e                  _writeDotEntries
                  0x0061be                  _FSrmdir
                  0x0061d2                  _rmdirhelper
                  0x006628                  _eraseDir
                  0x0066b6                  _FormatDirName
                  0x006730                  _FindFirst
                  0x006990                  _FindNext
                  0x006b96                  _GetFullClusterNumber
                  0x006bbe                  _ReadByte
                  0x006bd0                  _ReadWord
                  0x006c04                  _ReadDWord
                  0x006c38                  _USBHostClearEndpointErrors
                  0x006c86                  _USBHostDeviceRequest
                  0x006d50                  _USBHostDeviceSpecificClientDriver
                  0x006d62                  _USBHostDeviceStatus
                  0x006db6                  _USBHostInit
                  0x006dfe                  _USBHostRead
                  0x006eae                  _USBHostResetDevice
                  0x006edc                  _USBHostResumeDevice
                  0x006f0a                  _USBHostSetDeviceConfiguration
                  0x006f4c                  _USBHostShutdown
                  0x006f7c                  _USBHostSuspendDevice
                  0x006faa                  _USBHostTasks
                  0x007b2e                  _USBHostTerminateTransfer
                  0x007b6c                  _USBHostTransferIsComplete
                  0x007c16                  _USBHostVbusEvent
                  0x007c52                  _USBHostWrite
                  0x007d02                  __USB_CheckCommandAndEnumerationAttempts
                  0x007d48                  __USB_FindClassDriver
                  0x007dc4                  __USB_FindDeviceLevelClientDriver
                  0x007eb2                  __USB_FindInterface
                  0x007ee6                  __USB_FindNextToken
                  0x0082c6                  __USB_FreeConfigMemory
                  0x008314                  __USB_FreeMemory
                  0x00835c                  __USB_InitControlRead
                  0x0083d8                  __USB_InitControlWrite
                  0x008462                  __USB_InitRead
                  0x0084ea                  __USB_InitWrite
                  0x008572                  __USB_NotifyClients
                  0x008670                  __USB_ParseConfigurationDescriptor
                  0x008986                  __USB_ResetDATA0
                  0x0089b4                  __USB_SendToken
                  0x008a08                  __USB_SetBDT
                  0x008b5c                  __USB_TransferInProgress
                  0x008b88                  __USB1Interrupt
                  0x009052                  _InitializeRandomNumberGenerator
                  0x009068                  _ProcessMessageGames
                  0x0090e4                  _ProcessMessageScore
                  0x0090f6                  _Random
                  0x00911e                  _ShowScreenGames
                  0x009172                  _ShowScreenScore
                  0x009208                  _TranslateMessageScore
                  0x00922c                  _DrawBlaster
                  0x009be0                  _FindNextPosition
                  0x009db0                  _ProcessMessageBlaster
                  0x009e40                  _ShowScreenBlaster
                  0x009eea                  _TranslateMessageBlaster
                  0x009f84                  _CompactHorizontal
                  0x00a05e                  _CompactVertical
                  0x00a10e                  _FindBallNumber
                  0x00a15c                  _MarkAllNeighbors
                  0x00a252                  _MovesRemaining
                  0x00a32c                  _ProcessMessageShapelet
                  0x00a4ea                  _ShowScreenShapelet
                  0x00a5ba                  _TranslateMessageShapelet
                  0x00a5d2                  _DrawSnake
                  0x00a97a                  _ProcessMessageSnake
                  0x00a9ea                  _ShowScreenSnake
                  0x00ab78                  _TranslateMessageSnake
                  0x00abf8                  _USBHostMSDDeviceStatus
                  0x00accc                  _USBHostMSDResetDevice
                  0x00ad88                  _USBHostMSDTasks
                  0x00ba3c                  _USBHostMSDTerminateTransfer
                  0x00bade                  _USBHostMSDTransfer
                  0x00bd6e                  _USBHostMSDTransferIsComplete
                  0x00be4a                  _USBHostMSDInitialize
                  0x00bfec                  _USBHostMSDEventHandler
                  0x00c08c                  __USBHostMSD_GetNextTag
                  0x00c0a2                  __USBHostMSD_ResetStateJump
                  0x00c160                  _AdjustColorPWM
                  0x00c19a                  _CaptureMonitorMedia
                  0x00c2dc                  _DrawGraphLine
                  0x00c390                  _DrawGridHorizontals
                  0x00c3b6                  _DrawGridVerticals
                  0x00c3de                  _GraphReadPotentiometer
                  0x00c4a6                  _ProcessMessageDemos
                  0x00c53a                  _ProcessMessageGraph
                  0x00c5b0                  _ProcessMessageRGB
                  0x00c7aa                  _RGBSetBlue
                  0x00c7c4                  _RGBSetGreen
                  0x00c7de                  _RGBSetRed
                  0x00c7f8                  _RGBMapColorPins
                  0x00c84a                  _RGBTurnOffLED
                  0x00c86c                  _RGBTurnOnLED
                  0x00c8cc                  _ProcessMessageBarDemo
                  0x00c8de                  _ShowScreenCapture
                  0x00c99c                  _ShowScreenCaptureMedia
                  0x00ca30                  _ShowScreenDemos
                  0x00ca8e                  _ShowScreenGraph
                  0x00cb4c                  _ShowScreenRGB
                  0x00ccda                  _ShowScreenBarDemo
                  0x00cd74                  _DrawBarDemo
                  0x00cf4e                  _TranslateMessageGraph
                  0x00cfb4                  _TranslateMessageRGB
                  0x00d074                  _UpdateGraph
                  0x00d0fe                  _WriteOneBuffer
                  0x00d162                  _InitGraph
                  0x00d190                  _Arc
                  0x00d66a                  _Line
                  0x00d8b4                  _Bevel
                  0x00dba4                  _FillBevel
                  0x00dd96                  _DrawPoly
                  0x00ddf6                  _Bar
                  0x00de32                  _SetFont
                  0x00de62                  _OutText
                  0x00de8c                  _OutTextXY
                  0x00dec2                  _OutChar
                  0x00dff4                  _GetTextWidth
                  0x00e07e                  _GetTextHeight
                  0x00e0a2                  _GetImageWidth
                  0x00e0d4                  _GetImageHeight
                  0x00e106                  _DelayMs
                  0x00e12a                  _ResetDevice
                  0x00e3e6                  _PutPixel
                  0x00e5a2                  _GetPixel
                  0x00e71e                  _BarHS2
                  0x00eac0                  _BarHSP
                  0x00ee7c                  _ClearDevice
                  0x00ef08                  _PutImage
                  0x00ef3e                  _PutImage1BPP
                  0x00f066                  _main
                  0x00f0c8                  _GOLDrawCallback
                  0x00f360                  _GOLMsgCallback
                  0x00f4d2                  _InitializeScreen
                  0x00f522                  _PerformBoardTest
                  0x00f622                  _ProcessMessageMain
                  0x00f680                  _ShowScreenGeneric
                  0x00f748                  _ShowScreenMain
                  0x00f7b2                  _TickInit
                  0x00f7ca                  _TranslateMessageGeneric
                  0x00fbea                  _TranslateTouchpad
                  0x00fce6                  __T4Interrupt
                  0x00fd16                  __DefaultInterrupt
                  0x00fd2a                  __OscillatorFail
                  0x00fd3e                  __AddressError
                  0x00fd52                  __StackError
                  0x00fd66                  __MathError
                  0x00fd7a                  _CalibrateCTMU
                  0x01000e                  _IndicateFocus
                  0x010054                  _ProcessMessageCTMU
                  0x010062                  _ProcessMessageTime
                  0x0102fe                  _ProcessMessageUtilities
                  0x01037a                  _ShowScreenCTMU
                  0x0103b6                  _ShowScreenTime
                  0x010770                  _ShowScreenUtilities
                  0x0107ca                  _TranslateMessageCTMU
                  0x0107d8                  _TranslateMessageTime
                  0x01093e                  _UpdateDateTime
                  0x0109d4                  _SldCreate
                  0x010a76                  _SldSetThumbSize
                  0x010aaa                  _SldGetWidth
                  0x010b12                  _SldGetHeight
                  0x010b7a                  _SldGetMinMaxPos
                  0x010be8                  _SldSetRange
                  0x010c76                  _SldSetPage
                  0x010cba                  _SldSetPos
                  0x010d8e                  _SldMsgDefault
                  0x010e1a                  _SldTranslateMsg
                  0x010e8e                  _SldDraw
                  0x01137a                  _GridCreate
                  0x011454                  _GridDraw
                  0x011858                  _GridFreeItems
                  0x01187a                  _GridSetCell
                  0x0118de                  _GridClearCellState
                  0x011938                  _GridSetFocus
                  0x011966                  _GridSetCellState
                  0x0119be                  _GridGetCell
                  0x011a20                  _GridMsgDefault
                  0x011c1a                  _GridTranslateMsg
                  0x011cb2                  _GOLGetFocusNext
                  0x011ce6                  _GOLSetFocus
                  0x011d24                  _GOLCanBeFocused
                  0x011d6c                  _GOLCreateScheme
                  0x011dbc                  _GOLInit
                  0x011dca                  _GOLFree
                  0x011e0e                  _GOLDeleteObject
                  0x011e92                  _GOLDeleteObjectByID
                  0x011eb2                  _GOLFindObject
                  0x011ee0                  _GOLAddObject
                  0x011f14                  _GOLDraw
                  0x012006                  _GOLRedrawRec
                  0x0120a8                  _GOLMsg
                  0x012234                  _GOLPanelDrawTsk
                  0x012586                  _LbCreate
                  0x012690                  _LbAddItem
                  0x01272e                  _LbDelItem
                  0x012790                  _LbDelItemsList
                  0x0127bc                  _LbGetSel
                  0x0127ec                  _LbChangeSel
                  0x01284e                  _LbSetFocusedItem
                  0x0128a6                  _LbGetFocusedItem
                  0x0128e8                  _LbTranslateMsg
                  0x012960                  _LbMsgDefault
                  0x0129ea                  _LbDraw
                  0x012dd6                  _FlashDeleteListBoxItems
                  0x012e08                  _FlashDisplayDirectory
                  0x012e6c                  _FlashDisplayFiles
                  0x012f04                  _FlashFormatFileInformation
                  0x012f56                  _FlashMonitorMedia
                  0x012ff2                  _FlashUpdateVolume
                  0x013058                  _ProcessMessageFlash
                  0x013142                  _ProcessMessageFlashError
                  0x013154                  _ShowScreenFlash
                  0x0131e8                  _ShowScreenFlashError
                  0x013510                  _TranslateMessageFlash
                  0x01357c                  _TranslateMessageFlashError
                  0x0135a0                  _USB_ApplicationEventHandler
                  0x013600                  _RTCCProcessEvents
                  0x0138a2                  _RTCCInit
                  0x0138e2                  _RTCCSet
                  0x013928                  _RTCCUnlock
                  0x01393e                  _RTCCSetBinSec
                  0x013980                  _RTCCSetBinMin
                  0x0139c2                  _RTCCSetBinHour
                  0x013a04                  _RTCCCalculateWeekDay
                  0x013a8a                  _RTCCSetBinDay
                  0x013b20                  _RTCCSetBinMonth
                  0x013b60                  _RTCCSetBinYear
                  0x013bb6                  _RdiaCreate
                  0x013c58                  _RdiaMsgDefault
                  0x013c90                  _RdiaCosine
                  0x013cf6                  _RdiaSine
                  0x013d5c                  _RdiaTranslateMsg
                  0x013e58                  _RdiaDraw
                  0x0140a4                  _BtnCreate
                  0x014178                  _BtnSetText
                  0x0141aa                  _BtnMsgDefault
                  0x0141ee                  _BtnTranslateMsg
                  0x01429e                  _BtnDraw
                  0x01458a                  _CTMUInit
                  0x014602                  _ReadCTMU
                  0x0148bc                  _SetNextChannel
                  0x0148d2                  _TouchSenseButtonsMsg
                  0x014a4e                  _EbCreate
                  0x014b04                  _EbSetText
                  0x014b5a                  _EbAddChar
                  0x014b96                  _EbDeleteChar
                  0x014bbe                  _EbTranslateMsg
                  0x014c12                  _EbMsgDefault
                  0x014c58                  _EbDraw
                  0x014e9e                  _L4298
                  0x0152a8                  _L29552
                  0x0156b2                  _USBHostMSDSCSIInitialize
                  0x0156d4                  _USBHostMSDSCSIEventHandler
                  0x015746                  _USBHostMSDSCSIMediaDetect
                  0x015766                  _USBHostMSDSCSIMediaInitialize
                  0x0158a6                  _USBHostMSDSCSIMediaReset
                  0x0158f6                  _USBHostMSDSCSISectorRead
                  0x0159b8                  _USBHostMSDSCSISectorWrite
                  0x015a92                  _USBHostMSDSCSIWriteProtectState
                  0x015a9a                  _StCreate
                  0x015b3a                  _StSetText
                  0x015b5a                  _StTranslateMsg
                  0x015b7c                  _StDraw
                  0x015db4                  _PictCreate
                  0x015e3c                  _PictTranslateMsg
                  0x015e5e                  _PictDraw
                  0x0161ec                  _L17009
                  0x016216                  _L8740
                  0x016234                  _L17048
                  0x016246                  _L18321
                  0x016258                  _L2447
                  0x01626a                  _L32264
                  0x01627c                  _L10673
                  0x01628e                  _L4126
                  0x0162a0                  _L8993
                  0x0162b2                  _L18976

External Symbols in Program Memory (by name):

                  0x00c160                  _AdjustColorPWM
                  0x00d190                  _Arc
                  0x00ddf6                  _Bar
                  0x00e71e                  _BarHS2
                  0x00eac0                  _BarHSP
                  0x00d8b4                  _Bevel
                  0x0140a4                  _BtnCreate
                  0x01429e                  _BtnDraw
                  0x0141aa                  _BtnMsgDefault
                  0x014178                  _BtnSetText
                  0x0141ee                  _BtnTranslateMsg
                  0x01458a                  _CTMUInit
                  0x0031b4                  _CacheTime
                  0x002ce0                  _Cache_File_Entry
                  0x00fd7a                  _CalibrateCTMU
                  0x00c19a                  _CaptureMonitorMedia
                  0x00ee7c                  _ClearDevice
                  0x004168                  _Cluster2Sector
                  0x009f84                  _CompactHorizontal
                  0x00a05e                  _CompactVertical
                  0x005f32                  _CreateDIR
                  0x002ec2                  _CreateFileEntry
                  0x002f2c                  _CreateFirstCluster
                  0x002074                  _DISKmount
                  0x00e106                  _DelayMs
                  0x00cd74                  _DrawBarDemo
                  0x00922c                  _DrawBlaster
                  0x00c2dc                  _DrawGraphLine
                  0x00c390                  _DrawGridHorizontals
                  0x00c3b6                  _DrawGridVerticals
                  0x00dd96                  _DrawPoly
                  0x00a5d2                  _DrawSnake
                  0x014b5a                  _EbAddChar
                  0x014a4e                  _EbCreate
                  0x014b96                  _EbDeleteChar
                  0x014c58                  _EbDraw
                  0x014c12                  _EbMsgDefault
                  0x014b04                  _EbSetText
                  0x014bbe                  _EbTranslateMsg
                  0x0040dc                  _EraseCluster
                  0x002bce                  _FAT_erase_cluster_chain
                  0x0033b2                  _FATfindEmptyCluster
                  0x004030                  _FILECreateHeadCluster
                  0x00330a                  _FILEallocate_new_cluster
                  0x00375a                  _FILEerase
                  0x001c8c                  _FILEfind
                  0x001f9c                  _FILEget_next_cluster
                  0x001e76                  _FILEopen
                  0x001bf4                  _FSInit
                  0x005426                  _FSchdir
                  0x0034b0                  _FSfclose
                  0x0044e2                  _FSfeof
                  0x003cce                  _FSfopen
                  0x002460                  _FSformat
                  0x004506                  _FSfread
                  0x0049f2                  _FSfseek
                  0x003f0c                  _FSftell
                  0x004210                  _FSfwrite
                  0x0057d2                  _FSgetcwd
                  0x005cc8                  _FSmkdir
                  0x003f1a                  _FSremove
                  0x003816                  _FSrename
                  0x003fbc                  _FSrewind
                  0x0061be                  _FSrmdir
                  0x003ff0                  _FileObjectCopy
                  0x00dba4                  _FillBevel
                  0x00357a                  _Fill_File_Object
                  0x00a10e                  _FindBallNumber
                  0x002fb8                  _FindEmptyEntries
                  0x006730                  _FindFirst
                  0x006990                  _FindNext
                  0x009be0                  _FindNextPosition
                  0x012dd6                  _FlashDeleteListBoxItems
                  0x012e08                  _FlashDisplayDirectory
                  0x012e6c                  _FlashDisplayFiles
                  0x012f04                  _FlashFormatFileInformation
                  0x012f56                  _FlashMonitorMedia
                  0x012ff2                  _FlashUpdateVolume
                  0x0066b6                  _FormatDirName
                  0x0046b2                  _FormatFileName
                  0x011ee0                  _GOLAddObject
                  0x011d24                  _GOLCanBeFocused
                  0x011d6c                  _GOLCreateScheme
                  0x011e0e                  _GOLDeleteObject
                  0x011e92                  _GOLDeleteObjectByID
                  0x011f14                  _GOLDraw
                  0x00f0c8                  _GOLDrawCallback
                  0x011eb2                  _GOLFindObject
                  0x000fea                  _GOLFontDefault
                  0x011dca                  _GOLFree
                  0x011cb2                  _GOLGetFocusNext
                  0x011dbc                  _GOLInit
                  0x0120a8                  _GOLMsg
                  0x00f360                  _GOLMsgCallback
                  0x012234                  _GOLPanelDrawTsk
                  0x012006                  _GOLRedrawRec
                  0x011ce6                  _GOLSetFocus
                  0x006b96                  _GetFullClusterNumber
                  0x00e0d4                  _GetImageHeight
                  0x00e0a2                  _GetImageWidth
                  0x00e5a2                  _GetPixel
                  0x005b36                  _GetPreviousEntry
                  0x00e07e                  _GetTextHeight
                  0x00dff4                  _GetTextWidth
                  0x00c3de                  _GraphReadPotentiometer
                  0x0118de                  _GridClearCellState
                  0x01137a                  _GridCreate
                  0x011454                  _GridDraw
                  0x011858                  _GridFreeItems
                  0x0119be                  _GridGetCell
                  0x011a20                  _GridMsgDefault
                  0x01187a                  _GridSetCell
                  0x011966                  _GridSetCellState
                  0x011938                  _GridSetFocus
                  0x011c1a                  _GridTranslateMsg
                  0x01000e                  _IndicateFocus
                  0x00d162                  _InitGraph
                  0x009052                  _InitializeRandomNumberGenerator
                  0x00f4d2                  _InitializeScreen
                  0x01627c                  _L10673
                  0x000fee                  _L13579
                  0x0161ec                  _L17009
                  0x016234                  _L17048
                  0x016246                  _L18321
                  0x0162b2                  _L18976
                  0x016258                  _L2447
                  0x0152a8                  _L29552
                  0x01626a                  _L32264
                  0x01628e                  _L4126
                  0x014e9e                  _L4298
                  0x016216                  _L8740
                  0x0162a0                  _L8993
                  0x012690                  _LbAddItem
                  0x0127ec                  _LbChangeSel
                  0x012586                  _LbCreate
                  0x01272e                  _LbDelItem
                  0x012790                  _LbDelItemsList
                  0x0129ea                  _LbDraw
                  0x0128a6                  _LbGetFocusedItem
                  0x0127bc                  _LbGetSel
                  0x012960                  _LbMsgDefault
                  0x01284e                  _LbSetFocusedItem
                  0x0128e8                  _LbTranslateMsg
                  0x00d66a                  _Line
                  0x002258                  _LoadBootSector
                  0x0036d4                  _LoadDirAttrib
                  0x0020b6                  _LoadMBR
                  0x00a15c                  _MarkAllNeighbors
                  0x00a252                  _MovesRemaining
                  0x00dec2                  _OutChar
                  0x00de62                  _OutText
                  0x00de8c                  _OutTextXY
                  0x00f522                  _PerformBoardTest
                  0x015db4                  _PictCreate
                  0x015e5e                  _PictDraw
                  0x015e3c                  _PictTranslateMsg
                  0x0030cc                  _PopulateEntries
                  0x00c8cc                  _ProcessMessageBarDemo
                  0x009db0                  _ProcessMessageBlaster
                  0x010054                  _ProcessMessageCTMU
                  0x00c4a6                  _ProcessMessageDemos
                  0x013058                  _ProcessMessageFlash
                  0x013142                  _ProcessMessageFlashError
                  0x009068                  _ProcessMessageGames
                  0x00c53a                  _ProcessMessageGraph
                  0x00f622                  _ProcessMessageMain
                  0x00c5b0                  _ProcessMessageRGB
                  0x0090e4                  _ProcessMessageScore
                  0x00a32c                  _ProcessMessageShapelet
                  0x00a97a                  _ProcessMessageSnake
                  0x010062                  _ProcessMessageTime
                  0x0102fe                  _ProcessMessageUtilities
                  0x00ef08                  _PutImage
                  0x00ef3e                  _PutImage1BPP
                  0x00e3e6                  _PutPixel
                  0x00c7f8                  _RGBMapColorPins
                  0x00c7aa                  _RGBSetBlue
                  0x00c7c4                  _RGBSetGreen
                  0x00c7de                  _RGBSetRed
                  0x00c84a                  _RGBTurnOffLED
                  0x00c86c                  _RGBTurnOnLED
                  0x013a04                  _RTCCCalculateWeekDay
                  0x0138a2                  _RTCCInit
                  0x013600                  _RTCCProcessEvents
                  0x0138e2                  _RTCCSet
                  0x013a8a                  _RTCCSetBinDay
                  0x0139c2                  _RTCCSetBinHour
                  0x013980                  _RTCCSetBinMin
                  0x013b20                  _RTCCSetBinMonth
                  0x01393e                  _RTCCSetBinSec
                  0x013b60                  _RTCCSetBinYear
                  0x013928                  _RTCCUnlock
                  0x0090f6                  _Random
                  0x013c90                  _RdiaCosine
                  0x013bb6                  _RdiaCreate
                  0x013e58                  _RdiaDraw
                  0x013c58                  _RdiaMsgDefault
                  0x013cf6                  _RdiaSine
                  0x013d5c                  _RdiaTranslateMsg
                  0x006bbe                  _ReadByte
                  0x014602                  _ReadCTMU
                  0x006c04                  _ReadDWord
                  0x004c16                  _ReadFAT
                  0x006bd0                  _ReadWord
                  0x00e12a                  _ResetDevice
                  0x00de32                  _SetFont
                  0x0148bc                  _SetNextChannel
                  0x00ccda                  _ShowScreenBarDemo
                  0x009e40                  _ShowScreenBlaster
                  0x01037a                  _ShowScreenCTMU
                  0x00c8de                  _ShowScreenCapture
                  0x00c99c                  _ShowScreenCaptureMedia
                  0x00ca30                  _ShowScreenDemos
                  0x013154                  _ShowScreenFlash
                  0x0131e8                  _ShowScreenFlashError
                  0x00911e                  _ShowScreenGames
                  0x00f680                  _ShowScreenGeneric
                  0x00ca8e                  _ShowScreenGraph
                  0x00f748                  _ShowScreenMain
                  0x00cb4c                  _ShowScreenRGB
                  0x009172                  _ShowScreenScore
                  0x00a4ea                  _ShowScreenShapelet
                  0x00a9ea                  _ShowScreenSnake
                  0x0103b6                  _ShowScreenTime
                  0x010770                  _ShowScreenUtilities
                  0x0109d4                  _SldCreate
                  0x010e8e                  _SldDraw
                  0x010b12                  _SldGetHeight
                  0x010b7a                  _SldGetMinMaxPos
                  0x010aaa                  _SldGetWidth
                  0x010d8e                  _SldMsgDefault
                  0x010c76                  _SldSetPage
                  0x010cba                  _SldSetPos
                  0x010be8                  _SldSetRange
                  0x010a76                  _SldSetThumbSize
                  0x010e1a                  _SldTranslateMsg
                  0x015a9a                  _StCreate
                  0x015b7c                  _StDraw
                  0x015b3a                  _StSetText
                  0x015b5a                  _StTranslateMsg
                  0x00f7b2                  _TickInit
                  0x0148d2                  _TouchSenseButtonsMsg
                  0x009eea                  _TranslateMessageBlaster
                  0x0107ca                  _TranslateMessageCTMU
                  0x013510                  _TranslateMessageFlash
                  0x01357c                  _TranslateMessageFlashError
                  0x00f7ca                  _TranslateMessageGeneric
                  0x00cf4e                  _TranslateMessageGraph
                  0x00cfb4                  _TranslateMessageRGB
                  0x009208                  _TranslateMessageScore
                  0x00a5ba                  _TranslateMessageShapelet
                  0x00ab78                  _TranslateMessageSnake
                  0x0107d8                  _TranslateMessageTime
                  0x00fbea                  _TranslateTouchpad
                  0x006c38                  _USBHostClearEndpointErrors
                  0x006c86                  _USBHostDeviceRequest
                  0x006d50                  _USBHostDeviceSpecificClientDriver
                  0x006d62                  _USBHostDeviceStatus
                  0x006db6                  _USBHostInit
                  0x00abf8                  _USBHostMSDDeviceStatus
                  0x00bfec                  _USBHostMSDEventHandler
                  0x00be4a                  _USBHostMSDInitialize
                  0x00accc                  _USBHostMSDResetDevice
                  0x0156d4                  _USBHostMSDSCSIEventHandler
                  0x0156b2                  _USBHostMSDSCSIInitialize
                  0x015746                  _USBHostMSDSCSIMediaDetect
                  0x015766                  _USBHostMSDSCSIMediaInitialize
                  0x0158a6                  _USBHostMSDSCSIMediaReset
                  0x0158f6                  _USBHostMSDSCSISectorRead
                  0x0159b8                  _USBHostMSDSCSISectorWrite
                  0x015a92                  _USBHostMSDSCSIWriteProtectState
                  0x00ad88                  _USBHostMSDTasks
                  0x00ba3c                  _USBHostMSDTerminateTransfer
                  0x00bade                  _USBHostMSDTransfer
                  0x00bd6e                  _USBHostMSDTransferIsComplete
                  0x006dfe                  _USBHostRead
                  0x006eae                  _USBHostResetDevice
                  0x006edc                  _USBHostResumeDevice
                  0x006f0a                  _USBHostSetDeviceConfiguration
                  0x006f4c                  _USBHostShutdown
                  0x006f7c                  _USBHostSuspendDevice
                  0x006faa                  _USBHostTasks
                  0x007b2e                  _USBHostTerminateTransfer
                  0x007b6c                  _USBHostTransferIsComplete
                  0x007c16                  _USBHostVbusEvent
                  0x007c52                  _USBHostWrite
                  0x0135a0                  _USB_ApplicationEventHandler
                  0x01093e                  _UpdateDateTime
                  0x00d074                  _UpdateGraph
                  0x0047c6                  _ValidateChars
                  0x004fc2                  _WriteFAT
                  0x00d0fe                  _WriteOneBuffer
                  0x002b2c                  _Write_File_Entry
                  0x00fd3e                  __AddressError
                  0x00fd16                  __DefaultInterrupt
                  0x000588                  __Getmem
                  0x000b3a                  __Litob
                  0x00fd66                  __MathError
                  0x00fd2a                  __OscillatorFail
                  0x0009a6                  __Puttxt
                  0x00fd52                  __StackError
                  0x00fce6                  __T4Interrupt
                  0x008b88                  __USB1Interrupt
                  0x00c08c                  __USBHostMSD_GetNextTag
                  0x00c0a2                  __USBHostMSD_ResetStateJump
                  0x007d02                  __USB_CheckCommandAndEnumerationAttempts
                  0x007d48                  __USB_FindClassDriver
                  0x007dc4                  __USB_FindDeviceLevelClientDriver
                  0x007eb2                  __USB_FindInterface
                  0x007ee6                  __USB_FindNextToken
                  0x0082c6                  __USB_FreeConfigMemory
                  0x008314                  __USB_FreeMemory
                  0x00835c                  __USB_InitControlRead
                  0x0083d8                  __USB_InitControlWrite
                  0x008462                  __USB_InitRead
                  0x0084ea                  __USB_InitWrite
                  0x008572                  __USB_NotifyClients
                  0x008670                  __USB_ParseConfigurationDescriptor
                  0x008986                  __USB_ResetDATA0
                  0x0089b4                  __USB_SendToken
                  0x008a08                  __USB_SetBDT
                  0x008b5c                  __USB_TransferInProgress
                  0x000716                  __Vacopy
                  0x000e3e                  ___divdi3
                  0x0005a4                  ___iPrintf
                  0x000720                  ___iPutfld
                  0x000e78                  ___moddi3
                  0x000f4a                  ___muldi3
                  0x000d28                  ___mulsi3
                  0x000e28                  ___udivdi3
                  0x000d5a                  ___udivmoddi3
                  0x000d08                  ___udivsi3
                  0x000e36                  ___umoddi3
                  0x000fa6                  ___umuldi3
                  0x00022e                  __data_init
                  0x000476                  __isprintf
                  0x00021e                  __psv_init
                  0x000200                  __resetPRI
                  0x001b72                  _ballCircle
                  0x001b78                  _ballCross
                  0x001b7e                  _ballMarking
                  0x001b84                  _ballSquare
                  0x001b8a                  _ballTriangle
                  0x005436                  _chdirhelper
                  0x006628                  _eraseDir
                  0x004488                  _flushData
                  0x000340                  _free
                  0x001b90                  _iconFolderSmall
                  0x001b96                  _iconMicrochip
                  0x001b9c                  _intro
                  0x001ba2                  _introDevice
                  0x004946                  _isDIR
                  0x00488e                  _isShort
                  0x00f066                  _main
                  0x00029c                  _malloc
                  0x001a86                  _mediaRequest
                  0x000caa                  _memchr
                  0x000596                  _memcpy
                  0x0003b6                  _memset
                  0x005cd8                  _mkdirhelper
                  0x0004de                  _rand
                  0x0061d2                  _rmdirhelper
                  0x001ba8                  _snakeBody
                  0x001bae                  _snakeFood
                  0x001bb4                  _snakeHead
                  0x0004bc                  _srand
                  0x000428                  _strcat
                  0x000416                  _strchr
                  0x000446                  _strcmp
                  0x000406                  _strcpy
                  0x0003f8                  _strlen
                  0x000498                  _strncmp
                  0x0003c4                  _strncpy
                  0x0003a8                  _tolower
                  0x0003ea                  _toupper
                  0x00602e                  _writeDotEntries
                  0x00046a                  sprintf.io:_prout

Memory Configuration

Name             Origin             Length             Attributes
data             0x000800           0x004000           a !xr
reset            0x000000           0x000004  
ivt              0x000004           0x0000fc  
aivt             0x000104           0x0000fc  
program          0x000200           0x02a9f8           xr
config4          0x02abf8           0x000002  
config3          0x02abfa           0x000002  
config2          0x02abfc           0x000002  
config1          0x02abfe           0x000002  
*default*        0x000000           0xffffffff  

Linker script and memory map

LOAD Objects - PIC24F Starter Kit\rtcc.o
LOAD Objects - PIC24F Starter Kit\usb_config.o
LOAD ..\Microchip\Usb\Objects - PIC24F Starter Kit\usb_host.o
LOAD ..\Microchip\MDD File System\Objects - PIC24F Starter Kit\FSIO.o
LOAD Objects - PIC24F Starter Kit\PIC24F Starter Kit.o
LOAD Objects - PIC24F Starter Kit\Gentium8.o
LOAD ..\Microchip\Graphics\Objects - PIC24F Starter Kit\Primitive.o
LOAD ..\Microchip\Graphics\Objects - PIC24F Starter Kit\Slider.o
LOAD ..\Microchip\Graphics\Objects - PIC24F Starter Kit\StaticText.o
LOAD ..\Microchip\Graphics\Objects - PIC24F Starter Kit\GOL.o
LOAD ..\Microchip\Graphics\Objects - PIC24F Starter Kit\ListBox.o
LOAD ..\Microchip\Graphics\Objects - PIC24F Starter Kit\Picture.o
LOAD ..\Microchip\Graphics\Objects - PIC24F Starter Kit\Button.o
LOAD Objects - PIC24F Starter Kit\Pictures.o
LOAD Objects - PIC24F Starter Kit\Demos.o
LOAD Objects - PIC24F Starter Kit\Flash.o
LOAD Objects - PIC24F Starter Kit\Utilities.o
LOAD Objects - PIC24F Starter Kit\TouchSense.o
LOAD Objects - PIC24F Starter Kit\Games.o
LOAD ..\Microchip\Graphics\Objects - PIC24F Starter Kit\EditBox.o
LOAD ..\Microchip\Graphics\Objects - PIC24F Starter Kit\RoundDial.o
LOAD ..\Microchip\Graphics\Objects - PIC24F Starter Kit\Grid.o
LOAD ..\Microchip\Graphics\Objects - PIC24F Starter Kit\SH1101A.o
LOAD ..\Microchip\Usb\MSD Host Driver\Objects - PIC24F Starter Kit\usb_host_msd_scsi.o
LOAD ..\Microchip\Usb\MSD Host Driver\Objects - PIC24F Starter Kit\usb_host_msd.o
LOAD c:/program files/microchip/mplab c30/bin/bin/../../lib/PIC24F\libpPIC24Fxxx-coff.a
                    0x2abfa                  __CONFIG3 = 0x2abfa
                    0x2abfc                  __CONFIG2 = 0x2abfc
                    0x2abfe                  __CONFIG1 = 0x2abfe
                    0x0004                  __IVT_BASE = 0x4
                    0x0104                  __AIVT_BASE = 0x104
                    0x0800                  __DATA_BASE = 0x800
                    0x0200                  __CODE_BASE = 0x200

.reset            0x000000          0x4
                  0x000000          0x2 SHORT 0x200 <code 337> (__reset)
                  0x000001          0x2 SHORT 0x4
                  0x000002          0x2 SHORT 0x0 ((<code 337> (__reset) >> 0x10) & 0x7f)
                  0x000003          0x2 SHORT 0x0

.text             0x000200        0xdea
 *(.init)
 .init            0x000200         0x88 c:/program files/microchip/mplab c30/bin/bin/../../lib\libpic30-coff.a(crt0.o)
                  0x000200                  _resetPRI
                  0x000200                  _reset
                  0x00021e                  _psv_init
                  0x00022e                  _data_init
 *(.user_init)
 *(.handle)
 .handle          0x000288         0x14 jump_table
 *(.libc)
 .libc            0x00029c         0xa4 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(malloc.o)
                  0x00029c                  malloc
 .libc            0x000340         0x68 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(free.o)
                  0x000340                  free
 .libc            0x0003a8          0xe c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(tolower.os)
                  0x0003a8                  tolower
 .libc            0x0003b6          0xe c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memset.o)
                  0x0003b6                  memset
 .libc            0x0003c4         0x26 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strncpy.o)
                  0x0003c4                  strncpy
 .libc            0x0003ea          0xe c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(toupper.os)
                  0x0003ea                  toupper
 .libc            0x0003f8          0xe c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strlen.o)
                  0x0003f8                  strlen
 .libc            0x000406         0x10 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strcpy.o)
                  0x000406                  strcpy
 .libc            0x000416         0x12 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strchr.o)
                  0x000416                  strchr
 .libc            0x000428         0x1e c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strcat.o)
                  0x000428                  strcat
 .libc            0x000446         0x24 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strcmp.o)
                  0x000446                  strcmp
 .libc            0x00046a         0x2e c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(sprintf.io)
                  0x00046a                  sprintf.io:_prout
                  0x000476                  _isprintf
 .libc            0x000498         0x24 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strncmp.o)
                  0x000498                  strncmp
 .libc            0x0004bc         0x22 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(srand.o)
                  0x0004bc                  srand
 .libc            0x0004de         0xaa c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(rand.o)
                  0x0004de                  rand
 .libc            0x000588          0xe c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xgetmem.o)
                  0x000588                  _Getmem
 .libc            0x000596          0xe c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memcpy.o)
                  0x000596                  memcpy
 .libc            0x0005a4        0x172 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xprintf.io)
                  0x0005a4                  __iPrintf
 .libc            0x000716          0xa c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xvacopy.o)
                  0x000716                  _Vacopy
 .libc            0x000720        0x286 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xputfld.io)
                  0x000720                  __iPutfld
 .libc            0x0009a6        0x194 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xputtxt.o)
                  0x0009a6                  _Puttxt
 .libc            0x000b3a        0x170 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xlitob.o)
                  0x000b3a                  _Litob
 .libc            0x000caa         0x14 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memchr.o)
                  0x000caa                  memchr
 .libc            0x000cbe         0x2c c:/program files/microchip/mplab c30/bin/bin/../../lib\libpic30-coff.a(sbrk.o)
                  0x000cbe                  sbrk
 .libc            0x000cea         0x1e c:/program files/microchip/mplab c30/bin/bin/../../lib\libpic30-coff.a(brk.o)
                  0x000cea                  brk
 *(.libm)
 .libm            0x000d08         0x20 c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(udivsi3.o)
                  0x000d08                  __udivsi3
 .libm            0x000d28          0xc c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(mulsi3.o)
                  0x000d28                  __mulsi3
 .libm            0x000d34        0x216 c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(divmoddi3.o)
                  0x000d5a                  __udivmoddi3
                  0x000e28                  __udivdi3
                  0x000e36                  __umoddi3
                  0x000e3e                  __divdi3
                  0x000e78                  __moddi3
 .libm            0x000f4a         0x5c c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(muldi3.o)
                  0x000f4a                  __muldi3
 .libm            0x000fa6         0x44 c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(umuldi3.o)
                  0x000fa6                  __umuldi3
 *(.libdsp)
 *(.lib*)

__CONFIG3
 *(__CONFIG3.sec)

__CONFIG2         0x02abfc          0x2
 *(__CONFIG2.sec)
 __CONFIG2.sec    0x02abfc          0x2 Objects - PIC24F Starter Kit\PIC24F Starter Kit.o

__CONFIG1         0x02abfe          0x2
 *(__CONFIG1.sec)
 __CONFIG1.sec    0x02abfe          0x2 Objects - PIC24F Starter Kit\PIC24F Starter Kit.o

.comment
 *(.comment)

.debug_info
 *(.debug_info)
 *(.gnu.linkonce.wi.*)

.debug_abbrev
 *(.debug_abbrev)

.debug_line
 *(.debug_line)

.debug_frame
 *(.debug_frame)

.debug_str
 *(.debug_str)

.debug_loc
 *(.debug_loc)

.debug_macinfo
 *(.debug_macinfo)

.debug_pubnames
 *(.debug_pubnames)

.debug_ranges
 *(.debug_ranges)

.debug_aranges
 *(.debug_aranges)

.ivt              0x000004         0xfc
                  0x000004          0x4 LONG 0xfd16 DEFINED (__ReservedTrap0)?<code 337> (__ReservedTrap0):<code 337> (__DefaultInterrupt)
                  0x000006          0x4 LONG 0xfd2a DEFINED (__OscillatorFail)?<code 337> (__OscillatorFail):<code 337> (__DefaultInterrupt)
                  0x000008          0x4 LONG 0xfd3e DEFINED (__AddressError)?<code 337> (__AddressError):<code 337> (__DefaultInterrupt)
                  0x00000a          0x4 LONG 0xfd52 DEFINED (__StackError)?<code 337> (__StackError):<code 337> (__DefaultInterrupt)
                  0x00000c          0x4 LONG 0xfd66 DEFINED (__MathError)?<code 337> (__MathError):<code 337> (__DefaultInterrupt)
                  0x00000e          0x4 LONG 0xfd16 DEFINED (__ReservedTrap5)?<code 337> (__ReservedTrap5):<code 337> (__DefaultInterrupt)
                  0x000010          0x4 LONG 0xfd16 DEFINED (__ReservedTrap6)?<code 337> (__ReservedTrap6):<code 337> (__DefaultInterrupt)
                  0x000012          0x4 LONG 0xfd16 DEFINED (__ReservedTrap7)?<code 337> (__ReservedTrap7):<code 337> (__DefaultInterrupt)
                  0x000014          0x4 LONG 0xfd16 DEFINED (__INT0Interrupt)?<code 337> (__INT0Interrupt):<code 337> (__DefaultInterrupt)
                  0x000016          0x4 LONG 0xfd16 DEFINED (__IC1Interrupt)?<code 337> (__IC1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000018          0x4 LONG 0xfd16 DEFINED (__OC1Interrupt)?<code 337> (__OC1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00001a          0x4 LONG 0xfd16 DEFINED (__T1Interrupt)?<code 337> (__T1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00001c          0x4 LONG 0xfd16 DEFINED (__Interrupt4)?<code 337> (__Interrupt4):<code 337> (__DefaultInterrupt)
                  0x00001e          0x4 LONG 0xfd16 DEFINED (__IC2Interrupt)?<code 337> (__IC2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000020          0x4 LONG 0xfd16 DEFINED (__OC2Interrupt)?<code 337> (__OC2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000022          0x4 LONG 0xfd16 DEFINED (__T2Interrupt)?<code 337> (__T2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000024          0x4 LONG 0xfd16 DEFINED (__T3Interrupt)?<code 337> (__T3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000026          0x4 LONG 0xfd16 DEFINED (__SPI1ErrInterrupt)?<code 337> (__SPI1ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x000028          0x4 LONG 0xfd16 DEFINED (__SPI1Interrupt)?<code 337> (__SPI1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00002a          0x4 LONG 0xfd16 DEFINED (__U1RXInterrupt)?<code 337> (__U1RXInterrupt):<code 337> (__DefaultInterrupt)
                  0x00002c          0x4 LONG 0xfd16 DEFINED (__U1TXInterrupt)?<code 337> (__U1TXInterrupt):<code 337> (__DefaultInterrupt)
                  0x00002e          0x4 LONG 0xfd16 DEFINED (__ADC1Interrupt)?<code 337> (__ADC1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000030          0x4 LONG 0xfd16 DEFINED (__Interrupt14)?<code 337> (__Interrupt14):<code 337> (__DefaultInterrupt)
                  0x000032          0x4 LONG 0xfd16 DEFINED (__Interrupt15)?<code 337> (__Interrupt15):<code 337> (__DefaultInterrupt)
                  0x000034          0x4 LONG 0xfd16 DEFINED (__SI2C1Interrupt)?<code 337> (__SI2C1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000036          0x4 LONG 0xfd16 DEFINED (__MI2C1Interrupt)?<code 337> (__MI2C1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000038          0x4 LONG 0xfd16 DEFINED (__CompInterrupt)?<code 337> (__CompInterrupt):<code 337> (__DefaultInterrupt)
                  0x00003a          0x4 LONG 0xfd16 DEFINED (__CNInterrupt)?<code 337> (__CNInterrupt):<code 337> (__DefaultInterrupt)
                  0x00003c          0x4 LONG 0xfd16 DEFINED (__INT1Interrupt)?<code 337> (__INT1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00003e          0x4 LONG 0xfd16 DEFINED (__Interrupt21)?<code 337> (__Interrupt21):<code 337> (__DefaultInterrupt)
                  0x000040          0x4 LONG 0xfd16 DEFINED (__IC7Interrupt)?<code 337> (__IC7Interrupt):<code 337> (__DefaultInterrupt)
                  0x000042          0x4 LONG 0xfd16 DEFINED (__IC8Interrupt)?<code 337> (__IC8Interrupt):<code 337> (__DefaultInterrupt)
                  0x000044          0x4 LONG 0xfd16 DEFINED (__Interrupt24)?<code 337> (__Interrupt24):<code 337> (__DefaultInterrupt)
                  0x000046          0x4 LONG 0xfd16 DEFINED (__OC3Interrupt)?<code 337> (__OC3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000048          0x4 LONG 0xfd16 DEFINED (__OC4Interrupt)?<code 337> (__OC4Interrupt):<code 337> (__DefaultInterrupt)
                  0x00004a          0x4 LONG 0xfce6 DEFINED (__T4Interrupt)?<code 337> (__T4Interrupt):<code 337> (__DefaultInterrupt)
                  0x00004c          0x4 LONG 0xfd16 DEFINED (__T5Interrupt)?<code 337> (__T5Interrupt):<code 337> (__DefaultInterrupt)
                  0x00004e          0x4 LONG 0xfd16 DEFINED (__INT2Interrupt)?<code 337> (__INT2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000050          0x4 LONG 0xfd16 DEFINED (__U2RXInterrupt)?<code 337> (__U2RXInterrupt):<code 337> (__DefaultInterrupt)
                  0x000052          0x4 LONG 0xfd16 DEFINED (__U2TXInterrupt)?<code 337> (__U2TXInterrupt):<code 337> (__DefaultInterrupt)
                  0x000054          0x4 LONG 0xfd16 DEFINED (__SPI2ErrInterrupt)?<code 337> (__SPI2ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x000056          0x4 LONG 0xfd16 DEFINED (__SPI2Interrupt)?<code 337> (__SPI2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000058          0x4 LONG 0xfd16 DEFINED (__Interrupt34)?<code 337> (__Interrupt34):<code 337> (__DefaultInterrupt)
                  0x00005a          0x4 LONG 0xfd16 DEFINED (__Interrupt35)?<code 337> (__Interrupt35):<code 337> (__DefaultInterrupt)
                  0x00005c          0x4 LONG 0xfd16 DEFINED (__Interrupt36)?<code 337> (__Interrupt36):<code 337> (__DefaultInterrupt)
                  0x00005e          0x4 LONG 0xfd16 DEFINED (__IC3Interrupt)?<code 337> (__IC3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000060          0x4 LONG 0xfd16 DEFINED (__IC4Interrupt)?<code 337> (__IC4Interrupt):<code 337> (__DefaultInterrupt)
                  0x000062          0x4 LONG 0xfd16 DEFINED (__IC5Interrupt)?<code 337> (__IC5Interrupt):<code 337> (__DefaultInterrupt)
                  0x000064          0x4 LONG 0xfd16 DEFINED (__IC6Interrupt)?<code 337> (__IC6Interrupt):<code 337> (__DefaultInterrupt)
                  0x000066          0x4 LONG 0xfd16 DEFINED (__OC5Interrupt)?<code 337> (__OC5Interrupt):<code 337> (__DefaultInterrupt)
                  0x000068          0x4 LONG 0xfd16 DEFINED (__OC6Interrupt)?<code 337> (__OC6Interrupt):<code 337> (__DefaultInterrupt)
                  0x00006a          0x4 LONG 0xfd16 DEFINED (__OC7Interrupt)?<code 337> (__OC7Interrupt):<code 337> (__DefaultInterrupt)
                  0x00006c          0x4 LONG 0xfd16 DEFINED (__OC8Interrupt)?<code 337> (__OC8Interrupt):<code 337> (__DefaultInterrupt)
                  0x00006e          0x4 LONG 0xfd16 DEFINED (__PMPInterrupt)?<code 337> (__PMPInterrupt):<code 337> (__DefaultInterrupt)
                  0x000070          0x4 LONG 0xfd16 DEFINED (__Interrupt46)?<code 337> (__Interrupt46):<code 337> (__DefaultInterrupt)
                  0x000072          0x4 LONG 0xfd16 DEFINED (__Interrupt47)?<code 337> (__Interrupt47):<code 337> (__DefaultInterrupt)
                  0x000074          0x4 LONG 0xfd16 DEFINED (__Interrupt48)?<code 337> (__Interrupt48):<code 337> (__DefaultInterrupt)
                  0x000076          0x4 LONG 0xfd16 DEFINED (__SI2C2Interrupt)?<code 337> (__SI2C2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000078          0x4 LONG 0xfd16 DEFINED (__MI2C2Interrupt)?<code 337> (__MI2C2Interrupt):<code 337> (__DefaultInterrupt)
                  0x00007a          0x4 LONG 0xfd16 DEFINED (__Interrupt51)?<code 337> (__Interrupt51):<code 337> (__DefaultInterrupt)
                  0x00007c          0x4 LONG 0xfd16 DEFINED (__Interrupt52)?<code 337> (__Interrupt52):<code 337> (__DefaultInterrupt)
                  0x00007e          0x4 LONG 0xfd16 DEFINED (__INT3Interrupt)?<code 337> (__INT3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000080          0x4 LONG 0xfd16 DEFINED (__INT4Interrupt)?<code 337> (__INT4Interrupt):<code 337> (__DefaultInterrupt)
                  0x000082          0x4 LONG 0xfd16 DEFINED (__Interrupt55)?<code 337> (__Interrupt55):<code 337> (__DefaultInterrupt)
                  0x000084          0x4 LONG 0xfd16 DEFINED (__Interrupt56)?<code 337> (__Interrupt56):<code 337> (__DefaultInterrupt)
                  0x000086          0x4 LONG 0xfd16 DEFINED (__Interrupt57)?<code 337> (__Interrupt57):<code 337> (__DefaultInterrupt)
                  0x000088          0x4 LONG 0xfd16 DEFINED (__Interrupt58)?<code 337> (__Interrupt58):<code 337> (__DefaultInterrupt)
                  0x00008a          0x4 LONG 0xfd16 DEFINED (__Interrupt59)?<code 337> (__Interrupt59):<code 337> (__DefaultInterrupt)
                  0x00008c          0x4 LONG 0xfd16 DEFINED (__Interrupt60)?<code 337> (__Interrupt60):<code 337> (__DefaultInterrupt)
                  0x00008e          0x4 LONG 0xfd16 DEFINED (__Interrupt61)?<code 337> (__Interrupt61):<code 337> (__DefaultInterrupt)
                  0x000090          0x4 LONG 0xfd16 DEFINED (__RTCCInterrupt)?<code 337> (__RTCCInterrupt):<code 337> (__DefaultInterrupt)
                  0x000092          0x4 LONG 0xfd16 DEFINED (__Interrupt63)?<code 337> (__Interrupt63):<code 337> (__DefaultInterrupt)
                  0x000094          0x4 LONG 0xfd16 DEFINED (__Interrupt64)?<code 337> (__Interrupt64):<code 337> (__DefaultInterrupt)
                  0x000096          0x4 LONG 0xfd16 DEFINED (__U1ErrInterrupt)?<code 337> (__U1ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x000098          0x4 LONG 0xfd16 DEFINED (__U2ErrInterrupt)?<code 337> (__U2ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x00009a          0x4 LONG 0xfd16 DEFINED (__CRCInterrupt)?<code 337> (__CRCInterrupt):<code 337> (__DefaultInterrupt)
                  0x00009c          0x4 LONG 0xfd16 DEFINED (__Interrupt68)?<code 337> (__Interrupt68):<code 337> (__DefaultInterrupt)
                  0x00009e          0x4 LONG 0xfd16 DEFINED (__Interrupt69)?<code 337> (__Interrupt69):<code 337> (__DefaultInterrupt)
                  0x0000a0          0x4 LONG 0xfd16 DEFINED (__Interrupt70)?<code 337> (__Interrupt70):<code 337> (__DefaultInterrupt)
                  0x0000a2          0x4 LONG 0xfd16 DEFINED (__Interrupt71)?<code 337> (__Interrupt71):<code 337> (__DefaultInterrupt)
                  0x0000a4          0x4 LONG 0xfd16 DEFINED (__LVDInterrupt)?<code 337> (__LVDInterrupt):<code 337> (__DefaultInterrupt)
                  0x0000a6          0x4 LONG 0xfd16 DEFINED (__Interrupt73)?<code 337> (__Interrupt73):<code 337> (__DefaultInterrupt)
                  0x0000a8          0x4 LONG 0xfd16 DEFINED (__Interrupt74)?<code 337> (__Interrupt74):<code 337> (__DefaultInterrupt)
                  0x0000aa          0x4 LONG 0xfd16 DEFINED (__Interrupt75)?<code 337> (__Interrupt75):<code 337> (__DefaultInterrupt)
                  0x0000ac          0x4 LONG 0xfd16 DEFINED (__Interrupt76)?<code 337> (__Interrupt76):<code 337> (__DefaultInterrupt)
                  0x0000ae          0x4 LONG 0xfd16 DEFINED (__CTMUInterrupt)?<code 337> (__CTMUInterrupt):<code 337> (__DefaultInterrupt)
                  0x0000b0          0x4 LONG 0xfd16 DEFINED (__Interrupt78)?<code 337> (__Interrupt78):<code 337> (__DefaultInterrupt)
                  0x0000b2          0x4 LONG 0xfd16 DEFINED (__Interrupt79)?<code 337> (__Interrupt79):<code 337> (__DefaultInterrupt)
                  0x0000b4          0x4 LONG 0xfd16 DEFINED (__Interrupt80)?<code 337> (__Interrupt80):<code 337> (__DefaultInterrupt)
                  0x0000b6          0x4 LONG 0xfd16 DEFINED (__U3ErrInterrupt)?<code 337> (__U3ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x0000b8          0x4 LONG 0xfd16 DEFINED (__U3RXInterrupt)?<code 337> (__U3RXInterrupt):<code 337> (__DefaultInterrupt)
                  0x0000ba          0x4 LONG 0xfd16 DEFINED (__U3TXInterrupt)?<code 337> (__U3TXInterrupt):<code 337> (__DefaultInterrupt)
                  0x0000bc          0x4 LONG 0xfd16 DEFINED (__SI2C3Interrupt)?<code 337> (__SI2C3Interrupt):<code 337> (__DefaultInterrupt)
                  0x0000be          0x4 LONG 0xfd16 DEFINED (__MI2C3Interrupt)?<code 337> (__MI2C3Interrupt):<code 337> (__DefaultInterrupt)
                  0x0000c0          0x4 LONG 0x8b88 DEFINED (__USB1Interrupt)?<code 337> (__USB1Interrupt):<code 337> (__DefaultInterrupt)
                  0x0000c2          0x4 LONG 0xfd16 DEFINED (__U4ErrInterrupt)?<code 337> (__U4ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x0000c4          0x4 LONG 0xfd16 DEFINED (__U4RXInterrupt)?<code 337> (__U4RXInterrupt):<code 337> (__DefaultInterrupt)
                  0x0000c6          0x4 LONG 0xfd16 DEFINED (__U4TXInterrupt)?<code 337> (__U4TXInterrupt):<code 337> (__DefaultInterrupt)
                  0x0000c8          0x4 LONG 0xfd16 DEFINED (__SPI3ErrInterrupt)?<code 337> (__SPI3ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x0000ca          0x4 LONG 0xfd16 DEFINED (__SPI3Interrupt)?<code 337> (__SPI3Interrupt):<code 337> (__DefaultInterrupt)
                  0x0000cc          0x4 LONG 0xfd16 DEFINED (__OC9Interrupt)?<code 337> (__OC9Interrupt):<code 337> (__DefaultInterrupt)
                  0x0000ce          0x4 LONG 0xfd16 DEFINED (__IC9Interrupt)?<code 337> (__IC9Interrupt):<code 337> (__DefaultInterrupt)
                  0x0000d0          0x4 LONG 0xfd16 DEFINED (__Interrupt94)?<code 337> (__Interrupt94):<code 337> (__DefaultInterrupt)
                  0x0000d2          0x4 LONG 0xfd16 DEFINED (__Interrupt95)?<code 337> (__Interrupt95):<code 337> (__DefaultInterrupt)
                  0x0000d4          0x4 LONG 0xfd16 DEFINED (__Interrupt96)?<code 337> (__Interrupt96):<code 337> (__DefaultInterrupt)
                  0x0000d6          0x4 LONG 0xfd16 DEFINED (__Interrupt97)?<code 337> (__Interrupt97):<code 337> (__DefaultInterrupt)
                  0x0000d8          0x4 LONG 0xfd16 DEFINED (__Interrupt98)?<code 337> (__Interrupt98):<code 337> (__DefaultInterrupt)
                  0x0000da          0x4 LONG 0xfd16 DEFINED (__Interrupt99)?<code 337> (__Interrupt99):<code 337> (__DefaultInterrupt)
                  0x0000dc          0x4 LONG 0xfd16 DEFINED (__Interrupt100)?<code 337> (__Interrupt100):<code 337> (__DefaultInterrupt)
                  0x0000de          0x4 LONG 0xfd16 DEFINED (__Interrupt101)?<code 337> (__Interrupt101):<code 337> (__DefaultInterrupt)
                  0x0000e0          0x4 LONG 0xfd16 DEFINED (__Interrupt102)?<code 337> (__Interrupt102):<code 337> (__DefaultInterrupt)
                  0x0000e2          0x4 LONG 0xfd16 DEFINED (__Interrupt103)?<code 337> (__Interrupt103):<code 337> (__DefaultInterrupt)
                  0x0000e4          0x4 LONG 0xfd16 DEFINED (__Interrupt104)?<code 337> (__Interrupt104):<code 337> (__DefaultInterrupt)
                  0x0000e6          0x4 LONG 0xfd16 DEFINED (__Interrupt105)?<code 337> (__Interrupt105):<code 337> (__DefaultInterrupt)
                  0x0000e8          0x4 LONG 0xfd16 DEFINED (__Interrupt106)?<code 337> (__Interrupt106):<code 337> (__DefaultInterrupt)
                  0x0000ea          0x4 LONG 0xfd16 DEFINED (__Interrupt107)?<code 337> (__Interrupt107):<code 337> (__DefaultInterrupt)
                  0x0000ec          0x4 LONG 0xfd16 DEFINED (__Interrupt108)?<code 337> (__Interrupt108):<code 337> (__DefaultInterrupt)
                  0x0000ee          0x4 LONG 0xfd16 DEFINED (__Interrupt109)?<code 337> (__Interrupt109):<code 337> (__DefaultInterrupt)
                  0x0000f0          0x4 LONG 0xfd16 DEFINED (__Interrupt110)?<code 337> (__Interrupt110):<code 337> (__DefaultInterrupt)
                  0x0000f2          0x4 LONG 0xfd16 DEFINED (__Interrupt111)?<code 337> (__Interrupt111):<code 337> (__DefaultInterrupt)
                  0x0000f4          0x4 LONG 0xfd16 DEFINED (__Interrupt112)?<code 337> (__Interrupt112):<code 337> (__DefaultInterrupt)
                  0x0000f6          0x4 LONG 0xfd16 DEFINED (__Interrupt113)?<code 337> (__Interrupt113):<code 337> (__DefaultInterrupt)
                  0x0000f8          0x4 LONG 0xfd16 DEFINED (__Interrupt114)?<code 337> (__Interrupt114):<code 337> (__DefaultInterrupt)
                  0x0000fa          0x4 LONG 0xfd16 DEFINED (__Interrupt115)?<code 337> (__Interrupt115):<code 337> (__DefaultInterrupt)
                  0x0000fc          0x4 LONG 0xfd16 DEFINED (__Interrupt116)?<code 337> (__Interrupt116):<code 337> (__DefaultInterrupt)
                  0x0000fe          0x4 LONG 0xfd16 DEFINED (__Interrupt117)?<code 337> (__Interrupt117):<code 337> (__DefaultInterrupt)

.aivt             0x000104         0xfc
                  0x000104          0x4 LONG 0xfd16 DEFINED (__AltReservedTrap0)?<code 337> (__AltReservedTrap0):DEFINED (__ReservedTrap0)?<code 337> (__ReservedTrap0):<code 337> (__DefaultInterrupt)
                  0x000106          0x4 LONG 0xfd2a DEFINED (__AltOscillatorFail)?<code 337> (__AltOscillatorFail):DEFINED (__OscillatorFail)?<code 337> (__OscillatorFail):<code 337> (__DefaultInterrupt)
                  0x000108          0x4 LONG 0xfd3e DEFINED (__AltAddressError)?<code 337> (__AltAddressError):DEFINED (__AddressError)?<code 337> (__AddressError):<code 337> (__DefaultInterrupt)
                  0x00010a          0x4 LONG 0xfd52 DEFINED (__AltStackError)?<code 337> (__AltStackError):DEFINED (__StackError)?<code 337> (__StackError):<code 337> (__DefaultInterrupt)
                  0x00010c          0x4 LONG 0xfd66 DEFINED (__AltMathError)?<code 337> (__AltMathError):DEFINED (__MathError)?<code 337> (__MathError):<code 337> (__DefaultInterrupt)
                  0x00010e          0x4 LONG 0xfd16 DEFINED (__AltReservedTrap5)?<code 337> (__AltReservedTrap5):DEFINED (__ReservedTrap5)?<code 337> (__ReservedTrap5):<code 337> (__DefaultInterrupt)
                  0x000110          0x4 LONG 0xfd16 DEFINED (__AltReservedTrap6)?<code 337> (__AltReservedTrap6):DEFINED (__ReservedTrap6)?<code 337> (__ReservedTrap6):<code 337> (__DefaultInterrupt)
                  0x000112          0x4 LONG 0xfd16 DEFINED (__AltReservedTrap7)?<code 337> (__AltReservedTrap7):DEFINED (__ReservedTrap7)?<code 337> (__ReservedTrap7):<code 337> (__DefaultInterrupt)
                  0x000114          0x4 LONG 0xfd16 DEFINED (__AltINT0Interrupt)?<code 337> (__AltINT0Interrupt):DEFINED (__INT0Interrupt)?<code 337> (__INT0Interrupt):<code 337> (__DefaultInterrupt)
                  0x000116          0x4 LONG 0xfd16 DEFINED (__AltIC1Interrupt)?<code 337> (__AltIC1Interrupt):DEFINED (__IC1Interrupt)?<code 337> (__IC1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000118          0x4 LONG 0xfd16 DEFINED (__AltOC1Interrupt)?<code 337> (__AltOC1Interrupt):DEFINED (__OC1Interrupt)?<code 337> (__OC1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00011a          0x4 LONG 0xfd16 DEFINED (__AltT1Interrupt)?<code 337> (__AltT1Interrupt):DEFINED (__T1Interrupt)?<code 337> (__T1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00011c          0x4 LONG 0xfd16 DEFINED (__AltInterrupt4)?<code 337> (__AltInterrupt4):DEFINED (__Interrupt4)?<code 337> (__Interrupt4):<code 337> (__DefaultInterrupt)
                  0x00011e          0x4 LONG 0xfd16 DEFINED (__AltIC2Interrupt)?<code 337> (__AltIC2Interrupt):DEFINED (__IC2Interrupt)?<code 337> (__IC2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000120          0x4 LONG 0xfd16 DEFINED (__AltOC2Interrupt)?<code 337> (__AltOC2Interrupt):DEFINED (__OC2Interrupt)?<code 337> (__OC2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000122          0x4 LONG 0xfd16 DEFINED (__AltT2Interrupt)?<code 337> (__AltT2Interrupt):DEFINED (__T2Interrupt)?<code 337> (__T2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000124          0x4 LONG 0xfd16 DEFINED (__AltT3Interrupt)?<code 337> (__AltT3Interrupt):DEFINED (__T3Interrupt)?<code 337> (__T3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000126          0x4 LONG 0xfd16 DEFINED (__AltSPI1ErrInterrupt)?<code 337> (__AltSPI1ErrInterrupt):DEFINED (__SPI1ErrInterrupt)?<code 337> (__SPI1ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x000128          0x4 LONG 0xfd16 DEFINED (__AltSPI1Interrupt)?<code 337> (__AltSPI1Interrupt):DEFINED (__SPI1Interrupt)?<code 337> (__SPI1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00012a          0x4 LONG 0xfd16 DEFINED (__AltU1RXInterrupt)?<code 337> (__AltU1RXInterrupt):DEFINED (__U1RXInterrupt)?<code 337> (__U1RXInterrupt):<code 337> (__DefaultInterrupt)
                  0x00012c          0x4 LONG 0xfd16 DEFINED (__AltU1TXInterrupt)?<code 337> (__AltU1TXInterrupt):DEFINED (__U1TXInterrupt)?<code 337> (__U1TXInterrupt):<code 337> (__DefaultInterrupt)
                  0x00012e          0x4 LONG 0xfd16 DEFINED (__AltADC1Interrupt)?<code 337> (__AltADC1Interrupt):DEFINED (__ADC1Interrupt)?<code 337> (__ADC1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000130          0x4 LONG 0xfd16 DEFINED (__AltInterrupt14)?<code 337> (__AltInterrupt14):DEFINED (__Interrupt14)?<code 337> (__Interrupt14):<code 337> (__DefaultInterrupt)
                  0x000132          0x4 LONG 0xfd16 DEFINED (__AltInterrupt15)?<code 337> (__AltInterrupt15):DEFINED (__Interrupt15)?<code 337> (__Interrupt15):<code 337> (__DefaultInterrupt)
                  0x000134          0x4 LONG 0xfd16 DEFINED (__AltSI2C1Interrupt)?<code 337> (__AltSI2C1Interrupt):DEFINED (__SI2C1Interrupt)?<code 337> (__SI2C1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000136          0x4 LONG 0xfd16 DEFINED (__AltMI2C1Interrupt)?<code 337> (__AltMI2C1Interrupt):DEFINED (__MI2C1Interrupt)?<code 337> (__MI2C1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000138          0x4 LONG 0xfd16 DEFINED (__AltCompInterrupt)?<code 337> (__AltCompInterrupt):DEFINED (__CompInterrupt)?<code 337> (__CompInterrupt):<code 337> (__DefaultInterrupt)
                  0x00013a          0x4 LONG 0xfd16 DEFINED (__AltCNInterrupt)?<code 337> (__AltCNInterrupt):DEFINED (__CNInterrupt)?<code 337> (__CNInterrupt):<code 337> (__DefaultInterrupt)
                  0x00013c          0x4 LONG 0xfd16 DEFINED (__AltINT1Interrupt)?<code 337> (__AltINT1Interrupt):DEFINED (__INT1Interrupt)?<code 337> (__INT1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00013e          0x4 LONG 0xfd16 DEFINED (__AltInterrupt21)?<code 337> (__AltInterrupt21):DEFINED (__Interrupt21)?<code 337> (__Interrupt21):<code 337> (__DefaultInterrupt)
                  0x000140          0x4 LONG 0xfd16 DEFINED (__AltIC7Interrupt)?<code 337> (__AltIC7Interrupt):DEFINED (__IC7Interrupt)?<code 337> (__IC7Interrupt):<code 337> (__DefaultInterrupt)
                  0x000142          0x4 LONG 0xfd16 DEFINED (__AltIC8Interrupt)?<code 337> (__AltIC8Interrupt):DEFINED (__IC8Interrupt)?<code 337> (__IC8Interrupt):<code 337> (__DefaultInterrupt)
                  0x000144          0x4 LONG 0xfd16 DEFINED (__AltInterrupt24)?<code 337> (__AltInterrupt24):DEFINED (__Interrupt24)?<code 337> (__Interrupt24):<code 337> (__DefaultInterrupt)
                  0x000146          0x4 LONG 0xfd16 DEFINED (__AltOC3Interrupt)?<code 337> (__AltOC3Interrupt):DEFINED (__OC3Interrupt)?<code 337> (__OC3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000148          0x4 LONG 0xfd16 DEFINED (__AltOC4Interrupt)?<code 337> (__AltOC4Interrupt):DEFINED (__OC4Interrupt)?<code 337> (__OC4Interrupt):<code 337> (__DefaultInterrupt)
                  0x00014a          0x4 LONG 0xfce6 DEFINED (__AltT4Interrupt)?<code 337> (__AltT4Interrupt):DEFINED (__T4Interrupt)?<code 337> (__T4Interrupt):<code 337> (__DefaultInterrupt)
                  0x00014c          0x4 LONG 0xfd16 DEFINED (__AltT5Interrupt)?<code 337> (__AltT5Interrupt):DEFINED (__T5Interrupt)?<code 337> (__T5Interrupt):<code 337> (__DefaultInterrupt)
                  0x00014e          0x4 LONG 0xfd16 DEFINED (__AltINT2Interrupt)?<code 337> (__AltINT2Interrupt):DEFINED (__INT2Interrupt)?<code 337> (__INT2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000150          0x4 LONG 0xfd16 DEFINED (__AltU2RXInterrupt)?<code 337> (__AltU2RXInterrupt):DEFINED (__U2RXInterrupt)?<code 337> (__U2RXInterrupt):<code 337> (__DefaultInterrupt)
                  0x000152          0x4 LONG 0xfd16 DEFINED (__AltU2TXInterrupt)?<code 337> (__AltU2TXInterrupt):DEFINED (__U2TXInterrupt)?<code 337> (__U2TXInterrupt):<code 337> (__DefaultInterrupt)
                  0x000154          0x4 LONG 0xfd16 DEFINED (__AltSPI2ErrInterrupt)?<code 337> (__AltSPI2ErrInterrupt):DEFINED (__SPI2ErrInterrupt)?<code 337> (__SPI2ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x000156          0x4 LONG 0xfd16 DEFINED (__AltSPI2Interrupt)?<code 337> (__AltSPI2Interrupt):DEFINED (__SPI2Interrupt)?<code 337> (__SPI2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000158          0x4 LONG 0xfd16 DEFINED (__AltInterrupt34)?<code 337> (__AltInterrupt34):DEFINED (__Interrupt34)?<code 337> (__Interrupt34):<code 337> (__DefaultInterrupt)
                  0x00015a          0x4 LONG 0xfd16 DEFINED (__AltInterrupt35)?<code 337> (__AltInterrupt35):DEFINED (__Interrupt35)?<code 337> (__Interrupt35):<code 337> (__DefaultInterrupt)
                  0x00015c          0x4 LONG 0xfd16 DEFINED (__AltInterrupt36)?<code 337> (__AltInterrupt36):DEFINED (__Interrupt36)?<code 337> (__Interrupt36):<code 337> (__DefaultInterrupt)
                  0x00015e          0x4 LONG 0xfd16 DEFINED (__AltIC3Interrupt)?<code 337> (__AltIC3Interrupt):DEFINED (__IC3Interrupt)?<code 337> (__IC3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000160          0x4 LONG 0xfd16 DEFINED (__AltIC4Interrupt)?<code 337> (__AltIC4Interrupt):DEFINED (__IC4Interrupt)?<code 337> (__IC4Interrupt):<code 337> (__DefaultInterrupt)
                  0x000162          0x4 LONG 0xfd16 DEFINED (__AltIC5Interrupt)?<code 337> (__AltIC5Interrupt):DEFINED (__IC5Interrupt)?<code 337> (__IC5Interrupt):<code 337> (__DefaultInterrupt)
                  0x000164          0x4 LONG 0xfd16 DEFINED (__AltIC6Interrupt)?<code 337> (__AltIC6Interrupt):DEFINED (__IC6Interrupt)?<code 337> (__IC6Interrupt):<code 337> (__DefaultInterrupt)
                  0x000166          0x4 LONG 0xfd16 DEFINED (__AltOC5Interrupt)?<code 337> (__AltOC5Interrupt):DEFINED (__OC5Interrupt)?<code 337> (__OC5Interrupt):<code 337> (__DefaultInterrupt)
                  0x000168          0x4 LONG 0xfd16 DEFINED (__AltOC6Interrupt)?<code 337> (__AltOC6Interrupt):DEFINED (__OC6Interrupt)?<code 337> (__OC6Interrupt):<code 337> (__DefaultInterrupt)
                  0x00016a          0x4 LONG 0xfd16 DEFINED (__AltOC7Interrupt)?<code 337> (__AltOC7Interrupt):DEFINED (__OC7Interrupt)?<code 337> (__OC7Interrupt):<code 337> (__DefaultInterrupt)
                  0x00016c          0x4 LONG 0xfd16 DEFINED (__AltOC8Interrupt)?<code 337> (__AltOC8Interrupt):DEFINED (__OC8Interrupt)?<code 337> (__OC8Interrupt):<code 337> (__DefaultInterrupt)
                  0x00016e          0x4 LONG 0xfd16 DEFINED (__AltPMPInterrupt)?<code 337> (__AltPMPInterrupt):DEFINED (__PMPInterrupt)?<code 337> (__PMPInterrupt):<code 337> (__DefaultInterrupt)
                  0x000170          0x4 LONG 0xfd16 DEFINED (__AltInterrupt46)?<code 337> (__AltInterrupt46):DEFINED (__Interrupt46)?<code 337> (__Interrupt46):<code 337> (__DefaultInterrupt)
                  0x000172          0x4 LONG 0xfd16 DEFINED (__AltInterrupt47)?<code 337> (__AltInterrupt47):DEFINED (__Interrupt47)?<code 337> (__Interrupt47):<code 337> (__DefaultInterrupt)
                  0x000174          0x4 LONG 0xfd16 DEFINED (__AltInterrupt48)?<code 337> (__AltInterrupt48):DEFINED (__Interrupt48)?<code 337> (__Interrupt48):<code 337> (__DefaultInterrupt)
                  0x000176          0x4 LONG 0xfd16 DEFINED (__AltSI2C2Interrupt)?<code 337> (__AltSI2C2Interrupt):DEFINED (__SI2C2Interrupt)?<code 337> (__SI2C2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000178          0x4 LONG 0xfd16 DEFINED (__AltMI2C2Interrupt)?<code 337> (__AltMI2C2Interrupt):DEFINED (__MI2C2Interrupt)?<code 337> (__MI2C2Interrupt):<code 337> (__DefaultInterrupt)
                  0x00017a          0x4 LONG 0xfd16 DEFINED (__AltInterrupt51)?<code 337> (__AltInterrupt51):DEFINED (__Interrupt51)?<code 337> (__Interrupt51):<code 337> (__DefaultInterrupt)
                  0x00017c          0x4 LONG 0xfd16 DEFINED (__AltInterrupt52)?<code 337> (__AltInterrupt52):DEFINED (__Interrupt52)?<code 337> (__Interrupt52):<code 337> (__DefaultInterrupt)
                  0x00017e          0x4 LONG 0xfd16 DEFINED (__AltINT3Interrupt)?<code 337> (__AltINT3Interrupt):DEFINED (__INT3Interrupt)?<code 337> (__INT3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000180          0x4 LONG 0xfd16 DEFINED (__AltINT4Interrupt)?<code 337> (__AltINT4Interrupt):DEFINED (__INT4Interrupt)?<code 337> (__INT4Interrupt):<code 337> (__DefaultInterrupt)
                  0x000182          0x4 LONG 0xfd16 DEFINED (__AltInterrupt55)?<code 337> (__AltInterrupt55):DEFINED (__Interrupt55)?<code 337> (__Interrupt55):<code 337> (__DefaultInterrupt)
                  0x000184          0x4 LONG 0xfd16 DEFINED (__AltInterrupt56)?<code 337> (__AltInterrupt56):DEFINED (__Interrupt56)?<code 337> (__Interrupt56):<code 337> (__DefaultInterrupt)
                  0x000186          0x4 LONG 0xfd16 DEFINED (__AltInterrupt57)?<code 337> (__AltInterrupt57):DEFINED (__Interrupt57)?<code 337> (__Interrupt57):<code 337> (__DefaultInterrupt)
                  0x000188          0x4 LONG 0xfd16 DEFINED (__AltInterrupt58)?<code 337> (__AltInterrupt58):DEFINED (__Interrupt58)?<code 337> (__Interrupt58):<code 337> (__DefaultInterrupt)
                  0x00018a          0x4 LONG 0xfd16 DEFINED (__AltInterrupt59)?<code 337> (__AltInterrupt59):DEFINED (__Interrupt59)?<code 337> (__Interrupt59):<code 337> (__DefaultInterrupt)
                  0x00018c          0x4 LONG 0xfd16 DEFINED (__AltInterrupt60)?<code 337> (__AltInterrupt60):DEFINED (__Interrupt60)?<code 337> (__Interrupt60):<code 337> (__DefaultInterrupt)
                  0x00018e          0x4 LONG 0xfd16 DEFINED (__AltInterrupt61)?<code 337> (__AltInterrupt61):DEFINED (__Interrupt61)?<code 337> (__Interrupt61):<code 337> (__DefaultInterrupt)
                  0x000190          0x4 LONG 0xfd16 DEFINED (__AltRTCCInterrupt)?<code 337> (__AltRTCCInterrupt):DEFINED (__RTCCInterrupt)?<code 337> (__RTCCInterrupt):<code 337> (__DefaultInterrupt)
                  0x000192          0x4 LONG 0xfd16 DEFINED (__AltInterrupt63)?<code 337> (__AltInterrupt63):DEFINED (__Interrupt63)?<code 337> (__Interrupt63):<code 337> (__DefaultInterrupt)
                  0x000194          0x4 LONG 0xfd16 DEFINED (__AltInterrupt64)?<code 337> (__AltInterrupt64):DEFINED (__Interrupt64)?<code 337> (__Interrupt64):<code 337> (__DefaultInterrupt)
                  0x000196          0x4 LONG 0xfd16 DEFINED (__AltU1ErrInterrupt)?<code 337> (__AltU1ErrInterrupt):DEFINED (__U1ErrInterrupt)?<code 337> (__U1ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x000198          0x4 LONG 0xfd16 DEFINED (__AltU2ErrInterrupt)?<code 337> (__AltU2ErrInterrupt):DEFINED (__U2ErrInterrupt)?<code 337> (__U2ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x00019a          0x4 LONG 0xfd16 DEFINED (__AltCRCInterrupt)?<code 337> (__AltCRCInterrupt):DEFINED (__CRCInterrupt)?<code 337> (__CRCInterrupt):<code 337> (__DefaultInterrupt)
                  0x00019c          0x4 LONG 0xfd16 DEFINED (__AltInterrupt68)?<code 337> (__AltInterrupt68):DEFINED (__Interrupt68)?<code 337> (__Interrupt68):<code 337> (__DefaultInterrupt)
                  0x00019e          0x4 LONG 0xfd16 DEFINED (__AltInterrupt69)?<code 337> (__AltInterrupt69):DEFINED (__Interrupt69)?<code 337> (__Interrupt69):<code 337> (__DefaultInterrupt)
                  0x0001a0          0x4 LONG 0xfd16 DEFINED (__AltInterrupt70)?<code 337> (__AltInterrupt70):DEFINED (__Interrupt70)?<code 337> (__Interrupt70):<code 337> (__DefaultInterrupt)
                  0x0001a2          0x4 LONG 0xfd16 DEFINED (__AltInterrupt71)?<code 337> (__AltInterrupt71):DEFINED (__Interrupt71)?<code 337> (__Interrupt71):<code 337> (__DefaultInterrupt)
                  0x0001a4          0x4 LONG 0xfd16 DEFINED (__AltLVDInterrupt)?<code 337> (__AltLVDInterrupt):DEFINED (__LVDInterrupt)?<code 337> (__LVDInterrupt):<code 337> (__DefaultInterrupt)
                  0x0001a6          0x4 LONG 0xfd16 DEFINED (__AltInterrupt73)?<code 337> (__AltInterrupt73):DEFINED (__Interrupt73)?<code 337> (__Interrupt73):<code 337> (__DefaultInterrupt)
                  0x0001a8          0x4 LONG 0xfd16 DEFINED (__AltInterrupt74)?<code 337> (__AltInterrupt74):DEFINED (__Interrupt74)?<code 337> (__Interrupt74):<code 337> (__DefaultInterrupt)
                  0x0001aa          0x4 LONG 0xfd16 DEFINED (__AltInterrupt75)?<code 337> (__AltInterrupt75):DEFINED (__Interrupt75)?<code 337> (__Interrupt75):<code 337> (__DefaultInterrupt)
                  0x0001ac          0x4 LONG 0xfd16 DEFINED (__AltInterrupt76)?<code 337> (__AltInterrupt76):DEFINED (__Interrupt76)?<code 337> (__Interrupt76):<code 337> (__DefaultInterrupt)
                  0x0001ae          0x4 LONG 0xfd16 DEFINED (__AltCTMUInterrupt)?<code 337> (__AltCTMUInterrupt):DEFINED (__CTMUInterrupt)?<code 337> (__CTMUInterrupt):<code 337> (__DefaultInterrupt)
                  0x0001b0          0x4 LONG 0xfd16 DEFINED (__AltInterrupt78)?<code 337> (__AltInterrupt78):DEFINED (__Interrupt78)?<code 337> (__Interrupt78):<code 337> (__DefaultInterrupt)
                  0x0001b2          0x4 LONG 0xfd16 DEFINED (__AltInterrupt79)?<code 337> (__AltInterrupt79):DEFINED (__Interrupt79)?<code 337> (__Interrupt79):<code 337> (__DefaultInterrupt)
                  0x0001b4          0x4 LONG 0xfd16 DEFINED (__AltInterrupt80)?<code 337> (__AltInterrupt80):DEFINED (__Interrupt80)?<code 337> (__Interrupt80):<code 337> (__DefaultInterrupt)
                  0x0001b6          0x4 LONG 0xfd16 DEFINED (__AltU3ErrInterrupt)?<code 337> (__AltU3ErrInterrupt):DEFINED (__U3ErrInterrupt)?<code 337> (__U3ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x0001b8          0x4 LONG 0xfd16 DEFINED (__AltU3RXInterrupt)?<code 337> (__AltU3RXInterrupt):DEFINED (__U3RXInterrupt)?<code 337> (__U3RXInterrupt):<code 337> (__DefaultInterrupt)
                  0x0001ba          0x4 LONG 0xfd16 DEFINED (__AltU3TXInterrupt)?<code 337> (__AltU3TXInterrupt):DEFINED (__U3TXInterrupt)?<code 337> (__U3TXInterrupt):<code 337> (__DefaultInterrupt)
                  0x0001bc          0x4 LONG 0xfd16 DEFINED (__AltSI2C3Interrupt)?<code 337> (__AltSI2C3Interrupt):DEFINED (__SI2C3Interrupt)?<code 337> (__SI2C3Interrupt):<code 337> (__DefaultInterrupt)
                  0x0001be          0x4 LONG 0xfd16 DEFINED (__AltMI2C3Interrupt)?<code 337> (__AltMI2C3Interrupt):DEFINED (__MI2C3Interrupt)?<code 337> (__MI2C3Interrupt):<code 337> (__DefaultInterrupt)
                  0x0001c0          0x4 LONG 0x8b88 DEFINED (__AltUSB1Interrupt)?<code 337> (__AltUSB1Interrupt):DEFINED (__USB1Interrupt)?<code 337> (__USB1Interrupt):<code 337> (__DefaultInterrupt)
                  0x0001c2          0x4 LONG 0xfd16 DEFINED (__AltU4ErrInterrupt)?<code 337> (__AltU4ErrInterrupt):DEFINED (__U4ErrInterrupt)?<code 337> (__U4ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x0001c4          0x4 LONG 0xfd16 DEFINED (__AltU4RXInterrupt)?<code 337> (__AltU4RXInterrupt):DEFINED (__U4RXInterrupt)?<code 337> (__U4RXInterrupt):<code 337> (__DefaultInterrupt)
                  0x0001c6          0x4 LONG 0xfd16 DEFINED (__AltU4TXInterrupt)?<code 337> (__AltU4TXInterrupt):DEFINED (__U4TXInterrupt)?<code 337> (__U4TXInterrupt):<code 337> (__DefaultInterrupt)
                  0x0001c8          0x4 LONG 0xfd16 DEFINED (__AltSPI3ErrInterrupt)?<code 337> (__AltSPI3ErrInterrupt):DEFINED (__SPI3ErrInterrupt)?<code 337> (__SPI3ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x0001ca          0x4 LONG 0xfd16 DEFINED (__AltSPI3Interrupt)?<code 337> (__AltSPI3Interrupt):DEFINED (__SPI3Interrupt)?<code 337> (__SPI3Interrupt):<code 337> (__DefaultInterrupt)
                  0x0001cc          0x4 LONG 0xfd16 DEFINED (__AltOC9Interrupt)?<code 337> (__AltOC9Interrupt):DEFINED (__OC9Interrupt)?<code 337> (__OC9Interrupt):<code 337> (__DefaultInterrupt)
                  0x0001ce          0x4 LONG 0xfd16 DEFINED (__AltIC9Interrupt)?<code 337> (__AltIC9Interrupt):DEFINED (__IC9Interrupt)?<code 337> (__IC9Interrupt):<code 337> (__DefaultInterrupt)
                  0x0001d0          0x4 LONG 0xfd16 DEFINED (__AltInterrupt94)?<code 337> (__AltInterrupt94):DEFINED (__Interrupt94)?<code 337> (__Interrupt94):<code 337> (__DefaultInterrupt)
                  0x0001d2          0x4 LONG 0xfd16 DEFINED (__AltInterrupt95)?<code 337> (__AltInterrupt95):DEFINED (__Interrupt95)?<code 337> (__Interrupt95):<code 337> (__DefaultInterrupt)
                  0x0001d4          0x4 LONG 0xfd16 DEFINED (__AltInterrupt96)?<code 337> (__AltInterrupt96):DEFINED (__Interrupt96)?<code 337> (__Interrupt96):<code 337> (__DefaultInterrupt)
                  0x0001d6          0x4 LONG 0xfd16 DEFINED (__AltInterrupt97)?<code 337> (__AltInterrupt97):DEFINED (__Interrupt97)?<code 337> (__Interrupt97):<code 337> (__DefaultInterrupt)
                  0x0001d8          0x4 LONG 0xfd16 DEFINED (__AltInterrupt98)?<code 337> (__AltInterrupt98):DEFINED (__Interrupt98)?<code 337> (__Interrupt98):<code 337> (__DefaultInterrupt)
                  0x0001da          0x4 LONG 0xfd16 DEFINED (__AltInterrupt99)?<code 337> (__AltInterrupt99):DEFINED (__Interrupt99)?<code 337> (__Interrupt99):<code 337> (__DefaultInterrupt)
                  0x0001dc          0x4 LONG 0xfd16 DEFINED (__AltInterrupt100)?<code 337> (__AltInterrupt100):DEFINED (__Interrupt100)?<code 337> (__Interrupt100):<code 337> (__DefaultInterrupt)
                  0x0001de          0x4 LONG 0xfd16 DEFINED (__AltInterrupt101)?<code 337> (__AltInterrupt101):DEFINED (__Interrupt101)?<code 337> (__Interrupt101):<code 337> (__DefaultInterrupt)
                  0x0001e0          0x4 LONG 0xfd16 DEFINED (__AltInterrupt102)?<code 337> (__AltInterrupt102):DEFINED (__Interrupt102)?<code 337> (__Interrupt102):<code 337> (__DefaultInterrupt)
                  0x0001e2          0x4 LONG 0xfd16 DEFINED (__AltInterrupt103)?<code 337> (__AltInterrupt103):DEFINED (__Interrupt103)?<code 337> (__Interrupt103):<code 337> (__DefaultInterrupt)
                  0x0001e4          0x4 LONG 0xfd16 DEFINED (__AltInterrupt104)?<code 337> (__AltInterrupt104):DEFINED (__Interrupt104)?<code 337> (__Interrupt104):<code 337> (__DefaultInterrupt)
                  0x0001e6          0x4 LONG 0xfd16 DEFINED (__AltInterrupt105)?<code 337> (__AltInterrupt105):DEFINED (__Interrupt105)?<code 337> (__Interrupt105):<code 337> (__DefaultInterrupt)
                  0x0001e8          0x4 LONG 0xfd16 DEFINED (__AltInterrupt106)?<code 337> (__AltInterrupt106):DEFINED (__Interrupt106)?<code 337> (__Interrupt106):<code 337> (__DefaultInterrupt)
                  0x0001ea          0x4 LONG 0xfd16 DEFINED (__AltInterrupt107)?<code 337> (__AltInterrupt107):DEFINED (__Interrupt107)?<code 337> (__Interrupt107):<code 337> (__DefaultInterrupt)
                  0x0001ec          0x4 LONG 0xfd16 DEFINED (__AltInterrupt108)?<code 337> (__AltInterrupt108):DEFINED (__Interrupt108)?<code 337> (__Interrupt108):<code 337> (__DefaultInterrupt)
                  0x0001ee          0x4 LONG 0xfd16 DEFINED (__AltInterrupt109)?<code 337> (__AltInterrupt109):DEFINED (__Interrupt109)?<code 337> (__Interrupt109):<code 337> (__DefaultInterrupt)
                  0x0001f0          0x4 LONG 0xfd16 DEFINED (__AltInterrupt110)?<code 337> (__AltInterrupt110):DEFINED (__Interrupt110)?<code 337> (__Interrupt110):<code 337> (__DefaultInterrupt)
                  0x0001f2          0x4 LONG 0xfd16 DEFINED (__AltInterrupt111)?<code 337> (__AltInterrupt111):DEFINED (__Interrupt111)?<code 337> (__Interrupt111):<code 337> (__DefaultInterrupt)
                  0x0001f4          0x4 LONG 0xfd16 DEFINED (__AltInterrupt112)?<code 337> (__AltInterrupt112):DEFINED (__Interrupt112)?<code 337> (__Interrupt112):<code 337> (__DefaultInterrupt)
                  0x0001f6          0x4 LONG 0xfd16 DEFINED (__AltInterrupt113)?<code 337> (__AltInterrupt113):DEFINED (__Interrupt113)?<code 337> (__Interrupt113):<code 337> (__DefaultInterrupt)
                  0x0001f8          0x4 LONG 0xfd16 DEFINED (__AltInterrupt114)?<code 337> (__AltInterrupt114):DEFINED (__Interrupt114)?<code 337> (__Interrupt114):<code 337> (__DefaultInterrupt)
                  0x0001fa          0x4 LONG 0xfd16 DEFINED (__AltInterrupt115)?<code 337> (__AltInterrupt115):DEFINED (__Interrupt115)?<code 337> (__Interrupt115):<code 337> (__DefaultInterrupt)
                  0x0001fc          0x4 LONG 0xfd16 DEFINED (__AltInterrupt116)?<code 337> (__AltInterrupt116):DEFINED (__Interrupt116)?<code 337> (__Interrupt116):<code 337> (__DefaultInterrupt)
                  0x0001fe          0x4 LONG 0xfd16 DEFINED (__AltInterrupt117)?<code 337> (__AltInterrupt117):DEFINED (__Interrupt117)?<code 337> (__Interrupt117):<code 337> (__DefaultInterrupt)
                    0x0000                  WREG0 = 0x0
                    0x0000                  _WREG0 = 0x0
                    0x0002                  WREG1 = 0x2
                    0x0002                  _WREG1 = 0x2
                    0x0004                  WREG2 = 0x4
                    0x0004                  _WREG2 = 0x4
                    0x0006                  WREG3 = 0x6
                    0x0006                  _WREG3 = 0x6
                    0x0008                  WREG4 = 0x8
                    0x0008                  _WREG4 = 0x8
                    0x000a                  WREG5 = 0xa
                    0x000a                  _WREG5 = 0xa
                    0x000c                  WREG6 = 0xc
                    0x000c                  _WREG6 = 0xc
                    0x000e                  WREG7 = 0xe
                    0x000e                  _WREG7 = 0xe
                    0x0010                  WREG8 = 0x10
                    0x0010                  _WREG8 = 0x10
                    0x0012                  WREG9 = 0x12
                    0x0012                  _WREG9 = 0x12
                    0x0014                  WREG10 = 0x14
                    0x0014                  _WREG10 = 0x14
                    0x0016                  WREG11 = 0x16
                    0x0016                  _WREG11 = 0x16
                    0x0018                  WREG12 = 0x18
                    0x0018                  _WREG12 = 0x18
                    0x001a                  WREG13 = 0x1a
                    0x001a                  _WREG13 = 0x1a
                    0x001c                  WREG14 = 0x1c
                    0x001c                  _WREG14 = 0x1c
                    0x001e                  WREG15 = 0x1e
                    0x001e                  _WREG15 = 0x1e
                    0x0020                  SPLIM = 0x20
                    0x0020                  _SPLIM = 0x20
                    0x002e                  PCL = 0x2e
                    0x002e                  _PCL = 0x2e
                    0x0030                  PCH = 0x30
                    0x0030                  _PCH = 0x30
                    0x0032                  TBLPAG = 0x32
                    0x0032                  _TBLPAG = 0x32
                    0x0034                  PSVPAG = 0x34
                    0x0034                  _PSVPAG = 0x34
                    0x0036                  RCOUNT = 0x36
                    0x0036                  _RCOUNT = 0x36
                    0x0042                  SR = 0x42
                    0x0042                  _SR = 0x42
                    0x0042                  _SRbits = 0x42
                    0x0044                  CORCON = 0x44
                    0x0044                  _CORCON = 0x44
                    0x0044                  _CORCONbits = 0x44
                    0x0052                  DISICNT = 0x52
                    0x0052                  _DISICNT = 0x52
                    0x0054                  CNPD1 = 0x54
                    0x0054                  _CNPD1 = 0x54
                    0x0054                  _CNPD1bits = 0x54
                    0x0056                  CNPD2 = 0x56
                    0x0056                  _CNPD2 = 0x56
                    0x0056                  _CNPD2bits = 0x56
                    0x0058                  CNPD3 = 0x58
                    0x0058                  _CNPD3 = 0x58
                    0x0058                  _CNPD3bits = 0x58
                    0x005a                  CNPD4 = 0x5a
                    0x005a                  _CNPD4 = 0x5a
                    0x005a                  _CNPD4bits = 0x5a
                    0x005c                  CNPD5 = 0x5c
                    0x005c                  _CNPD5 = 0x5c
                    0x005c                  _CNPD5bits = 0x5c
                    0x0060                  CNEN1 = 0x60
                    0x0060                  _CNEN1 = 0x60
                    0x0060                  _CNEN1bits = 0x60
                    0x0062                  CNEN2 = 0x62
                    0x0062                  _CNEN2 = 0x62
                    0x0062                  _CNEN2bits = 0x62
                    0x0064                  CNEN3 = 0x64
                    0x0064                  _CNEN3 = 0x64
                    0x0064                  _CNEN3bits = 0x64
                    0x0066                  CNEN4 = 0x66
                    0x0066                  _CNEN4 = 0x66
                    0x0066                  _CNEN4bits = 0x66
                    0x0068                  CNEN5 = 0x68
                    0x0068                  _CNEN5 = 0x68
                    0x0068                  _CNEN5bits = 0x68
                    0x006c                  CNPU1 = 0x6c
                    0x006c                  _CNPU1 = 0x6c
                    0x006c                  _CNPU1bits = 0x6c
                    0x006e                  CNPU2 = 0x6e
                    0x006e                  _CNPU2 = 0x6e
                    0x006e                  _CNPU2bits = 0x6e
                    0x0070                  CNPU3 = 0x70
                    0x0070                  _CNPU3 = 0x70
                    0x0070                  _CNPU3bits = 0x70
                    0x0072                  CNPU4 = 0x72
                    0x0072                  _CNPU4 = 0x72
                    0x0072                  _CNPU4bits = 0x72
                    0x0074                  CNPU5 = 0x74
                    0x0074                  _CNPU5 = 0x74
                    0x0074                  _CNPU5bits = 0x74
                    0x0080                  INTCON1 = 0x80
                    0x0080                  _INTCON1 = 0x80
                    0x0080                  _INTCON1bits = 0x80
                    0x0082                  INTCON2 = 0x82
                    0x0082                  _INTCON2 = 0x82
                    0x0082                  _INTCON2bits = 0x82
                    0x0084                  IFS0 = 0x84
                    0x0084                  _IFS0 = 0x84
                    0x0084                  _IFS0bits = 0x84
                    0x0086                  IFS1 = 0x86
                    0x0086                  _IFS1 = 0x86
                    0x0086                  _IFS1bits = 0x86
                    0x0088                  IFS2 = 0x88
                    0x0088                  _IFS2 = 0x88
                    0x0088                  _IFS2bits = 0x88
                    0x008a                  IFS3 = 0x8a
                    0x008a                  _IFS3 = 0x8a
                    0x008a                  _IFS3bits = 0x8a
                    0x008c                  IFS4 = 0x8c
                    0x008c                  _IFS4 = 0x8c
                    0x008c                  _IFS4bits = 0x8c
                    0x008e                  IFS5 = 0x8e
                    0x008e                  _IFS5 = 0x8e
                    0x008e                  _IFS5bits = 0x8e
                    0x0094                  IEC0 = 0x94
                    0x0094                  _IEC0 = 0x94
                    0x0094                  _IEC0bits = 0x94
                    0x0096                  IEC1 = 0x96
                    0x0096                  _IEC1 = 0x96
                    0x0096                  _IEC1bits = 0x96
                    0x0098                  IEC2 = 0x98
                    0x0098                  _IEC2 = 0x98
                    0x0098                  _IEC2bits = 0x98
                    0x009a                  IEC3 = 0x9a
                    0x009a                  _IEC3 = 0x9a
                    0x009a                  _IEC3bits = 0x9a
                    0x009c                  IEC4 = 0x9c
                    0x009c                  _IEC4 = 0x9c
                    0x009c                  _IEC4bits = 0x9c
                    0x009e                  IEC5 = 0x9e
                    0x009e                  _IEC5 = 0x9e
                    0x009e                  _IEC5bits = 0x9e
                    0x00a4                  IPC0 = 0xa4
                    0x00a4                  _IPC0 = 0xa4
                    0x00a4                  _IPC0bits = 0xa4
                    0x00a6                  IPC1 = 0xa6
                    0x00a6                  _IPC1 = 0xa6
                    0x00a6                  _IPC1bits = 0xa6
                    0x00a8                  IPC2 = 0xa8
                    0x00a8                  _IPC2 = 0xa8
                    0x00a8                  _IPC2bits = 0xa8
                    0x00aa                  IPC3 = 0xaa
                    0x00aa                  _IPC3 = 0xaa
                    0x00aa                  _IPC3bits = 0xaa
                    0x00ac                  IPC4 = 0xac
                    0x00ac                  _IPC4 = 0xac
                    0x00ac                  _IPC4bits = 0xac
                    0x00ae                  IPC5 = 0xae
                    0x00ae                  _IPC5 = 0xae
                    0x00ae                  _IPC5bits = 0xae
                    0x00b0                  IPC6 = 0xb0
                    0x00b0                  _IPC6 = 0xb0
                    0x00b0                  _IPC6bits = 0xb0
                    0x00b2                  IPC7 = 0xb2
                    0x00b2                  _IPC7 = 0xb2
                    0x00b2                  _IPC7bits = 0xb2
                    0x00b4                  IPC8 = 0xb4
                    0x00b4                  _IPC8 = 0xb4
                    0x00b4                  _IPC8bits = 0xb4
                    0x00b6                  IPC9 = 0xb6
                    0x00b6                  _IPC9 = 0xb6
                    0x00b6                  _IPC9bits = 0xb6
                    0x00b8                  IPC10 = 0xb8
                    0x00b8                  _IPC10 = 0xb8
                    0x00b8                  _IPC10bits = 0xb8
                    0x00ba                  IPC11 = 0xba
                    0x00ba                  _IPC11 = 0xba
                    0x00ba                  _IPC11bits = 0xba
                    0x00bc                  IPC12 = 0xbc
                    0x00bc                  _IPC12 = 0xbc
                    0x00bc                  _IPC12bits = 0xbc
                    0x00be                  IPC13 = 0xbe
                    0x00be                  _IPC13 = 0xbe
                    0x00be                  _IPC13bits = 0xbe
                    0x00c2                  IPC15 = 0xc2
                    0x00c2                  _IPC15 = 0xc2
                    0x00c2                  _IPC15bits = 0xc2
                    0x00c4                  IPC16 = 0xc4
                    0x00c4                  _IPC16 = 0xc4
                    0x00c4                  _IPC16bits = 0xc4
                    0x00c8                  IPC18 = 0xc8
                    0x00c8                  _IPC18 = 0xc8
                    0x00c8                  _IPC18bits = 0xc8
                    0x00ca                  IPC19 = 0xca
                    0x00ca                  _IPC19 = 0xca
                    0x00ca                  _IPC19bits = 0xca
                    0x00cc                  IPC20 = 0xcc
                    0x00cc                  _IPC20 = 0xcc
                    0x00cc                  _IPC20bits = 0xcc
                    0x00ce                  IPC21 = 0xce
                    0x00ce                  _IPC21 = 0xce
                    0x00ce                  _IPC21bits = 0xce
                    0x00d0                  IPC22 = 0xd0
                    0x00d0                  _IPC22 = 0xd0
                    0x00d0                  _IPC22bits = 0xd0
                    0x00d2                  IPC23 = 0xd2
                    0x00d2                  _IPC23 = 0xd2
                    0x00d2                  _IPC23bits = 0xd2
                    0x0100                  TMR1 = 0x100
                    0x0100                  _TMR1 = 0x100
                    0x0102                  PR1 = 0x102
                    0x0102                  _PR1 = 0x102
                    0x0104                  T1CON = 0x104
                    0x0104                  _T1CON = 0x104
                    0x0104                  _T1CONbits = 0x104
                    0x0106                  TMR2 = 0x106
                    0x0106                  _TMR2 = 0x106
                    0x0108                  TMR3HLD = 0x108
                    0x0108                  _TMR3HLD = 0x108
                    0x010a                  TMR3 = 0x10a
                    0x010a                  _TMR3 = 0x10a
                    0x010c                  PR2 = 0x10c
                    0x010c                  _PR2 = 0x10c
                    0x010e                  PR3 = 0x10e
                    0x010e                  _PR3 = 0x10e
                    0x0110                  T2CON = 0x110
                    0x0110                  _T2CON = 0x110
                    0x0110                  _T2CONbits = 0x110
                    0x0112                  T3CON = 0x112
                    0x0112                  _T3CON = 0x112
                    0x0112                  _T3CONbits = 0x112
                    0x0114                  TMR4 = 0x114
                    0x0114                  _TMR4 = 0x114
                    0x0116                  TMR5HLD = 0x116
                    0x0116                  _TMR5HLD = 0x116
                    0x0118                  TMR5 = 0x118
                    0x0118                  _TMR5 = 0x118
                    0x011a                  PR4 = 0x11a
                    0x011a                  _PR4 = 0x11a
                    0x011c                  PR5 = 0x11c
                    0x011c                  _PR5 = 0x11c
                    0x011e                  T4CON = 0x11e
                    0x011e                  _T4CON = 0x11e
                    0x011e                  _T4CONbits = 0x11e
                    0x0120                  T5CON = 0x120
                    0x0120                  _T5CON = 0x120
                    0x0120                  _T5CONbits = 0x120
                    0x0140                  IC1CON1 = 0x140
                    0x0140                  _IC1CON1 = 0x140
                    0x0140                  _IC1CON1bits = 0x140
                    0x0142                  IC1CON2 = 0x142
                    0x0142                  _IC1CON2 = 0x142
                    0x0142                  _IC1CON2bits = 0x142
                    0x0144                  IC1BUF = 0x144
                    0x0144                  _IC1BUF = 0x144
                    0x0146                  IC1TMR = 0x146
                    0x0146                  _IC1TMR = 0x146
                    0x0148                  IC2CON1 = 0x148
                    0x0148                  _IC2CON1 = 0x148
                    0x0148                  _IC2CON1bits = 0x148
                    0x014a                  IC2CON2 = 0x14a
                    0x014a                  _IC2CON2 = 0x14a
                    0x014a                  _IC2CON2bits = 0x14a
                    0x014c                  IC2BUF = 0x14c
                    0x014c                  _IC2BUF = 0x14c
                    0x014e                  IC2TMR = 0x14e
                    0x014e                  _IC2TMR = 0x14e
                    0x0150                  IC3CON1 = 0x150
                    0x0150                  _IC3CON1 = 0x150
                    0x0150                  _IC3CON1bits = 0x150
                    0x0152                  IC3CON2 = 0x152
                    0x0152                  _IC3CON2 = 0x152
                    0x0152                  _IC3CON2bits = 0x152
                    0x0154                  IC3BUF = 0x154
                    0x0154                  _IC3BUF = 0x154
                    0x0156                  IC3TMR = 0x156
                    0x0156                  _IC3TMR = 0x156
                    0x0158                  IC4CON1 = 0x158
                    0x0158                  _IC4CON1 = 0x158
                    0x0158                  _IC4CON1bits = 0x158
                    0x015a                  IC4CON2 = 0x15a
                    0x015a                  _IC4CON2 = 0x15a
                    0x015a                  _IC4CON2bits = 0x15a
                    0x015c                  IC4BUF = 0x15c
                    0x015c                  _IC4BUF = 0x15c
                    0x015e                  IC4TMR = 0x15e
                    0x015e                  _IC4TMR = 0x15e
                    0x0160                  IC5CON1 = 0x160
                    0x0160                  _IC5CON1 = 0x160
                    0x0160                  _IC5CON1bits = 0x160
                    0x0162                  IC5CON2 = 0x162
                    0x0162                  _IC5CON2 = 0x162
                    0x0162                  _IC5CON2bits = 0x162
                    0x0164                  IC5BUF = 0x164
                    0x0164                  _IC5BUF = 0x164
                    0x0166                  IC5TMR = 0x166
                    0x0166                  _IC5TMR = 0x166
                    0x0168                  IC6CON1 = 0x168
                    0x0168                  _IC6CON1 = 0x168
                    0x0168                  _IC6CON1bits = 0x168
                    0x016a                  IC6CON2 = 0x16a
                    0x016a                  _IC6CON2 = 0x16a
                    0x016a                  _IC6CON2bits = 0x16a
                    0x016c                  IC6BUF = 0x16c
                    0x016c                  _IC6BUF = 0x16c
                    0x016e                  IC6TMR = 0x16e
                    0x016e                  _IC6TMR = 0x16e
                    0x0170                  IC7CON1 = 0x170
                    0x0170                  _IC7CON1 = 0x170
                    0x0170                  _IC7CON1bits = 0x170
                    0x0172                  IC7CON2 = 0x172
                    0x0172                  _IC7CON2 = 0x172
                    0x0172                  _IC7CON2bits = 0x172
                    0x0174                  IC7BUF = 0x174
                    0x0174                  _IC7BUF = 0x174
                    0x0176                  IC7TMR = 0x176
                    0x0176                  _IC7TMR = 0x176
                    0x0178                  IC8CON1 = 0x178
                    0x0178                  _IC8CON1 = 0x178
                    0x0178                  _IC8CON1bits = 0x178
                    0x017a                  IC8CON2 = 0x17a
                    0x017a                  _IC8CON2 = 0x17a
                    0x017a                  _IC8CON2bits = 0x17a
                    0x017c                  IC8BUF = 0x17c
                    0x017c                  _IC8BUF = 0x17c
                    0x017e                  IC8TMR = 0x17e
                    0x017e                  _IC8TMR = 0x17e
                    0x0180                  IC9CON1 = 0x180
                    0x0180                  _IC9CON1 = 0x180
                    0x0180                  _IC9CON1bits = 0x180
                    0x0182                  IC9CON2 = 0x182
                    0x0182                  _IC9CON2 = 0x182
                    0x0182                  _IC9CON2bits = 0x182
                    0x0184                  IC9BUF = 0x184
                    0x0184                  _IC9BUF = 0x184
                    0x0186                  IC9TMR = 0x186
                    0x0186                  _IC9TMR = 0x186
                    0x0190                  OC1CON1 = 0x190
                    0x0190                  _OC1CON1 = 0x190
                    0x0190                  _OC1CON1bits = 0x190
                    0x0192                  OC1CON2 = 0x192
                    0x0192                  _OC1CON2 = 0x192
                    0x0192                  _OC1CON2bits = 0x192
                    0x0194                  OC1RS = 0x194
                    0x0194                  _OC1RS = 0x194
                    0x0196                  OC1R = 0x196
                    0x0196                  _OC1R = 0x196
                    0x0198                  OC1TMR = 0x198
                    0x0198                  _OC1TMR = 0x198
                    0x019a                  OC2CON1 = 0x19a
                    0x019a                  _OC2CON1 = 0x19a
                    0x019a                  _OC2CON1bits = 0x19a
                    0x019c                  OC2CON2 = 0x19c
                    0x019c                  _OC2CON2 = 0x19c
                    0x019c                  _OC2CON2bits = 0x19c
                    0x019e                  OC2RS = 0x19e
                    0x019e                  _OC2RS = 0x19e
                    0x01a0                  OC2R = 0x1a0
                    0x01a0                  _OC2R = 0x1a0
                    0x01a2                  OC2TMR = 0x1a2
                    0x01a2                  _OC2TMR = 0x1a2
                    0x01a4                  OC3CON1 = 0x1a4
                    0x01a4                  _OC3CON1 = 0x1a4
                    0x01a4                  _OC3CON1bits = 0x1a4
                    0x01a6                  OC3CON2 = 0x1a6
                    0x01a6                  _OC3CON2 = 0x1a6
                    0x01a6                  _OC3CON2bits = 0x1a6
                    0x01a8                  OC3RS = 0x1a8
                    0x01a8                  _OC3RS = 0x1a8
                    0x01aa                  OC3R = 0x1aa
                    0x01aa                  _OC3R = 0x1aa
                    0x01ac                  OC3TMR = 0x1ac
                    0x01ac                  _OC3TMR = 0x1ac
                    0x01ae                  OC4CON1 = 0x1ae
                    0x01ae                  _OC4CON1 = 0x1ae
                    0x01ae                  _OC4CON1bits = 0x1ae
                    0x01b0                  OC4CON2 = 0x1b0
                    0x01b0                  _OC4CON2 = 0x1b0
                    0x01b0                  _OC4CON2bits = 0x1b0
                    0x01b2                  OC4RS = 0x1b2
                    0x01b2                  _OC4RS = 0x1b2
                    0x01b4                  OC4R = 0x1b4
                    0x01b4                  _OC4R = 0x1b4
                    0x01b6                  OC4TMR = 0x1b6
                    0x01b6                  _OC4TMR = 0x1b6
                    0x01b8                  OC5CON1 = 0x1b8
                    0x01b8                  _OC5CON1 = 0x1b8
                    0x01b8                  _OC5CON1bits = 0x1b8
                    0x01ba                  OC5CON2 = 0x1ba
                    0x01ba                  _OC5CON2 = 0x1ba
                    0x01ba                  _OC5CON2bits = 0x1ba
                    0x01bc                  OC5RS = 0x1bc
                    0x01bc                  _OC5RS = 0x1bc
                    0x01be                  OC5R = 0x1be
                    0x01be                  _OC5R = 0x1be
                    0x01c0                  OC5TMR = 0x1c0
                    0x01c0                  _OC5TMR = 0x1c0
                    0x01c2                  OC6CON1 = 0x1c2
                    0x01c2                  _OC6CON1 = 0x1c2
                    0x01c2                  _OC6CON1bits = 0x1c2
                    0x01c4                  OC6CON2 = 0x1c4
                    0x01c4                  _OC6CON2 = 0x1c4
                    0x01c4                  _OC6CON2bits = 0x1c4
                    0x01c6                  OC6RS = 0x1c6
                    0x01c6                  _OC6RS = 0x1c6
                    0x01c8                  OC6R = 0x1c8
                    0x01c8                  _OC6R = 0x1c8
                    0x01ca                  OC6TMR = 0x1ca
                    0x01ca                  _OC6TMR = 0x1ca
                    0x01cc                  OC7CON1 = 0x1cc
                    0x01cc                  _OC7CON1 = 0x1cc
                    0x01cc                  _OC7CON1bits = 0x1cc
                    0x01ce                  OC7CON2 = 0x1ce
                    0x01ce                  _OC7CON2 = 0x1ce
                    0x01ce                  _OC7CON2bits = 0x1ce
                    0x01d0                  OC7RS = 0x1d0
                    0x01d0                  _OC7RS = 0x1d0
                    0x01d2                  OC7R = 0x1d2
                    0x01d2                  _OC7R = 0x1d2
                    0x01d4                  OC7TMR = 0x1d4
                    0x01d4                  _OC7TMR = 0x1d4
                    0x01d6                  OC8CON1 = 0x1d6
                    0x01d6                  _OC8CON1 = 0x1d6
                    0x01d6                  _OC8CON1bits = 0x1d6
                    0x01d8                  OC8CON2 = 0x1d8
                    0x01d8                  _OC8CON2 = 0x1d8
                    0x01d8                  _OC8CON2bits = 0x1d8
                    0x01da                  OC8RS = 0x1da
                    0x01da                  _OC8RS = 0x1da
                    0x01dc                  OC8R = 0x1dc
                    0x01dc                  _OC8R = 0x1dc
                    0x01de                  OC8TMR = 0x1de
                    0x01de                  _OC8TMR = 0x1de
                    0x01e0                  OC9CON1 = 0x1e0
                    0x01e0                  _OC9CON1 = 0x1e0
                    0x01e0                  _OC9CON1bits = 0x1e0
                    0x01e2                  OC9CON2 = 0x1e2
                    0x01e2                  _OC9CON2 = 0x1e2
                    0x01e2                  _OC9CON2bits = 0x1e2
                    0x01e4                  OC9RS = 0x1e4
                    0x01e4                  _OC9RS = 0x1e4
                    0x01e6                  OC9R = 0x1e6
                    0x01e6                  _OC9R = 0x1e6
                    0x01e8                  OC9TMR = 0x1e8
                    0x01e8                  _OC9TMR = 0x1e8
                    0x0200                  I2C1RCV = 0x200
                    0x0200                  _I2C1RCV = 0x200
                    0x0202                  I2C1TRN = 0x202
                    0x0202                  _I2C1TRN = 0x202
                    0x0204                  I2C1BRG = 0x204
                    0x0204                  _I2C1BRG = 0x204
                    0x0206                  I2C1CON = 0x206
                    0x0206                  _I2C1CON = 0x206
                    0x0206                  _I2C1CONbits = 0x206
                    0x0208                  I2C1STAT = 0x208
                    0x0208                  _I2C1STAT = 0x208
                    0x0208                  _I2C1STATbits = 0x208
                    0x020a                  I2C1ADD = 0x20a
                    0x020a                  _I2C1ADD = 0x20a
                    0x020c                  I2C1MSK = 0x20c
                    0x020c                  _I2C1MSK = 0x20c
                    0x0210                  I2C2RCV = 0x210
                    0x0210                  _I2C2RCV = 0x210
                    0x0212                  I2C2TRN = 0x212
                    0x0212                  _I2C2TRN = 0x212
                    0x0214                  I2C2BRG = 0x214
                    0x0214                  _I2C2BRG = 0x214
                    0x0216                  I2C2CON = 0x216
                    0x0216                  _I2C2CON = 0x216
                    0x0216                  _I2C2CONbits = 0x216
                    0x0218                  I2C2STAT = 0x218
                    0x0218                  _I2C2STAT = 0x218
                    0x0218                  _I2C2STATbits = 0x218
                    0x021a                  I2C2ADD = 0x21a
                    0x021a                  _I2C2ADD = 0x21a
                    0x021c                  I2C2MSK = 0x21c
                    0x021c                  _I2C2MSK = 0x21c
                    0x0220                  U1MODE = 0x220
                    0x0220                  _U1MODE = 0x220
                    0x0220                  _U1MODEbits = 0x220
                    0x0222                  U1STA = 0x222
                    0x0222                  _U1STA = 0x222
                    0x0222                  _U1STAbits = 0x222
                    0x0224                  U1TXREG = 0x224
                    0x0224                  _U1TXREG = 0x224
                    0x0226                  U1RXREG = 0x226
                    0x0226                  _U1RXREG = 0x226
                    0x0228                  U1BRG = 0x228
                    0x0228                  _U1BRG = 0x228
                    0x0230                  U2MODE = 0x230
                    0x0230                  _U2MODE = 0x230
                    0x0230                  _U2MODEbits = 0x230
                    0x0232                  U2STA = 0x232
                    0x0232                  _U2STA = 0x232
                    0x0232                  _U2STAbits = 0x232
                    0x0234                  U2TXREG = 0x234
                    0x0234                  _U2TXREG = 0x234
                    0x0236                  U2RXREG = 0x236
                    0x0236                  _U2RXREG = 0x236
                    0x0238                  U2BRG = 0x238
                    0x0238                  _U2BRG = 0x238
                    0x0240                  SPI1STAT = 0x240
                    0x0240                  _SPI1STAT = 0x240
                    0x0240                  _SPI1STATbits = 0x240
                    0x0242                  SPI1CON1 = 0x242
                    0x0242                  _SPI1CON1 = 0x242
                    0x0242                  _SPI1CON1bits = 0x242
                    0x0244                  SPI1CON2 = 0x244
                    0x0244                  _SPI1CON2 = 0x244
                    0x0244                  _SPI1CON2bits = 0x244
                    0x0248                  SPI1BUF = 0x248
                    0x0248                  _SPI1BUF = 0x248
                    0x0250                  U3MODE = 0x250
                    0x0250                  _U3MODE = 0x250
                    0x0250                  _U3MODEbits = 0x250
                    0x0252                  U3STA = 0x252
                    0x0252                  _U3STA = 0x252
                    0x0252                  _U3STAbits = 0x252
                    0x0254                  U3TXREG = 0x254
                    0x0254                  _U3TXREG = 0x254
                    0x0256                  U3RXREG = 0x256
                    0x0256                  _U3RXREG = 0x256
                    0x0258                  U3BRG = 0x258
                    0x0258                  _U3BRG = 0x258
                    0x0260                  SPI2STAT = 0x260
                    0x0260                  _SPI2STAT = 0x260
                    0x0260                  _SPI2STATbits = 0x260
                    0x0262                  SPI2CON1 = 0x262
                    0x0262                  _SPI2CON1 = 0x262
                    0x0262                  _SPI2CON1bits = 0x262
                    0x0264                  SPI2CON2 = 0x264
                    0x0264                  _SPI2CON2 = 0x264
                    0x0264                  _SPI2CON2bits = 0x264
                    0x0268                  SPI2BUF = 0x268
                    0x0268                  _SPI2BUF = 0x268
                    0x0270                  I2C3RCV = 0x270
                    0x0270                  _I2C3RCV = 0x270
                    0x0272                  I2C3TRN = 0x272
                    0x0272                  _I2C3TRN = 0x272
                    0x0274                  I2C3BRG = 0x274
                    0x0274                  _I2C3BRG = 0x274
                    0x0276                  I2C3CON = 0x276
                    0x0276                  _I2C3CON = 0x276
                    0x0276                  _I2C3CONbits = 0x276
                    0x0278                  I2C3STAT = 0x278
                    0x0278                  _I2C3STAT = 0x278
                    0x0278                  _I2C3STATbits = 0x278
                    0x027a                  I2C3ADD = 0x27a
                    0x027a                  _I2C3ADD = 0x27a
                    0x027c                  I2C3MSK = 0x27c
                    0x027c                  _I2C3MSK = 0x27c
                    0x0280                  SPI3STAT = 0x280
                    0x0280                  _SPI3STAT = 0x280
                    0x0280                  _SPI3STATbits = 0x280
                    0x0282                  SPI3CON1 = 0x282
                    0x0282                  _SPI3CON1 = 0x282
                    0x0282                  _SPI3CON1bits = 0x282
                    0x0284                  SPI3CON2 = 0x284
                    0x0284                  _SPI3CON2 = 0x284
                    0x0284                  _SPI3CON2bits = 0x284
                    0x0288                  SPI3BUF = 0x288
                    0x0288                  _SPI3BUF = 0x288
                    0x02b0                  U4MODE = 0x2b0
                    0x02b0                  _U4MODE = 0x2b0
                    0x02b0                  _U4MODEbits = 0x2b0
                    0x02b2                  U4STA = 0x2b2
                    0x02b2                  _U4STA = 0x2b2
                    0x02b2                  _U4STAbits = 0x2b2
                    0x02b4                  U4TXREG = 0x2b4
                    0x02b4                  _U4TXREG = 0x2b4
                    0x02b6                  U4RXREG = 0x2b6
                    0x02b6                  _U4RXREG = 0x2b6
                    0x02b8                  U4BRG = 0x2b8
                    0x02b8                  _U4BRG = 0x2b8
                    0x02c8                  TRISB = 0x2c8
                    0x02c8                  _TRISB = 0x2c8
                    0x02c8                  _TRISBbits = 0x2c8
                    0x02ca                  PORTB = 0x2ca
                    0x02ca                  _PORTB = 0x2ca
                    0x02ca                  _PORTBbits = 0x2ca
                    0x02cc                  LATB = 0x2cc
                    0x02cc                  _LATB = 0x2cc
                    0x02cc                  _LATBbits = 0x2cc
                    0x02ce                  ODCB = 0x2ce
                    0x02ce                  _ODCB = 0x2ce
                    0x02ce                  _ODCBbits = 0x2ce
                    0x02d0                  TRISC = 0x2d0
                    0x02d0                  _TRISC = 0x2d0
                    0x02d0                  _TRISCbits = 0x2d0
                    0x02d2                  PORTC = 0x2d2
                    0x02d2                  _PORTC = 0x2d2
                    0x02d2                  _PORTCbits = 0x2d2
                    0x02d4                  LATC = 0x2d4
                    0x02d4                  _LATC = 0x2d4
                    0x02d4                  _LATCbits = 0x2d4
                    0x02d6                  ODCC = 0x2d6
                    0x02d6                  _ODCC = 0x2d6
                    0x02d6                  _ODCCbits = 0x2d6
                    0x02d8                  TRISD = 0x2d8
                    0x02d8                  _TRISD = 0x2d8
                    0x02d8                  _TRISDbits = 0x2d8
                    0x02da                  PORTD = 0x2da
                    0x02da                  _PORTD = 0x2da
                    0x02da                  _PORTDbits = 0x2da
                    0x02dc                  LATD = 0x2dc
                    0x02dc                  _LATD = 0x2dc
                    0x02dc                  _LATDbits = 0x2dc
                    0x02de                  ODCD = 0x2de
                    0x02de                  _ODCD = 0x2de
                    0x02de                  _ODCDbits = 0x2de
                    0x02e0                  TRISE = 0x2e0
                    0x02e0                  _TRISE = 0x2e0
                    0x02e0                  _TRISEbits = 0x2e0
                    0x02e2                  PORTE = 0x2e2
                    0x02e2                  _PORTE = 0x2e2
                    0x02e2                  _PORTEbits = 0x2e2
                    0x02e4                  LATE = 0x2e4
                    0x02e4                  _LATE = 0x2e4
                    0x02e4                  _LATEbits = 0x2e4
                    0x02e6                  ODCE = 0x2e6
                    0x02e6                  _ODCE = 0x2e6
                    0x02e6                  _ODCEbits = 0x2e6
                    0x02e8                  TRISF = 0x2e8
                    0x02e8                  _TRISF = 0x2e8
                    0x02e8                  _TRISFbits = 0x2e8
                    0x02ea                  PORTF = 0x2ea
                    0x02ea                  _PORTF = 0x2ea
                    0x02ea                  _PORTFbits = 0x2ea
                    0x02ec                  LATF = 0x2ec
                    0x02ec                  _LATF = 0x2ec
                    0x02ec                  _LATFbits = 0x2ec
                    0x02ee                  ODCF = 0x2ee
                    0x02ee                  _ODCF = 0x2ee
                    0x02ee                  _ODCFbits = 0x2ee
                    0x02f0                  TRISG = 0x2f0
                    0x02f0                  _TRISG = 0x2f0
                    0x02f0                  _TRISGbits = 0x2f0
                    0x02f2                  PORTG = 0x2f2
                    0x02f2                  _PORTG = 0x2f2
                    0x02f2                  _PORTGbits = 0x2f2
                    0x02f4                  LATG = 0x2f4
                    0x02f4                  _LATG = 0x2f4
                    0x02f4                  _LATGbits = 0x2f4
                    0x02f6                  ODCG = 0x2f6
                    0x02f6                  _ODCG = 0x2f6
                    0x02f6                  _ODCGbits = 0x2f6
                    0x02fc                  PADCFG1 = 0x2fc
                    0x02fc                  _PADCFG1 = 0x2fc
                    0x02fc                  _PADCFG1bits = 0x2fc
                    0x0300                  ADC1BUF0 = 0x300
                    0x0300                  _ADC1BUF0 = 0x300
                    0x0302                  ADC1BUF1 = 0x302
                    0x0302                  _ADC1BUF1 = 0x302
                    0x0304                  ADC1BUF2 = 0x304
                    0x0304                  _ADC1BUF2 = 0x304
                    0x0306                  ADC1BUF3 = 0x306
                    0x0306                  _ADC1BUF3 = 0x306
                    0x0308                  ADC1BUF4 = 0x308
                    0x0308                  _ADC1BUF4 = 0x308
                    0x030a                  ADC1BUF5 = 0x30a
                    0x030a                  _ADC1BUF5 = 0x30a
                    0x030c                  ADC1BUF6 = 0x30c
                    0x030c                  _ADC1BUF6 = 0x30c
                    0x030e                  ADC1BUF7 = 0x30e
                    0x030e                  _ADC1BUF7 = 0x30e
                    0x0310                  ADC1BUF8 = 0x310
                    0x0310                  _ADC1BUF8 = 0x310
                    0x0312                  ADC1BUF9 = 0x312
                    0x0312                  _ADC1BUF9 = 0x312
                    0x0314                  ADC1BUFA = 0x314
                    0x0314                  _ADC1BUFA = 0x314
                    0x0316                  ADC1BUFB = 0x316
                    0x0316                  _ADC1BUFB = 0x316
                    0x0318                  ADC1BUFC = 0x318
                    0x0318                  _ADC1BUFC = 0x318
                    0x031a                  ADC1BUFD = 0x31a
                    0x031a                  _ADC1BUFD = 0x31a
                    0x031c                  ADC1BUFE = 0x31c
                    0x031c                  _ADC1BUFE = 0x31c
                    0x031e                  ADC1BUFF = 0x31e
                    0x031e                  _ADC1BUFF = 0x31e
                    0x0320                  AD1CON1 = 0x320
                    0x0320                  _AD1CON1 = 0x320
                    0x0320                  _AD1CON1bits = 0x320
                    0x0322                  AD1CON2 = 0x322
                    0x0322                  _AD1CON2 = 0x322
                    0x0322                  _AD1CON2bits = 0x322
                    0x0324                  AD1CON3 = 0x324
                    0x0324                  _AD1CON3 = 0x324
                    0x0324                  _AD1CON3bits = 0x324
                    0x0328                  AD1CHS = 0x328
                    0x0328                  _AD1CHS = 0x328
                    0x0328                  _AD1CHSbits = 0x328
                    0x0328                  AD1CHS0 = 0x328
                    0x0328                  _AD1CHS0 = 0x328
                    0x0328                  _AD1CHS0bits = 0x328
                    0x032a                  AD1PCFGH = 0x32a
                    0x032a                  _AD1PCFGH = 0x32a
                    0x032a                  _AD1PCFGHbits = 0x32a
                    0x032c                  AD1PCFG = 0x32c
                    0x032c                  _AD1PCFG = 0x32c
                    0x032c                  _AD1PCFGbits = 0x32c
                    0x032c                  AD1PCFGL = 0x32c
                    0x032c                  _AD1PCFGL = 0x32c
                    0x032c                  _AD1PCFGLbits = 0x32c
                    0x0330                  AD1CSSL = 0x330
                    0x0330                  _AD1CSSL = 0x330
                    0x0330                  _AD1CSSLbits = 0x330
                    0x0332                  AD1CSSH = 0x332
                    0x0332                  _AD1CSSH = 0x332
                    0x0332                  _AD1CSSHbits = 0x332
                    0x033c                  CTMUCON = 0x33c
                    0x033c                  _CTMUCON = 0x33c
                    0x033c                  _CTMUCONbits = 0x33c
                    0x033e                  CTMUICON = 0x33e
                    0x033e                  _CTMUICON = 0x33e
                    0x033e                  _CTMUICONbits = 0x33e
                    0x0480                  U1OTGIR = 0x480
                    0x0480                  _U1OTGIR = 0x480
                    0x0480                  _U1OTGIRbits = 0x480
                    0x0482                  U1OTGIE = 0x482
                    0x0482                  _U1OTGIE = 0x482
                    0x0482                  _U1OTGIEbits = 0x482
                    0x0484                  U1OTGSTAT = 0x484
                    0x0484                  _U1OTGSTAT = 0x484
                    0x0484                  _U1OTGSTATbits = 0x484
                    0x0486                  U1OTGCON = 0x486
                    0x0486                  _U1OTGCON = 0x486
                    0x0486                  _U1OTGCONbits = 0x486
                    0x0488                  U1PWRC = 0x488
                    0x0488                  _U1PWRC = 0x488
                    0x0488                  _U1PWRCbits = 0x488
                    0x048a                  U1IR = 0x48a
                    0x048a                  _U1IR = 0x48a
                    0x048a                  _U1IRbits = 0x48a
                    0x048c                  U1IE = 0x48c
                    0x048c                  _U1IE = 0x48c
                    0x048c                  _U1IEbits = 0x48c
                    0x048e                  U1EIR = 0x48e
                    0x048e                  _U1EIR = 0x48e
                    0x048e                  _U1EIRbits = 0x48e
                    0x0490                  U1EIE = 0x490
                    0x0490                  _U1EIE = 0x490
                    0x0490                  _U1EIEbits = 0x490
                    0x0492                  U1STAT = 0x492
                    0x0492                  _U1STAT = 0x492
                    0x0492                  _U1STATbits = 0x492
                    0x0494                  U1CON = 0x494
                    0x0494                  _U1CON = 0x494
                    0x0494                  _U1CONbits = 0x494
                    0x0496                  U1ADDR = 0x496
                    0x0496                  _U1ADDR = 0x496
                    0x0496                  _U1ADDRbits = 0x496
                    0x0498                  U1BDTP1 = 0x498
                    0x0498                  _U1BDTP1 = 0x498
                    0x0498                  _U1BDTP1bits = 0x498
                    0x049a                  U1FRML = 0x49a
                    0x049a                  _U1FRML = 0x49a
                    0x049a                  _U1FRMLbits = 0x49a
                    0x049c                  U1FRMH = 0x49c
                    0x049c                  _U1FRMH = 0x49c
                    0x049c                  _U1FRMHbits = 0x49c
                    0x049e                  U1TOK = 0x49e
                    0x049e                  _U1TOK = 0x49e
                    0x049e                  _U1TOKbits = 0x49e
                    0x04a0                  U1SOF = 0x4a0
                    0x04a0                  _U1SOF = 0x4a0
                    0x04a0                  _U1SOFbits = 0x4a0
                    0x04a2                  U1BDTP2 = 0x4a2
                    0x04a2                  _U1BDTP2 = 0x4a2
                    0x04a2                  _U1BDTP2bits = 0x4a2
                    0x04a4                  U1BDTP3 = 0x4a4
                    0x04a4                  _U1BDTP3 = 0x4a4
                    0x04a4                  _U1BDTP3bits = 0x4a4
                    0x04a6                  U1CNFG1 = 0x4a6
                    0x04a6                  _U1CNFG1 = 0x4a6
                    0x04a6                  _U1CNFG1bits = 0x4a6
                    0x04a8                  U1CNFG2 = 0x4a8
                    0x04a8                  _U1CNFG2 = 0x4a8
                    0x04a8                  _U1CNFG2bits = 0x4a8
                    0x04aa                  U1EP0 = 0x4aa
                    0x04aa                  _U1EP0 = 0x4aa
                    0x04aa                  _U1EP0bits = 0x4aa
                    0x04ac                  U1EP1 = 0x4ac
                    0x04ac                  _U1EP1 = 0x4ac
                    0x04ac                  _U1EP1bits = 0x4ac
                    0x04ae                  U1EP2 = 0x4ae
                    0x04ae                  _U1EP2 = 0x4ae
                    0x04ae                  _U1EP2bits = 0x4ae
                    0x04b0                  U1EP3 = 0x4b0
                    0x04b0                  _U1EP3 = 0x4b0
                    0x04b0                  _U1EP3bits = 0x4b0
                    0x04b2                  U1EP4 = 0x4b2
                    0x04b2                  _U1EP4 = 0x4b2
                    0x04b2                  _U1EP4bits = 0x4b2
                    0x04b4                  U1EP5 = 0x4b4
                    0x04b4                  _U1EP5 = 0x4b4
                    0x04b4                  _U1EP5bits = 0x4b4
                    0x04b6                  U1EP6 = 0x4b6
                    0x04b6                  _U1EP6 = 0x4b6
                    0x04b6                  _U1EP6bits = 0x4b6
                    0x04b8                  U1EP7 = 0x4b8
                    0x04b8                  _U1EP7 = 0x4b8
                    0x04b8                  _U1EP7bits = 0x4b8
                    0x04ba                  U1EP8 = 0x4ba
                    0x04ba                  _U1EP8 = 0x4ba
                    0x04ba                  _U1EP8bits = 0x4ba
                    0x04bc                  U1EP9 = 0x4bc
                    0x04bc                  _U1EP9 = 0x4bc
                    0x04bc                  _U1EP9bits = 0x4bc
                    0x04be                  U1EP10 = 0x4be
                    0x04be                  _U1EP10 = 0x4be
                    0x04be                  _U1EP10bits = 0x4be
                    0x04c0                  U1EP11 = 0x4c0
                    0x04c0                  _U1EP11 = 0x4c0
                    0x04c0                  _U1EP11bits = 0x4c0
                    0x04c2                  U1EP12 = 0x4c2
                    0x04c2                  _U1EP12 = 0x4c2
                    0x04c2                  _U1EP12bits = 0x4c2
                    0x04c4                  U1EP13 = 0x4c4
                    0x04c4                  _U1EP13 = 0x4c4
                    0x04c4                  _U1EP13bits = 0x4c4
                    0x04c6                  U1EP14 = 0x4c6
                    0x04c6                  _U1EP14 = 0x4c6
                    0x04c6                  _U1EP14bits = 0x4c6
                    0x04c8                  U1EP15 = 0x4c8
                    0x04c8                  _U1EP15 = 0x4c8
                    0x04c8                  _U1EP15bits = 0x4c8
                    0x04cc                  U1PWMRRS = 0x4cc
                    0x04cc                  _U1PWMRRS = 0x4cc
                    0x04cc                  _U1PWMRRSbits = 0x4cc
                    0x04ce                  U1PWMCON = 0x4ce
                    0x04ce                  _U1PWMCON = 0x4ce
                    0x04ce                  _U1PWMCONbits = 0x4ce
                    0x0600                  PMCON = 0x600
                    0x0600                  _PMCON = 0x600
                    0x0600                  _PMCONbits = 0x600
                    0x0602                  PMMODE = 0x602
                    0x0602                  _PMMODE = 0x602
                    0x0602                  _PMMODEbits = 0x602
                    0x0604                  PMADDR = 0x604
                    0x0604                  _PMADDR = 0x604
                    0x0604                  _PMADDRbits = 0x604
                    0x0604                  PMDOUT1 = 0x604
                    0x0604                  _PMDOUT1 = 0x604
                    0x0604                  _PMDOUT1bits = 0x604
                    0x0606                  PMDOUT2 = 0x606
                    0x0606                  _PMDOUT2 = 0x606
                    0x0608                  PMDIN1 = 0x608
                    0x0608                  _PMDIN1 = 0x608
                    0x060a                  PMDIN2 = 0x60a
                    0x060a                  _PMDIN2 = 0x60a
                    0x060c                  PMAEN = 0x60c
                    0x060c                  _PMAEN = 0x60c
                    0x060c                  _PMAENbits = 0x60c
                    0x060e                  PMSTAT = 0x60e
                    0x060e                  _PMSTAT = 0x60e
                    0x060e                  _PMSTATbits = 0x60e
                    0x0620                  ALRMVAL = 0x620
                    0x0620                  _ALRMVAL = 0x620
                    0x0622                  ALCFGRPT = 0x622
                    0x0622                  _ALCFGRPT = 0x622
                    0x0622                  _ALCFGRPTbits = 0x622
                    0x0624                  RTCVAL = 0x624
                    0x0624                  _RTCVAL = 0x624
                    0x0626                  RCFGCAL = 0x626
                    0x0626                  _RCFGCAL = 0x626
                    0x0626                  _RCFGCALbits = 0x626
                    0x0630                  CMSTAT = 0x630
                    0x0630                  _CMSTAT = 0x630
                    0x0630                  _CMSTATbits = 0x630
                    0x0632                  CVRCON = 0x632
                    0x0632                  _CVRCON = 0x632
                    0x0632                  _CVRCONbits = 0x632
                    0x0634                  CM1CON = 0x634
                    0x0634                  _CM1CON = 0x634
                    0x0634                  _CM1CONbits = 0x634
                    0x0636                  CM2CON = 0x636
                    0x0636                  _CM2CON = 0x636
                    0x0636                  _CM2CONbits = 0x636
                    0x0638                  CM3CON = 0x638
                    0x0638                  _CM3CON = 0x638
                    0x0638                  _CM3CONbits = 0x638
                    0x0640                  CRCCON = 0x640
                    0x0640                  _CRCCON = 0x640
                    0x0640                  _CRCCONbits = 0x640
                    0x0642                  CRCXOR = 0x642
                    0x0642                  _CRCXOR = 0x642
                    0x0642                  _CRCXORbits = 0x642
                    0x0644                  CRCDAT = 0x644
                    0x0644                  _CRCDAT = 0x644
                    0x0646                  CRCWDAT = 0x646
                    0x0646                  _CRCWDAT = 0x646
                    0x0680                  RPINR0 = 0x680
                    0x0680                  _RPINR0 = 0x680
                    0x0680                  _RPINR0bits = 0x680
                    0x0682                  RPINR1 = 0x682
                    0x0682                  _RPINR1 = 0x682
                    0x0682                  _RPINR1bits = 0x682
                    0x0684                  RPINR2 = 0x684
                    0x0684                  _RPINR2 = 0x684
                    0x0684                  _RPINR2bits = 0x684
                    0x0686                  RPINR3 = 0x686
                    0x0686                  _RPINR3 = 0x686
                    0x0686                  _RPINR3bits = 0x686
                    0x0688                  RPINR4 = 0x688
                    0x0688                  _RPINR4 = 0x688
                    0x0688                  _RPINR4bits = 0x688
                    0x068e                  RPINR7 = 0x68e
                    0x068e                  _RPINR7 = 0x68e
                    0x068e                  _RPINR7bits = 0x68e
                    0x0690                  RPINR8 = 0x690
                    0x0690                  _RPINR8 = 0x690
                    0x0690                  _RPINR8bits = 0x690
                    0x0692                  RPINR9 = 0x692
                    0x0692                  _RPINR9 = 0x692
                    0x0692                  _RPINR9bits = 0x692
                    0x0694                  RPINR10 = 0x694
                    0x0694                  _RPINR10 = 0x694
                    0x0694                  _RPINR10bits = 0x694
                    0x0696                  RPINR11 = 0x696
                    0x0696                  _RPINR11 = 0x696
                    0x0696                  _RPINR11bits = 0x696
                    0x069e                  RPINR15 = 0x69e
                    0x069e                  _RPINR15 = 0x69e
                    0x069e                  _RPINR15bits = 0x69e
                    0x06a2                  RPINR17 = 0x6a2
                    0x06a2                  _RPINR17 = 0x6a2
                    0x06a2                  _RPINR17bits = 0x6a2
                    0x06a4                  RPINR18 = 0x6a4
                    0x06a4                  _RPINR18 = 0x6a4
                    0x06a4                  _RPINR18bits = 0x6a4
                    0x06a6                  RPINR19 = 0x6a6
                    0x06a6                  _RPINR19 = 0x6a6
                    0x06a6                  _RPINR19bits = 0x6a6
                    0x06a8                  RPINR20 = 0x6a8
                    0x06a8                  _RPINR20 = 0x6a8
                    0x06a8                  _RPINR20bits = 0x6a8
                    0x06aa                  RPINR21 = 0x6aa
                    0x06aa                  _RPINR21 = 0x6aa
                    0x06aa                  _RPINR21bits = 0x6aa
                    0x06ac                  RPINR22 = 0x6ac
                    0x06ac                  _RPINR22 = 0x6ac
                    0x06ac                  _RPINR22bits = 0x6ac
                    0x06ae                  RPINR23 = 0x6ae
                    0x06ae                  _RPINR23 = 0x6ae
                    0x06ae                  _RPINR23bits = 0x6ae
                    0x06b6                  RPINR27 = 0x6b6
                    0x06b6                  _RPINR27 = 0x6b6
                    0x06b6                  _RPINR27bits = 0x6b6
                    0x06b8                  RPINR28 = 0x6b8
                    0x06b8                  _RPINR28 = 0x6b8
                    0x06b8                  _RPINR28bits = 0x6b8
                    0x06ba                  RPINR29 = 0x6ba
                    0x06ba                  _RPINR29 = 0x6ba
                    0x06ba                  _RPINR29bits = 0x6ba
                    0x06c0                  RPOR0 = 0x6c0
                    0x06c0                  _RPOR0 = 0x6c0
                    0x06c0                  _RPOR0bits = 0x6c0
                    0x06c2                  RPOR1 = 0x6c2
                    0x06c2                  _RPOR1 = 0x6c2
                    0x06c2                  _RPOR1bits = 0x6c2
                    0x06c4                  RPOR2 = 0x6c4
                    0x06c4                  _RPOR2 = 0x6c4
                    0x06c4                  _RPOR2bits = 0x6c4
                    0x06c6                  RPOR3 = 0x6c6
                    0x06c6                  _RPOR3 = 0x6c6
                    0x06c6                  _RPOR3bits = 0x6c6
                    0x06c8                  RPOR4 = 0x6c8
                    0x06c8                  _RPOR4 = 0x6c8
                    0x06c8                  _RPOR4bits = 0x6c8
                    0x06ca                  RPOR5 = 0x6ca
                    0x06ca                  _RPOR5 = 0x6ca
                    0x06ca                  _RPOR5bits = 0x6ca
                    0x06cc                  RPOR6 = 0x6cc
                    0x06cc                  _RPOR6 = 0x6cc
                    0x06cc                  _RPOR6bits = 0x6cc
                    0x06ce                  RPOR7 = 0x6ce
                    0x06ce                  _RPOR7 = 0x6ce
                    0x06ce                  _RPOR7bits = 0x6ce
                    0x06d0                  RPOR8 = 0x6d0
                    0x06d0                  _RPOR8 = 0x6d0
                    0x06d0                  _RPOR8bits = 0x6d0
                    0x06d2                  RPOR9 = 0x6d2
                    0x06d2                  _RPOR9 = 0x6d2
                    0x06d2                  _RPOR9bits = 0x6d2
                    0x06d4                  RPOR10 = 0x6d4
                    0x06d4                  _RPOR10 = 0x6d4
                    0x06d4                  _RPOR10bits = 0x6d4
                    0x06d6                  RPOR11 = 0x6d6
                    0x06d6                  _RPOR11 = 0x6d6
                    0x06d6                  _RPOR11bits = 0x6d6
                    0x06d8                  RPOR12 = 0x6d8
                    0x06d8                  _RPOR12 = 0x6d8
                    0x06d8                  _RPOR12bits = 0x6d8
                    0x06da                  RPOR13 = 0x6da
                    0x06da                  _RPOR13 = 0x6da
                    0x06da                  _RPOR13bits = 0x6da
                    0x06dc                  RPOR14 = 0x6dc
                    0x06dc                  _RPOR14 = 0x6dc
                    0x06dc                  _RPOR14bits = 0x6dc
                    0x06de                  RPOR15 = 0x6de
                    0x06de                  _RPOR15 = 0x6de
                    0x06de                  _RPOR15bits = 0x6de
                    0x0740                  RCON = 0x740
                    0x0740                  _RCON = 0x740
                    0x0740                  _RCONbits = 0x740
                    0x0742                  OSCCON = 0x742
                    0x0742                  _OSCCON = 0x742
                    0x0742                  _OSCCONbits = 0x742
                    0x0742                  OSCCONL = 0x742
                    0x0742                  _OSCCONL = 0x742
                    0x0743                  OSCCONH = 0x743
                    0x0743                  _OSCCONH = 0x743
                    0x0744                  CLKDIV = 0x744
                    0x0744                  _CLKDIV = 0x744
                    0x0744                  _CLKDIVbits = 0x744
                    0x0748                  OSCTUN = 0x748
                    0x0748                  _OSCTUN = 0x748
                    0x0748                  _OSCTUNbits = 0x748
                    0x074e                  REFOCON = 0x74e
                    0x074e                  _REFOCON = 0x74e
                    0x074e                  _REFOCONbits = 0x74e
                    0x0760                  NVMCON = 0x760
                    0x0760                  _NVMCON = 0x760
                    0x0760                  _NVMCONbits = 0x760
                    0x0766                  NVMKEY = 0x766
                    0x0766                  _NVMKEY = 0x766
                    0x0770                  PMD1 = 0x770
                    0x0770                  _PMD1 = 0x770
                    0x0770                  _PMD1bits = 0x770
                    0x0772                  PMD2 = 0x772
                    0x0772                  _PMD2 = 0x772
                    0x0772                  _PMD2bits = 0x772
                    0x0774                  PMD3 = 0x774
                    0x0774                  _PMD3 = 0x774
                    0x0774                  _PMD3bits = 0x774
                    0x0776                  PMD4 = 0x776
                    0x0776                  _PMD4 = 0x776
                    0x0776                  _PMD4bits = 0x776
                    0x0778                  PMD5 = 0x778
                    0x0778                  _PMD5 = 0x778
                    0x0778                  _PMD5bits = 0x778
                    0x077a                  PMD6 = 0x77a
                    0x077a                  _PMD6 = 0x77a
                    0x077a                  _PMD6bits = 0x77a
                    0x0144                  IC1 = 0x144
                    0x0144                  _IC1 = 0x144
                    0x014c                  IC2 = 0x14c
                    0x014c                  _IC2 = 0x14c
                    0x0154                  IC3 = 0x154
                    0x0154                  _IC3 = 0x154
                    0x015c                  IC4 = 0x15c
                    0x015c                  _IC4 = 0x15c
                    0x0164                  IC5 = 0x164
                    0x0164                  _IC5 = 0x164
                    0x016c                  IC6 = 0x16c
                    0x016c                  _IC6 = 0x16c
                    0x0174                  IC7 = 0x174
                    0x0174                  _IC7 = 0x174
                    0x017c                  IC8 = 0x17c
                    0x017c                  _IC8 = 0x17c
                    0x0194                  OC1 = 0x194
                    0x0194                  _OC1 = 0x194
                    0x019e                  OC2 = 0x19e
                    0x019e                  _OC2 = 0x19e
                    0x01a8                  OC3 = 0x1a8
                    0x01a8                  _OC3 = 0x1a8
                    0x01b2                  OC4 = 0x1b2
                    0x01b2                  _OC4 = 0x1b2
                    0x01bc                  OC5 = 0x1bc
                    0x01bc                  _OC5 = 0x1bc
                    0x01c6                  OC6 = 0x1c6
                    0x01c6                  _OC6 = 0x1c6
                    0x01d0                  OC7 = 0x1d0
                    0x01d0                  _OC7 = 0x1d0
                    0x01da                  OC8 = 0x1da
                    0x01da                  _OC8 = 0x1da
                    0x0240                  SPI1 = 0x240
                    0x0240                  _SPI1 = 0x240
                    0x0260                  SPI2 = 0x260
                    0x0260                  _SPI2 = 0x260
                    0x0220                  UART1 = 0x220
                    0x0220                  _UART1 = 0x220
                    0x0230                  UART2 = 0x230
                    0x0230                  _UART2 = 0x230
                    0x0001                  __MPLAB_BUILD = 0x1
START GROUP
LOAD c:/program files/microchip/mplab c30/bin/bin/../../lib\libpic30-coff.a
LOAD c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a
LOAD c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a
END GROUP
OUTPUT(PIC24F Starter Kit.cof coff-pic30)
LOAD jump_table
LOAD data_init

.nbss               0x0800        0x8ec
 .nbss              0x0800        0x496 Objects - PIC24F Starter Kit\Demos.o
                    0x0802                  captureFile
                    0x0804                  graphData
                    0x0882                  graphDataHead
                    0x0884                  graphDataTail
                    0x0886                  graphOffset
                    0x0888                  graphUpdateRate
                    0x088a                  logBufferReading
                    0x088b                  logBufferWriting
                    0x088c                  logData
                    0x0c94                  potADC
 .nbss              0x0c96        0x456 Objects - PIC24F Starter Kit\Games.o
                    0x0c98                  gamesGrid
                    0x0c9a                  pScore
                    0x0c9c                  score
                    0x0c9e                  scoreText
                    0x0cb2                  scoreInfo
                    0x0ccc                  asteroid
                    0x0d0e                  bullet
                    0x0d1c                  pShip
                    0x0d1e                  balls
                    0x0d2a                  ballsRemoved
                    0x0d2c                  columnsRemoved
                    0x0d2e                  lastSelectedColumn
                    0x0d30                  lastSelectedRow
                    0x0d32                  lastBall
                    0x0d34                  lastBallCount
                    0x0d36                  selectionMarked
                    0x0d38                  defaultDirection
                    0x0d3a                  field
                    0x0e8a                  snake

_02b7193048f67891
                    0x10ec        0x200
 _02b7193048f67891
                    0x10ec        0x200 ..\Microchip\MDD File System\Objects - PIC24F Starter Kit\FSIO.o
                    0x10ec                  gDataBuffer

_02b71a8048f67891
                    0x12ec        0x200
 _02b71a8048f67891
                    0x12ec        0x200 ..\Microchip\MDD File System\Objects - PIC24F Starter Kit\FSIO.o
                    0x12ec                  gFATBuffer

.nbss               0x14ec        0x24e
 .nbss              0x14ec        0x164 ..\Microchip\MDD File System\Objects - PIC24F Starter Kit\FSIO.o
                    0x14ec                  gFileArray
                    0x1558                  gFileSlotOpen
                    0x155a                  gTimeCrtMS
                    0x155c                  gTimeCrtTime
                    0x155e                  gTimeCrtDate
                    0x1560                  gTimeAccDate
                    0x1562                  gTimeWrtTime
                    0x1564                  gTimeWrtDate
                    0x1566                  FatRootDirClusterValue
                    0x156a                  BytesPerSec
                    0x156c                  FAT32_BkBootSector
                    0x156e                  FAT32_FSInfo
                    0x1570                  TempClusterCalc
                    0x1574                  Index
                    0x1575                  dirCleared
                    0x1576                  dotdot
                    0x157a                  tempCWDobj
                    0x15b0                  gFileTemp
                    0x15e6                  cwd
                    0x161c                  gDiskData
                    0x163a                  defaultString
                    0x1645                  defaultArray
 .nbss              0x1650         0xa8 Objects - PIC24F Starter Kit\PIC24F Starter Kit.o
                    0x1654                  pageInformation
                    0x16f0                  displayChangeTime
                    0x16f4                  previousSecond
                    0x16f6                  pScheme
 .nbss              0x16f8         0x42 ..\Microchip\Graphics\Objects - PIC24F Starter Kit\Primitive.o
                    0x1728                  _lineType
                    0x172a                  _lineThickness
                    0x172c                  _cursorX
                    0x172e                  _cursorY
                    0x1730                  _fontOrientation
                    0x1732                  _font
                    0x1734                  _fontFirstChar
                    0x1736                  _fontLastChar
                    0x1738                  _fontHeight

_0207177048f678a6
                    0x173a         0x3a
 _0207177048f678a6
                    0x173a         0x3a ..\Microchip\Usb\MSD Host Driver\Objects - PIC24F Starter Kit\usb_host_msd.o
                    0x173a                  deviceInfoMSD

.nbss               0x1774         0x6a
 .nbss              0x1774         0x36 Objects - PIC24F Starter Kit\TouchSense.o
                    0x1774                  buttons
                    0x1776                  rawCTMU
                    0x1780                  average
                    0x178a                  trip
                    0x1794                  hyst
                    0x179e                  first
                    0x179f                  buttonIndex
                    0x17a0                  value
                    0x17a2                  bigVal
                    0x17a4                  smallAvg
                    0x17a6                  AvgIndex
                    0x17a8                  buttonsPrevious
 .nbss              0x17aa         0x34 Objects - PIC24F Starter Kit\Utilities.o
                    0x17aa                  calibrationState
                    0x17ac                  countCTMU
                    0x17ae                  currentTouchpad
                    0x17b0                  stateTick
                    0x17b4                  sumCTMUPressed
                    0x17c8                  sumCTMUReleased
                    0x17dc                  currentControlSet

.ndata              0x17de         0x30
 .ndata             0x17de         0x30 Objects - PIC24F Starter Kit\Utilities.o
                    0x17de                  daysPerMonth
                    0x17ea                  monthNames

.nbss               0x180e         0x4c
 .nbss              0x180e         0x2a Objects - PIC24F Starter Kit\Flash.o
                    0x180e                  mediaPresent
                    0x1810                  pFlashFiles
                    0x1812                  pSlider
                    0x1814                  usbErrorCode
                    0x1815                  usbErrorText
                    0x182a                  volume
 .nbss              0x1838         0x22 ..\Microchip\Usb\Objects - PIC24F Starter Kit\usb_host.o
                    0x1838                  countConfigurations
                    0x1839                  numCommandTries
                    0x183a                  numEnumerationTries
                    0x183c                  numTimerInterrupts
                    0x183e                  pCurrentEndpoint
                    0x1840                  usbBusInfo
                    0x1848                  usbDeviceInfo
                    0x1854                  usbHostState
                    0x1856                  usbOverrideHostState
                    0x1858                  usbRootHubInfo

.ndata              0x185a         0x1e
 .ndata             0x185a         0x1e Objects - PIC24F Starter Kit\Games.o
                    0x185a                  scoreSize
                    0x1860                  scoreSpeed
                    0x1866                  scoreTable

.nbss               0x1878         0x2c
 .nbss              0x1878         0x18 ..\Microchip\Graphics\Objects - PIC24F Starter Kit\GOL.o
                    0x187e                  _rpnlX1
                    0x1880                  _rpnlY1
                    0x1882                  _rpnlX2
                    0x1884                  _rpnlY2
                    0x1886                  _rpnlR
                    0x1888                  _rpnlFaceColor
                    0x188a                  _rpnlEmbossLtColor
                    0x188c                  _rpnlEmbossDkColor
                    0x188e                  _rpnlEmbossSize
 .nbss              0x1890         0x14 ..\Microchip\Graphics\Objects - PIC24F Starter Kit\Slider.o

.ndata              0x18a4         0x12
 .ndata             0x18a4         0x12 ..\Microchip\MDD File System\Objects - PIC24F Starter Kit\FSIO.o
                    0x18a4                  gLastFATSectorRead
                    0x18a8                  gNeedFATWrite
                    0x18aa                  gBufferOwner
                    0x18ac                  gLastDataSectorRead
                    0x18b0                  gNeedDataWrite
                    0x18b1                  nextClusterIsLast
                    0x18b2                  gBufferZeroed
                    0x18b3                  recache
                    0x18b4                  cwdptr

_02cdbaf048f67890
                    0x1a00         0x10
 _02cdbaf048f67890
                    0x1a00         0x10 ..\Microchip\Usb\Objects - PIC24F Starter Kit\usb_host.o
                    0x1a00                  BDT

.ndata              0x18b6         0x38
 .ndata             0x18b6         0x20 Objects - PIC24F Starter Kit\rtcc.o
                    0x18b6                  _time_str
                    0x18c6                  _date_str
 .ndata             0x18d6         0x18 Objects - PIC24F Starter Kit\usb_config.o
                    0x18d6                  usbMediaInterfaceTable
                    0x18de                  usbClientDrvTable
                    0x18e6                  usbTPL

.nbss               0x18ee         0x12
 .nbss              0x18ee         0x12 Objects - PIC24F Starter Kit\rtcc.o
                    0x18ee                  _time
                    0x18f6                  _time_chk
                    0x18fe                  _rtcc_flag

.ndata              0x1900         0x18
 .ndata             0x1900          0xc ..\Microchip\Usb\Objects - PIC24F Starter Kit\usb_host.o
                    0x1900                  pConfigurationDescriptorList
                    0x1902                  pCurrentConfigurationDescriptor
                    0x1904                  pDeviceDescriptor
                    0x1906                  pEndpointList
                    0x1908                  pEP0Data
                    0x190a                  pInterfaceList
 .ndata             0x190c          0xc ..\Microchip\Graphics\Objects - PIC24F Starter Kit\RoundDial.o
                    0x190c                  _cosine

.nbss               0x1918          0xc
 .nbss              0x1918          0xc ..\Microchip\Graphics\Objects - PIC24F Starter Kit\SH1101A.o
                    0x1918                  _color
                    0x191a                  _clipRgn
                    0x191c                  _clipLeft
                    0x191e                  _clipTop
                    0x1920                  _clipRight
                    0x1922                  _clipBottom

.ndata              0x1924          0xa
 .ndata             0x1924          0xa Objects - PIC24F Starter Kit\PIC24F Starter Kit.o
                    0x1924                  previousTick
                    0x1928                  screenState
                    0x192a                  tick

.nbss               0x192e         0x12
 .nbss              0x192e          0xa ..\Microchip\Graphics\Objects - PIC24F Starter Kit\Picture.o
 .nbss              0x1938          0x8 ..\Microchip\Graphics\Objects - PIC24F Starter Kit\StaticText.o

.ndata              0x1940          0x8
 .ndata             0x1940          0x8 ..\Microchip\Graphics\Objects - PIC24F Starter Kit\GOL.o
                    0x1940                  _pGolObjects
                    0x1942                  _pDefaultGolScheme
                    0x1944                  _pObjectFocused
                    0x1946                  _pRpnlBitmap

.nbss               0x1948         0x12
 .nbss              0x1948          0x8 ..\Microchip\Graphics\Objects - PIC24F Starter Kit\Button.o
 .nbss              0x1950          0x6 ..\Microchip\Graphics\Objects - PIC24F Starter Kit\ListBox.o
 .nbss              0x1956          0x4 ..\Microchip\Graphics\Objects - PIC24F Starter Kit\RoundDial.o

.ndata              0x195a          0x6
 .ndata             0x195a          0x4 ..\Microchip\Usb\MSD Host Driver\Objects - PIC24F Starter Kit\usb_host_msd.o
                    0x195a                  dCBWTagNext
 .ndata             0x195e          0x2 ..\Microchip\Graphics\Objects - PIC24F Starter Kit\Primitive.o

.nbss               0x1960          0x2
 .nbss              0x1960          0x2 ..\Microchip\Graphics\Objects - PIC24F Starter Kit\EditBox.o

.ndata              0x1962          0x2
 .ndata             0x1962          0x2 ..\Microchip\Usb\MSD Host Driver\Objects - PIC24F Starter Kit\usb_host_msd_scsi.o
                    0x1962                  deviceAddress
                    0x1963                  maxLUN

.nbss               0x1964          0x2
 .nbss              0x1964          0x2 c:/program files/microchip/mplab c30/bin/bin/../../lib\libpic30-coff.a(brk.o)
                    0x1964                  __curbrk

.bss                0x1966         0x88
 .bss               0x1966         0x88 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(rand.o)

.data               0x1a10         0x22
 .data              0x1a10         0x22 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xlitob.o)

.data               0x19ee         0x12
 .data              0x19ee         0x12 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xprintf.io)

.data               0x1a32          0xa
 .data              0x1a32          0xa c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(rand.o)
                    0x1a32                  _Tls_setup__Randseed
                    0x1a34                  _Randseed
                    0x1a38                  _Tls_setup__Randinit
                    0x1a3a                  _Randinit

.dconst             0x1a3c          0x8
 .dconst            0x1a3c          0x8 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xprintf.io)

.data               0x1a44          0x6
 .data              0x1a44          0x6 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(malloc.o)
                    0x1a44                  _Size_block
                    0x1a46                  _Aldata

.const              0x8fea        0xc0a load address 0x000fea  
 .const             0x8fea        0x768 Objects - PIC24F Starter Kit\Gentium8.o
                    0x8fea                  GOLFontDefault
                    0x8fee                  L13579
 .const             0x9752        0x1ac Objects - PIC24F Starter Kit\Flash.o
 .const             0x98fe         0xd8 Objects - PIC24F Starter Kit\Games.o
 .const             0x99d6         0xb0 Objects - PIC24F Starter Kit\Utilities.o
 .const             0x9a86         0x9a Objects - PIC24F Starter Kit\Demos.o
                    0x9a86                  mediaRequest
 .const             0x9b20         0x52 Objects - PIC24F Starter Kit\PIC24F Starter Kit.o
 .const             0x9b72         0x48 Objects - PIC24F Starter Kit\Pictures.o
                    0x9b72                  ballCircle
                    0x9b78                  ballCross
                    0x9b7e                  ballMarking
                    0x9b84                  ballSquare
                    0x9b8a                  ballTriangle
                    0x9b90                  iconFolderSmall
                    0x9b96                  iconMicrochip
                    0x9b9c                  intro
                    0x9ba2                  introDevice
                    0x9ba8                  snakeBody
                    0x9bae                  snakeFood
                    0x9bb4                  snakeHead
 .const             0x9bba         0x18 Objects - PIC24F Starter Kit\rtcc.o
 .const             0x9bd2         0x12 ..\Microchip\Graphics\Objects - PIC24F Starter Kit\SH1101A.o
 .const             0x9be4         0x10 ..\Microchip\MDD File System\Objects - PIC24F Starter Kit\FSIO.o

.text             0x001bf4      0x132aa
 .text            0x001bf4       0x5044 ..\Microchip\MDD File System\Objects - PIC24F Starter Kit\FSIO.o
                  0x001bf4                  FSInit
                  0x001c8c                  FILEfind
                  0x001e76                  FILEopen
                  0x001f9c                  FILEget_next_cluster
                  0x002074                  DISKmount
                  0x0020b6                  LoadMBR
                  0x002258                  LoadBootSector
                  0x002460                  FSformat
                  0x002b2c                  Write_File_Entry
                  0x002bce                  FAT_erase_cluster_chain
                  0x002ce0                  Cache_File_Entry
                  0x002ec2                  CreateFileEntry
                  0x002f2c                  CreateFirstCluster
                  0x002fb8                  FindEmptyEntries
                  0x0030cc                  PopulateEntries
                  0x0031b4                  CacheTime
                  0x00330a                  FILEallocate_new_cluster
                  0x0033b2                  FATfindEmptyCluster
                  0x0034b0                  FSfclose
                  0x00357a                  Fill_File_Object
                  0x0036d4                  LoadDirAttrib
                  0x00375a                  FILEerase
                  0x003816                  FSrename
                  0x003cce                  FSfopen
                  0x003f0c                  FSftell
                  0x003f1a                  FSremove
                  0x003fbc                  FSrewind
                  0x003ff0                  FileObjectCopy
                  0x004030                  FILECreateHeadCluster
                  0x0040dc                  EraseCluster
                  0x004168                  Cluster2Sector
                  0x004210                  FSfwrite
                  0x004488                  flushData
                  0x0044e2                  FSfeof
                  0x004506                  FSfread
                  0x0046b2                  FormatFileName
                  0x0047c6                  ValidateChars
                  0x00488e                  isShort
                  0x004946                  isDIR
                  0x0049f2                  FSfseek
                  0x004c16                  ReadFAT
                  0x004fc2                  WriteFAT
                  0x005426                  FSchdir
                  0x005436                  chdirhelper
                  0x0057d2                  FSgetcwd
                  0x005b36                  GetPreviousEntry
                  0x005cc8                  FSmkdir
                  0x005cd8                  mkdirhelper
                  0x005f32                  CreateDIR
                  0x00602e                  writeDotEntries
                  0x0061be                  FSrmdir
                  0x0061d2                  rmdirhelper
                  0x006628                  eraseDir
                  0x0066b6                  FormatDirName
                  0x006730                  FindFirst
                  0x006990                  FindNext
                  0x006b96                  GetFullClusterNumber
                  0x006bbe                  ReadByte
                  0x006bd0                  ReadWord
                  0x006c04                  ReadDWord
 .text            0x006c38       0x241a ..\Microchip\Usb\Objects - PIC24F Starter Kit\usb_host.o
                  0x006c38                  USBHostClearEndpointErrors
                  0x006c86                  USBHostDeviceRequest
                  0x006d50                  USBHostDeviceSpecificClientDriver
                  0x006d62                  USBHostDeviceStatus
                  0x006db6                  USBHostInit
                  0x006dfe                  USBHostRead
                  0x006eae                  USBHostResetDevice
                  0x006edc                  USBHostResumeDevice
                  0x006f0a                  USBHostSetDeviceConfiguration
                  0x006f4c                  USBHostShutdown
                  0x006f7c                  USBHostSuspendDevice
                  0x006faa                  USBHostTasks
                  0x007b2e                  USBHostTerminateTransfer
                  0x007b6c                  USBHostTransferIsComplete
                  0x007c16                  USBHostVbusEvent
                  0x007c52                  USBHostWrite
                  0x007d02                  _USB_CheckCommandAndEnumerationAttempts
                  0x007d48                  _USB_FindClassDriver
                  0x007dc4                  _USB_FindDeviceLevelClientDriver
                  0x007eb2                  _USB_FindInterface
                  0x007ee6                  _USB_FindNextToken
                  0x0082c6                  _USB_FreeConfigMemory
                  0x008314                  _USB_FreeMemory
                  0x00835c                  _USB_InitControlRead
                  0x0083d8                  _USB_InitControlWrite
                  0x008462                  _USB_InitRead
                  0x0084ea                  _USB_InitWrite
                  0x008572                  _USB_NotifyClients
                  0x008670                  _USB_ParseConfigurationDescriptor
                  0x008986                  _USB_ResetDATA0
                  0x0089b4                  _USB_SendToken
                  0x008a08                  _USB_SetBDT
                  0x008b5c                  _USB_TransferInProgress
                  0x008b88                  _USB1Interrupt
 .text            0x009052       0x1ba6 Objects - PIC24F Starter Kit\Games.o
                  0x009052                  InitializeRandomNumberGenerator
                  0x009068                  ProcessMessageGames
                  0x0090e4                  ProcessMessageScore
                  0x0090f6                  Random
                  0x00911e                  ShowScreenGames
                  0x009172                  ShowScreenScore
                  0x009208                  TranslateMessageScore
                  0x00922c                  DrawBlaster
                  0x009be0                  FindNextPosition
                  0x009db0                  ProcessMessageBlaster
                  0x009e40                  ShowScreenBlaster
                  0x009eea                  TranslateMessageBlaster
                  0x009f84                  CompactHorizontal
                  0x00a05e                  CompactVertical
                  0x00a10e                  FindBallNumber
                  0x00a15c                  MarkAllNeighbors
                  0x00a252                  MovesRemaining
                  0x00a32c                  ProcessMessageShapelet
                  0x00a4ea                  ShowScreenShapelet
                  0x00a5ba                  TranslateMessageShapelet
                  0x00a5d2                  DrawSnake
                  0x00a97a                  ProcessMessageSnake
                  0x00a9ea                  ShowScreenSnake
                  0x00ab78                  TranslateMessageSnake
 .text            0x00abf8       0x1568 ..\Microchip\Usb\MSD Host Driver\Objects - PIC24F Starter Kit\usb_host_msd.o
                  0x00abf8                  USBHostMSDDeviceStatus
                  0x00accc                  USBHostMSDResetDevice
                  0x00ad88                  USBHostMSDTasks
                  0x00ba3c                  USBHostMSDTerminateTransfer
                  0x00bade                  USBHostMSDTransfer
                  0x00bd6e                  USBHostMSDTransferIsComplete
                  0x00be4a                  USBHostMSDInitialize
                  0x00bfec                  USBHostMSDEventHandler
                  0x00c08c                  _USBHostMSD_GetNextTag
                  0x00c0a2                  _USBHostMSD_ResetStateJump
 .text            0x00c160       0x1002 Objects - PIC24F Starter Kit\Demos.o
                  0x00c160                  AdjustColorPWM
                  0x00c19a                  CaptureMonitorMedia
                  0x00c2dc                  DrawGraphLine
                  0x00c390                  DrawGridHorizontals
                  0x00c3b6                  DrawGridVerticals
                  0x00c3de                  GraphReadPotentiometer
                  0x00c4a6                  ProcessMessageDemos
                  0x00c53a                  ProcessMessageGraph
                  0x00c5b0                  ProcessMessageRGB
                  0x00c7aa                  RGBSetBlue
                  0x00c7c4                  RGBSetGreen
                  0x00c7de                  RGBSetRed
                  0x00c7f8                  RGBMapColorPins
                  0x00c84a                  RGBTurnOffLED
                  0x00c86c                  RGBTurnOnLED
                  0x00c8cc                  ProcessMessageBarDemo
                  0x00c8de                  ShowScreenCapture
                  0x00c99c                  ShowScreenCaptureMedia
                  0x00ca30                  ShowScreenDemos
                  0x00ca8e                  ShowScreenGraph
                  0x00cb4c                  ShowScreenRGB
                  0x00ccda                  ShowScreenBarDemo
                  0x00cd74                  DrawBarDemo
                  0x00cf4e                  TranslateMessageGraph
                  0x00cfb4                  TranslateMessageRGB
                  0x00d074                  UpdateGraph
                  0x00d0fe                  WriteOneBuffer
 .text            0x00d162        0xfa4 ..\Microchip\Graphics\Objects - PIC24F Starter Kit\Primitive.o
                  0x00d162                  InitGraph
                  0x00d190                  Arc
                  0x00d66a                  Line
                  0x00d8b4                  Bevel
                  0x00dba4                  FillBevel
                  0x00dd96                  DrawPoly
                  0x00ddf6                  Bar
                  0x00de32                  SetFont
                  0x00de62                  OutText
                  0x00de8c                  OutTextXY
                  0x00dec2                  OutChar
                  0x00dff4                  GetTextWidth
                  0x00e07e                  GetTextHeight
                  0x00e0a2                  GetImageWidth
                  0x00e0d4                  GetImageHeight
 .text            0x00e106        0xf60 ..\Microchip\Graphics\Objects - PIC24F Starter Kit\SH1101A.o
                  0x00e106                  DelayMs
                  0x00e12a                  ResetDevice
                  0x00e3e6                  PutPixel
                  0x00e5a2                  GetPixel
                  0x00e71e                  BarHS2
                  0x00eac0                  BarHSP
                  0x00ee7c                  ClearDevice
                  0x00ef08                  PutImage
                  0x00ef3e                  PutImage1BPP
 .text            0x00f066        0xd14 Objects - PIC24F Starter Kit\PIC24F Starter Kit.o
                  0x00f066                  main
                  0x00f0c8                  GOLDrawCallback
                  0x00f360                  GOLMsgCallback
                  0x00f4d2                  InitializeScreen
                  0x00f522                  PerformBoardTest
                  0x00f622                  ProcessMessageMain
                  0x00f680                  ShowScreenGeneric
                  0x00f748                  ShowScreenMain
                  0x00f7b2                  TickInit
                  0x00f7ca                  TranslateMessageGeneric
                  0x00fbea                  TranslateTouchpad
                  0x00fce6                  _T4Interrupt
                  0x00fd16                  _DefaultInterrupt
                  0x00fd2a                  _OscillatorFail
                  0x00fd3e                  _AddressError
                  0x00fd52                  _StackError
                  0x00fd66                  _MathError
 .text            0x00fd7a        0xc5a Objects - PIC24F Starter Kit\Utilities.o
                  0x00fd7a                  CalibrateCTMU
                  0x01000e                  IndicateFocus
                  0x010054                  ProcessMessageCTMU
                  0x010062                  ProcessMessageTime
                  0x0102fe                  ProcessMessageUtilities
                  0x01037a                  ShowScreenCTMU
                  0x0103b6                  ShowScreenTime
                  0x010770                  ShowScreenUtilities
                  0x0107ca                  TranslateMessageCTMU
                  0x0107d8                  TranslateMessageTime
                  0x01093e                  UpdateDateTime
 .text            0x0109d4        0x9a6 ..\Microchip\Graphics\Objects - PIC24F Starter Kit\Slider.o
                  0x0109d4                  SldCreate
                  0x010a76                  SldSetThumbSize
                  0x010aaa                  SldGetWidth
                  0x010b12                  SldGetHeight
                  0x010b7a                  SldGetMinMaxPos
                  0x010be8                  SldSetRange
                  0x010c76                  SldSetPage
                  0x010cba                  SldSetPos
                  0x010d8e                  SldMsgDefault
                  0x010e1a                  SldTranslateMsg
                  0x010e8e                  SldDraw
 .text            0x01137a        0x938 ..\Microchip\Graphics\Objects - PIC24F Starter Kit\Grid.o
                  0x01137a                  GridCreate
                  0x011454                  GridDraw
                  0x011858                  GridFreeItems
                  0x01187a                  GridSetCell
                  0x0118de                  GridClearCellState
                  0x011938                  GridSetFocus
                  0x011966                  GridSetCellState
                  0x0119be                  GridGetCell
                  0x011a20                  GridMsgDefault
                  0x011c1a                  GridTranslateMsg
 .text            0x011cb2        0x8d4 ..\Microchip\Graphics\Objects - PIC24F Starter Kit\GOL.o
                  0x011cb2                  GOLGetFocusNext
                  0x011ce6                  GOLSetFocus
                  0x011d24                  GOLCanBeFocused
                  0x011d6c                  GOLCreateScheme
                  0x011dbc                  GOLInit
                  0x011dca                  GOLFree
                  0x011e0e                  GOLDeleteObject
                  0x011e92                  GOLDeleteObjectByID
                  0x011eb2                  GOLFindObject
                  0x011ee0                  GOLAddObject
                  0x011f14                  GOLDraw
                  0x012006                  GOLRedrawRec
                  0x0120a8                  GOLMsg
                  0x012234                  GOLPanelDrawTsk
 .text            0x012586        0x850 ..\Microchip\Graphics\Objects - PIC24F Starter Kit\ListBox.o
                  0x012586                  LbCreate
                  0x012690                  LbAddItem
                  0x01272e                  LbDelItem
                  0x012790                  LbDelItemsList
                  0x0127bc                  LbGetSel
                  0x0127ec                  LbChangeSel
                  0x01284e                  LbSetFocusedItem
                  0x0128a6                  LbGetFocusedItem
                  0x0128e8                  LbTranslateMsg
                  0x012960                  LbMsgDefault
                  0x0129ea                  LbDraw
 .text            0x012dd6        0x82a Objects - PIC24F Starter Kit\Flash.o
                  0x012dd6                  FlashDeleteListBoxItems
                  0x012e08                  FlashDisplayDirectory
                  0x012e6c                  FlashDisplayFiles
                  0x012f04                  FlashFormatFileInformation
                  0x012f56                  FlashMonitorMedia
                  0x012ff2                  FlashUpdateVolume
                  0x013058                  ProcessMessageFlash
                  0x013142                  ProcessMessageFlashError
                  0x013154                  ShowScreenFlash
                  0x0131e8                  ShowScreenFlashError
                  0x013510                  TranslateMessageFlash
                  0x01357c                  TranslateMessageFlashError
                  0x0135a0                  USB_ApplicationEventHandler
 .text            0x013600        0x5b6 Objects - PIC24F Starter Kit\rtcc.o
                  0x013600                  RTCCProcessEvents
                  0x0138a2                  RTCCInit
                  0x0138e2                  RTCCSet
                  0x013928                  RTCCUnlock
                  0x01393e                  RTCCSetBinSec
                  0x013980                  RTCCSetBinMin
                  0x0139c2                  RTCCSetBinHour
                  0x013a04                  RTCCCalculateWeekDay
                  0x013a8a                  RTCCSetBinDay
                  0x013b20                  RTCCSetBinMonth
                  0x013b60                  RTCCSetBinYear
 .text            0x013bb6        0x4ee ..\Microchip\Graphics\Objects - PIC24F Starter Kit\RoundDial.o
                  0x013bb6                  RdiaCreate
                  0x013c58                  RdiaMsgDefault
                  0x013c90                  RdiaCosine
                  0x013cf6                  RdiaSine
                  0x013d5c                  RdiaTranslateMsg
                  0x013e58                  RdiaDraw
 .text            0x0140a4        0x4e6 ..\Microchip\Graphics\Objects - PIC24F Starter Kit\Button.o
                  0x0140a4                  BtnCreate
                  0x014178                  BtnSetText
                  0x0141aa                  BtnMsgDefault
                  0x0141ee                  BtnTranslateMsg
                  0x01429e                  BtnDraw
 .text            0x01458a        0x4c4 Objects - PIC24F Starter Kit\TouchSense.o
                  0x01458a                  CTMUInit
                  0x014602                  ReadCTMU
                  0x0148bc                  SetNextChannel
                  0x0148d2                  TouchSenseButtonsMsg
 .text            0x014a4e        0x450 ..\Microchip\Graphics\Objects - PIC24F Starter Kit\EditBox.o
                  0x014a4e                  EbCreate
                  0x014b04                  EbSetText
                  0x014b5a                  EbAddChar
                  0x014b96                  EbDeleteChar
                  0x014bbe                  EbTranslateMsg
                  0x014c12                  EbMsgDefault
                  0x014c58                  EbDraw

C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn8
                  0x014e9e        0x40a
 C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn8
                  0x014e9e        0x40a Objects - PIC24F Starter Kit\Pictures.o
                  0x014e9e                  L4298

C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn9
                  0x0152a8        0x40a
 C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn9
                  0x0152a8        0x40a Objects - PIC24F Starter Kit\Pictures.o
                  0x0152a8                  L29552

.text             0x0156b2        0x97a
 .text            0x0156b2        0x3e8 ..\Microchip\Usb\MSD Host Driver\Objects - PIC24F Starter Kit\usb_host_msd_scsi.o
                  0x0156b2                  USBHostMSDSCSIInitialize
                  0x0156d4                  USBHostMSDSCSIEventHandler
                  0x015746                  USBHostMSDSCSIMediaDetect
                  0x015766                  USBHostMSDSCSIMediaInitialize
                  0x0158a6                  USBHostMSDSCSIMediaReset
                  0x0158f6                  USBHostMSDSCSISectorRead
                  0x0159b8                  USBHostMSDSCSISectorWrite
                  0x015a92                  USBHostMSDSCSIWriteProtectState
 .text            0x015a9a        0x31a ..\Microchip\Graphics\Objects - PIC24F Starter Kit\StaticText.o
                  0x015a9a                  StCreate
                  0x015b3a                  StSetText
                  0x015b5a                  StTranslateMsg
                  0x015b7c                  StDraw
 .text            0x015db4        0x278 ..\Microchip\Graphics\Objects - PIC24F Starter Kit\Picture.o
                  0x015db4                  PictCreate
                  0x015e3c                  PictTranslateMsg
                  0x015e5e                  PictDraw

.dinit            0x01602c        0x1c0
 .dinit           0x01602c        0x1c0 data_init

C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn7
                  0x0161ec         0x2a
 C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn7
                  0x0161ec         0x2a Objects - PIC24F Starter Kit\Pictures.o
                  0x0161ec                  L17009

C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn6
                  0x016216         0x1e
 C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn6
                  0x016216         0x1e Objects - PIC24F Starter Kit\Pictures.o
                  0x016216                  L8740

C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn1
                  0x016234         0x12
 C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn1
                  0x016234         0x12 Objects - PIC24F Starter Kit\Pictures.o
                  0x016234                  L17048

C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn2
                  0x016246         0x12
 C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn2
                  0x016246         0x12 Objects - PIC24F Starter Kit\Pictures.o
                  0x016246                  L18321

C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn3
                  0x016258         0x12
 C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn3
                  0x016258         0x12 Objects - PIC24F Starter Kit\Pictures.o
                  0x016258                  L2447

C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn4
                  0x01626a         0x12
 C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn4
                  0x01626a         0x12 Objects - PIC24F Starter Kit\Pictures.o
                  0x01626a                  L32264

C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn5
                  0x01627c         0x12
 C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn5
                  0x01627c         0x12 Objects - PIC24F Starter Kit\Pictures.o
                  0x01627c                  L10673

C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn10
                  0x01628e         0x12
 C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn10
                  0x01628e         0x12 Objects - PIC24F Starter Kit\Pictures.o
                  0x01628e                  L4126

C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn11
                  0x0162a0         0x12
 C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn11
                  0x0162a0         0x12 Objects - PIC24F Starter Kit\Pictures.o
                  0x0162a0                  L8993

C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn12
                  0x0162b2         0x12
 C:\Users\MICROC~1\AppData\Local\Temp/ccMKnQfU.s.scn12
                  0x0162b2         0x12 Objects - PIC24F Starter Kit\Pictures.o
                  0x0162b2                  L18976
