Microchip TCP/IP Stack Features

| Microchip TCP/IP Stack

Home | Features | Architecture | Stack Footprint

The Microchip ENC28J60 and PIC18F97J60 family Ethernet module offers:
* IEEE 802.3 compatibility
* 10Base-T port
* 8Kbytes of SRAM buffer
* Internal DMA module for fast data movement
* Hardware assisted IP checksum calculations
* Programmable receive filters minimizing unwanted packets
* 5V tolerant inputs
Features specific to the ENC28J60 include:
* SPI interface with speeds up to 20Mb/s
* 28 pin package
The Microchip TCP/IP Stack offers:
* No royalty or license fee
* Portable across Microchip PIC18, PIC24F, PIC24H, dsPIC30, and dsPIC33 family of microcontrollers
* Out-of-box support for Microchip C18, C30 and HI TECH PICC18 compilers
* RTOS independent
* Implements complete TCP state machine
* Multiple TCP and UDP sockets with simultaneous connection/management
* Modular design to easily add new components
* Use it as a part of HTTP Server (included) or any custom TCP/IP based application
* Includes powerful and yet simple Microchip File System (MPFS)
* PC based program to convert PC files into MPFS image
* Included Modules: MAC, ARP, IP, ICMP, TCP, UDP, DHCP, FTP, IP Gleaning, HTTP, MPFS, Announce, DNS, NetBIOS Name Service, SMTP, SNMP, and more.
* Bonus firmware modules: external SPI serial EEPROM, Tick Manager, Xmodem Receiver