Archive member included because of file (symbol)

c:/program files/microchip/mplab c30/bin/bin/../../lib\libpic30-coff.a(crt1.o)
                              (_resetALT)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libpic30-coff.a(crt0.o)
                              (_resetPRI)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(divmoddi3.o)
                              ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Tick.o (__udivdi3)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(udivsi3.o)
                              ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Helpers.o (__udivsi3)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(muldi3.o)
                              ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCPPerformanceTest.o (__muldi3)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(umuldi3.o)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(muldi3.o) (__umuldi3)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strlen.o)
                              Objects - TCPIP Demo App-C30\MainDemo.o (strlen)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strcpy.o)
                              Objects - TCPIP Demo App-C30\MainDemo.o (strcpy)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memcmp.o)
                              Objects - TCPIP Demo App-C30\CustomHTTPApp.o (memcmp)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strcmp.o)
                              Objects - TCPIP Demo App-C30\CustomHTTPApp.o (strcmp)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memset.o)
                              Objects - TCPIP Demo App-C30\CustomHTTPApp.o (memset)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xstoul.o)
                              Objects - TCPIP Demo App-C30\CustomHTTPApp.o (_Stoul)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(rand.o)
                              ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Helpers.o (rand)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(srand.o)
                              ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Helpers.o (srand)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strchr.o)
                              ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SMTP.o (strchr)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strstr.o)
                              ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SMTP.o (strstr)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memcpy.o)
                              ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCP.o (memcpy)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strncmp.o)
                              Objects - TCPIP Demo App-C30\CustomSNMPApp.o (strncmp)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(isspace.os)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xstoul.o) (isspace)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(tolower.os)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xstoul.o) (tolower)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memchr.o)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xstoul.o) (memchr)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(errno.o)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xstoul.o) (errno)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(mulsi3.o)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xstoul.o) (__mulsi3)


Program Memory Usage

section                    address   length (PC units)   length (bytes) (dec)
-------                    -------   -----------------   --------------------
.reset                           0                 0x4             0x6  (6)
.ivt                           0x4                0xfc           0x17a  (378)
.aivt                        0x104                0xfc           0x17a  (378)
.text                        0x200               0x674           0x9ae  (2478)
.const                       0x874              0x170a          0x228f  (8847)
.text                       0x1f7e              0x20ca          0x312f  (12591)
.text                       0x4048              0x1f10          0x2e98  (11928)
.text                       0x5f58              0x1a32          0x274b  (10059)
.text                       0x798a              0x1a2a          0x273f  (10047)
.text                       0x93b4               0xec0          0x1620  (5664)
.text                       0xa274               0xcb6          0x1311  (4881)
.text                       0xaf2a               0xad2          0x103b  (4155)
.text                       0xb9fc               0xa58           0xf84  (3972)
.text                       0xc454               0x988           0xe4c  (3660)
.text                       0xcddc               0x964           0xe16  (3606)
.text                       0xd740               0x956           0xe01  (3585)
.text                       0xe096               0x8d2           0xd3b  (3387)
.text                       0xe968               0x792           0xb5b  (2907)
.text                       0xf0fa               0x532           0x7cb  (1995)
.text                       0xf62c               0x51a           0x7a7  (1959)
.text                       0xfb46               0x4c4           0x726  (1830)
.text                      0x1000a               0x498           0x6e4  (1764)
.text                      0x104a2               0x46c           0x6a2  (1698)
.text                      0x1090e               0x3a8           0x57c  (1404)
.text                      0x10cb6               0x386           0x549  (1353)
.text                      0x1103c               0x32e           0x4c5  (1221)
.text                      0x1136a               0x2da           0x447  (1095)
.text                      0x11644               0x2cc           0x432  (1074)
.dinit                     0x11910               0x2c6           0x429  (1065)
.text                      0x11bd6               0x29e           0x3ed  (1005)
.text                      0x11e74               0x27c           0x3ba  (954)
.text                      0x120f0               0x274           0x3ae  (942)
.text                      0x12364               0x262           0x393  (915)
.text                      0x125c6               0x1e0           0x2d0  (720)
.text                      0x127a6               0x1ac           0x282  (642)
.text                      0x12952               0x1a8           0x27c  (636)
.text                      0x12afa               0x166           0x219  (537)
.text                      0x12c60               0x15a           0x207  (519)
.text                      0x12dba               0x152           0x1fb  (507)
.text                      0x12f0c               0x150           0x1f8  (504)
.text                      0x1305c               0x14e           0x1f5  (501)
.text                      0x131aa               0x11e           0x1ad  (429)
.text                      0x132c8               0x106           0x189  (393)
.text                      0x133ce                0xfa           0x177  (375)
.text                      0x134c8                0xea           0x15f  (351)
.text                      0x135b2                0xd0           0x138  (312)
.text                      0x13682                0x56            0x81  (129)
.isr                       0x136d8                 0x2             0x3  (3)
__CONFIG2                  0x157fc                 0x2             0x3  (3)
__CONFIG1                  0x157fe                 0x2             0x3  (3)

                     Total program memory used (bytes):        0x1d247  (119367) 90%


Data Memory Usage

section                    address      alignment gaps    total length  (dec)
-------                    -------      --------------    -------------------
.nbss                        0x800                   0           0x3fc  (1020)
.ndata                       0xbfc                   0            0x72  (114)
.nbss                        0xc6e                   0           0x12a  (298)
.ndata                       0xd98                   0            0x98  (152)
.nbss                        0xe30                   0           0x130  (304)
.ndata                       0xf60                   0            0x26  (38)
.nbss                        0xf86                   0            0x22  (34)
.ndata                       0xfa8                   0            0x22  (34)
.nbss                        0xfca                   0            0xaa  (170)
.ndata                      0x1074                   0            0x16  (22)
.nbss                       0x108a                   0            0x4e  (78)
.ndata                      0x10d8                   0             0xa  (10)
.nbss                       0x10e2                   0            0x18  (24)
.ndata                      0x10fa                   0             0x6  (6)
.nbss                       0x1100                   0             0xc  (12)
.ndata                      0x110c                   0             0x4  (4)
.nbss                       0x1110                   0             0x4  (4)
.ndata                      0x1114                   0             0x4  (4)
.nbss                       0x1118                   0            0x10  (16)
.ndata                      0x1128                   0             0x6  (6)
_0185a7004a392480           0x112e                   0             0x2  (2)
.ndata                      0x1130                   0             0x2  (2)
_018768504a392489           0x1132                   0             0x2  (2)
.ndata                      0x1134                   0             0x8  (8)
_0189f7704a3924a4           0x113c                   0             0x2  (2)
.ndata                      0x113e                   0             0x6  (6)
.bss                        0x1144                   0            0x88  (136)
.data                       0x11cc                   0            0x58  (88)

                        Total data memory used (bytes):          0xa24  (2596) 31%


Dynamic Memory Usage

region                     address                      maximum length  (dec)
------                     -------                      ---------------------
heap                             0                                   0  (0)
stack                       0x1224                              0x15dc  (5596)

                        Maximum dynamic memory (bytes):         0x15dc  (5596)


External Symbols in Data Memory (by address):

                    0x0a68                  _UDPSocketInfo
                    0x0af4                  _activeUDPSocket
                    0x0af6                  _UDPTxCount
                    0x0af8                  _UDPRxCount
                    0x0afa                  _curHTTP
                    0x0b7c                  _httpStubs
                    0x0b84                  _curHTTPID
                    0x0b8a                  _AppConfig
                    0x0bf3                  _AN0String
                    0x0cda                  _lastRead
                    0x0e30                  _lastBlock
                    0x0e9a                  _DDNSClient
                    0x0ecc                  _SMTPClient
                    0x0f0a                  _snmpReqVarErrStatus
                    0x0f60                  _gSendTrapFlag
                    0x0f61                  _gOIDCorrespondingSnmpMibID
                    0x0f62                  _gGenericTrapNotification
                    0x0f63                  _gSpecificTrapNotification
                    0x0f64                  _trapInfo
                    0x0fc2                  _ddnsServiceHosts
                    0x0fca                  _LCDText
                    0x10c4                  _remoteNode
                    0x10fa                  _smDHCPState
                    0x10fc                  _DHCPFlags
                    0x10fe                  _DHCPBindCount
                    0x110c                  _myDHCPBindCount
                    0x110e                  ___C30_UART
                    0x1130                  _bDHCPServerEnabled
                    0x1216                  __Tls_setup__Randseed
                    0x1218                  __Randseed
                    0x121c                  __Tls_setup__Randinit
                    0x121e                  __Randinit
                    0x1220                  __Tls_setup_errno
                    0x1222                  _errno

External Symbols in Data Memory (by name):

                    0x0bf3                  _AN0String
                    0x0b8a                  _AppConfig
                    0x0e9a                  _DDNSClient
                    0x10fe                  _DHCPBindCount
                    0x10fc                  _DHCPFlags
                    0x0fca                  _LCDText
                    0x0ecc                  _SMTPClient
                    0x0af8                  _UDPRxCount
                    0x0a68                  _UDPSocketInfo
                    0x0af6                  _UDPTxCount
                    0x121e                  __Randinit
                    0x1218                  __Randseed
                    0x121c                  __Tls_setup__Randinit
                    0x1216                  __Tls_setup__Randseed
                    0x1220                  __Tls_setup_errno
                    0x110e                  ___C30_UART
                    0x0af4                  _activeUDPSocket
                    0x1130                  _bDHCPServerEnabled
                    0x0afa                  _curHTTP
                    0x0b84                  _curHTTPID
                    0x0fc2                  _ddnsServiceHosts
                    0x1222                  _errno
                    0x0f62                  _gGenericTrapNotification
                    0x0f61                  _gOIDCorrespondingSnmpMibID
                    0x0f60                  _gSendTrapFlag
                    0x0f63                  _gSpecificTrapNotification
                    0x0b7c                  _httpStubs
                    0x0e30                  _lastBlock
                    0x0cda                  _lastRead
                    0x110c                  _myDHCPBindCount
                    0x10c4                  _remoteNode
                    0x10fa                  _smDHCPState
                    0x0f0a                  _snmpReqVarErrStatus
                    0x0f64                  _trapInfo

External Symbols in Program Memory (by address):

                  0x000200                  __resetPRI
                  0x00021e                  __psv_init
                  0x00022e                  __data_init
                  0x000288                  _strlen
                  0x000296                  _strcpy
                  0x0002a6                  _memcmp
                  0x0002c2                  _strcmp
                  0x0002e6                  _memset
                  0x0002f4                  __Stoul
                  0x00041c                  _rand
                  0x0004c6                  _srand
                  0x0004e8                  _strchr
                  0x0004fa                  _strstr
                  0x000522                  _memcpy
                  0x000530                  _strncmp
                  0x000554                  _isspace
                  0x000564                  _tolower
                  0x000572                  _memchr
                  0x000586                  __Geterrno
                  0x0005b8                  ___udivmoddi3
                  0x000686                  ___udivdi3
                  0x000694                  ___umoddi3
                  0x00069c                  ___divdi3
                  0x0006d6                  ___moddi3
                  0x0007a8                  ___udivsi3
                  0x0007c8                  ___muldi3
                  0x000824                  ___umuldi3
                  0x000868                  ___mulsi3
                  0x0012b1                  _HTML_UP_ARROW
                  0x0012b4                  _HTML_DOWN_ARROW
                  0x001ed4                  _TCPSocketInitializer
                  0x00201a                  _TCPInit
                  0x0020e0                  _TCPOpen
                  0x002226                  _TCPWasReset
                  0x00224a                  _TCPIsConnected
                  0x002266                  _TCPDisconnect
                  0x0022e8                  _TCPGetRemoteInfo
                  0x002304                  _TCPFlush
                  0x002320                  _TCPIsPutReady
                  0x00236a                  _TCPPut
                  0x0023f6                  _TCPPutArray
                  0x0024c4                  _TCPPutString
                  0x0024e2                  _TCPGetTxFIFOFull
                  0x002500                  _TCPDiscard
                  0x00251e                  _TCPIsGetReady
                  0x002550                  _TCPGet
                  0x0025ba                  _TCPGetArray
                  0x002676                  _TCPGetRxFIFOFree
                  0x002692                  _TCPFindArrayEx
                  0x002916                  _TCPFindEx
                  0x002934                  _TCPTick
                  0x002da2                  _TCPProcess
                  0x003e2e                  _TCPAdjustFIFOSize
                  0x004048                  _SNMPInit
                  0x00405e                  _SNMPTask
                  0x0040ee                  _SNMPNotifyPrepare
                  0x004128                  _SNMPIsNotifyReady
                  0x00416c                  _SNMPNotify
                  0x005f58                  _HTTPPrint
                  0x0061ce                  _HTTPPrint_
                  0x0061e8                  _HTTPInit
                  0x006258                  _HTTPServer
                  0x007388                  _HTTPURLDecode
                  0x00744e                  _HTTPGetArg
                  0x007496                  _HTTPReadPostName
                  0x0074be                  _HTTPReadPostValue
                  0x0078c2                  _HTTPIncFile
                  0x00798a                  _HTTPNeedsAuth
                  0x0079d4                  _HTTPCheckAuth
                  0x007a2c                  _HTTPExecuteGet
                  0x007c56                  _HTTPExecutePost
                  0x00890a                  _HTTPPrint_builddate
                  0x00894a                  _HTTPPrint_version
                  0x008966                  _HTTPPrint_btn
                  0x0089e6                  _HTTPPrint_led
                  0x008ab6                  _HTTPPrint_ledSelected
                  0x008b90                  _HTTPPrint_pot
                  0x008bb6                  _HTTPPrint_lcdtext
                  0x008c9a                  _HTTPPrint_hellomsg
                  0x008cd8                  _HTTPPrint_cookiename
                  0x008d18                  _HTTPPrint_uploadedmd5
                  0x008df2                  _HTTPPrintIP
                  0x008e46                  _HTTPPrint_config_hostname
                  0x008e60                  _HTTPPrint_config_dhcpchecked
                  0x008e84                  _HTTPPrint_config_ip
                  0x008eaa                  _HTTPPrint_config_gw
                  0x008ed0                  _HTTPPrint_config_subnet
                  0x008ef6                  _HTTPPrint_config_dns1
                  0x008f1c                  _HTTPPrint_config_dns2
                  0x008f42                  _HTTPPrint_config_mac
                  0x008fe0                  _HTTPPrint_read_comm
                  0x00900e                  _HTTPPrint_write_comm
                  0x00903c                  _HTTPPrint_reboot
                  0x009044                  _HTTPPrint_rebootaddr
                  0x00905e                  _HTTPPrint_ddns_user
                  0x0090b6                  _HTTPPrint_ddns_pass
                  0x00910e                  _HTTPPrint_ddns_host
                  0x009166                  _HTTPPrint_ddns_service
                  0x0091a6                  _HTTPPrint_ddns_status
                  0x00920e                  _HTTPPrint_ddns_status_msg
                  0x009300                  _HTTPPrint_smtps_en
                  0x00931c                  _HTTPPrint_snmp_en
                  0x009338                  _HTTPPrint_status_ok
                  0x009376                  _HTTPPrint_status_fail
                  0x0093b4                  _SMTPBeginUsage
                  0x009408                  _SMTPEndUsage
                  0x009450                  _SMTPTask
                  0x009fac                  _SMTPSendMail
                  0x009fb4                  _SMTPIsBusy
                  0x009fca                  _SMTPIsPutReady
                  0x009fe6                  _SMTPPut
                  0x00a086                  _SMTPPutArray
                  0x00a0c2                  _SMTPPutString
                  0x00a0f8                  _SMTPFlush
                  0x00a104                  _SMTPPutDone
                  0x00a274                  _MACInit
                  0x00a394                  _MACIsLinked
                  0x00a3a8                  _MACIsTxReady
                  0x00a3c0                  _MACDiscardRx
                  0x00a3f4                  _MACGetFreeRxSize
                  0x00a47c                  _MACGetHeader
                  0x00a55e                  _MACPutHeader
                  0x00a5b2                  _MACFlush
                  0x00a6ce                  _MACSetReadPtrInRx
                  0x00a6fc                  _MACSetWritePtr
                  0x00a72a                  _MACSetReadPtr
                  0x00a758                  _MACCalcRxChecksum
                  0x00a7b0                  _CalcIPBufferChecksum
                  0x00a864                  _MACMemCopyAsync
                  0x00aa12                  _MACIsMemCopyDone
                  0x00aa2a                  _MACGet
                  0x00aa5c                  _MACGetArray
                  0x00ab36                  _MACPut
                  0x00ab6e                  _MACPutArray
                  0x00ad2a                  _ReadPHYReg
                  0x00ae5c                  _WritePHYReg
                  0x00aeac                  _MACPowerDown
                  0x00aeda                  _MACPowerUp
                  0x00aefa                  _SetCLKOUT
                  0x00af10                  _GetCLKOUT
                  0x00af2a                  _MPFSInit
                  0x00af60                  _MPFSOpen
                  0x00b0ae                  _MPFSOpenID
                  0x00b132                  _MPFSClose
                  0x00b154                  _MPFSGet
                  0x00b25a                  _MPFSGetArray
                  0x00b36e                  _MPFSGetLong
                  0x00b38e                  _MPFSSeek
                  0x00b56a                  _MPFSFormat
                  0x00b604                  _MPFSPutArray
                  0x00b6a8                  _MPFSPutEnd
                  0x00b704                  _MPFSGetTimestamp
                  0x00b752                  _MPFSGetMicrotime
                  0x00b7a0                  _MPFSGetFlags
                  0x00b7e4                  _MPFSGetSize
                  0x00b832                  _MPFSGetBytesRem
                  0x00b87a                  _MPFSGetStartAddr
                  0x00b8ca                  _MPFSGetEndAddr
                  0x00b924                  _MPFSGetFilename
                  0x00b98c                  _MPFSGetPosition
                  0x00b9ac                  _MPFSGetID
                  0x00bab8                  _SNMPTrapDemo
                  0x00bbe8                  _SNMPSendTrap
                  0x00bd1c                  _SNMPValidateCommunity
                  0x00bdc0                  _SNMPIsValidSetLen
                  0x00bdfc                  _SNMPSetVar
                  0x00bfbe                  _SNMPGetNextIndex
                  0x00c016                  _SNMPGetVar
                  0x00c454                  _BerkeleySocketInit
                  0x00c49a                  _socket
                  0x00c518                  _bind
                  0x00c58c                  _listen
                  0x00c68a                  _accept
                  0x00c76c                  _connect
                  0x00c8aa                  _send
                  0x00c9ec                  _sendto
                  0x00cb2e                  _recv
                  0x00cc5a                  _recvfrom
                  0x00cd14                  _gethostname
                  0x00cd78                  _closesocket
                  0x00cddc                  _DDNSInit
                  0x00ce1e                  _DDNSTask
                  0x00d6f6                  _DDNSForceUpdate
                  0x00d70c                  _DDNSSetService
                  0x00d72c                  _DDNSGetLastIP
                  0x00d738                  _DDNSGetLastStatus
                  0x00d740                  _GenerateRandomDWORD
                  0x00d85a                  _StringToIPAddress
                  0x00d9da                  _Base64Decode
                  0x00db40                  _Base64Encode
                  0x00dc9c                  _uitoa
                  0x00dd1a                  _ultoa
                  0x00ddca                  _hexatob
                  0x00de40                  _btohexa_high
                  0x00de68                  _btohexa_low
                  0x00de8e                  _stricmppgm2ram
                  0x00df26                  _swaps
                  0x00df40                  _swapl
                  0x00df9e                  _CalcIPChecksum
                  0x00e014                  _strupr
                  0x00e04e                  _FormatNetBIOSName
                  0x00e096                  _DHCPReset
                  0x00e0b8                  _DHCPDisable
                  0x00e0d4                  _DHCPEnable
                  0x00e0ec                  _DHCPTask
                  0x00e968                  _DNSBeginUsage
                  0x00e984                  _DNSEndUsage
                  0x00e9aa                  _DNSResolve
                  0x00e9da                  _DNSIsResolved
                  0x00f0fa                  _UDPInit
                  0x00f114                  _UDPTask
                  0x00f11e                  _UDPOpen
                  0x00f1ac                  _UDPClose
                  0x00f1d6                  _UDPSetTxBuffer
                  0x00f1ea                  _UDPSetRxBuffer
                  0x00f1fe                  _UDPIsPutReady
                  0x00f234                  _UDPPut
                  0x00f268                  _UDPPutArray
                  0x00f2a0                  _UDPPutString
                  0x00f2b6                  _UDPFlush
                  0x00f38c                  _UDPIsGetReady
                  0x00f3bc                  _UDPGet
                  0x00f3f2                  _UDPGetArray
                  0x00f43c                  _UDPDiscard
                  0x00f458                  _UDPProcess
                  0x00f62c                  _DHCPServerTask
                  0x00fb46                  _HashAddData
                  0x00fb62                  _MD5Initialize
                  0x00fb9e                  _MD5AddData
                  0x00fe9e                  _MD5Calculate
                  0x01000a                  _TelnetTask
                  0x0104a2                  __AddressError
                  0x0104ac                  __StackError
                  0x0104b6                  _main
                  0x01060a                  _DisplayIPValue
                  0x0108f4                  _SaveAppConfig
                  0x010988                  _ARPInit
                  0x0109be                  _ARPProcess
                  0x010abe                  _ARPResolve
                  0x010b8a                  _ARPIsResolved
                  0x010cb6                  _NBNSTask
                  0x01103c                  _XEEInit
                  0x01105a                  _XEEBeginRead
                  0x01106e                  _XEERead
                  0x0110ac                  _XEEEndRead
                  0x0110b4                  _XEEReadArray
                  0x011180                  _XEEBeginWrite
                  0x011194                  _XEEWrite
                  0x0111d0                  _XEEWriteArray
                  0x0111f2                  _XEEEndWrite
                  0x0112fe                  _XEEIsBusy
                  0x01136a                  _TCPPerformanceTask
                  0x011374                  _TCPTXPerformanceTask
                  0x011532                  _TCPRXPerformanceTask
                  0x011644                  _SNTPClient
                  0x0118b8                  _SNTPGetUTCSeconds
                  0x011bd6                  _BerkeleyUDPClientDemo
                  0x011e1c                  _BerkeleySNTPGetUTCSeconds
                  0x011e74                  _StackInit
                  0x011eb4                  _StackTask
                  0x0120ba                  _StackApplications
                  0x0120f0                  _ICMPProcess
                  0x0121b0                  _ICMPSendPing
                  0x0121cc                  _ICMPSendPingToHost
                  0x0121e8                  _ICMPGetReply
                  0x012340                  _ICMPBeginUsage
                  0x01235c                  _ICMPEndUsage
                  0x012364                  _DoUARTConfig
                  0x0125c6                  _UART2TCPBridgeInit
                  0x0125dc                  _UART2TCPBridgeTask
                  0x012738                  __U2RXInterrupt
                  0x012776                  __U2TXInterrupt
                  0x0127a6                  _IPGetHeader
                  0x012870                  _IPPutHeader
                  0x01290e                  _IPSetRxBuffer
                  0x012996                  _LCDInit
                  0x012a22                  _LCDUpdate
                  0x012ade                  _LCDErase
                  0x012afa                  _AnnounceIP
                  0x012b7c                  _DiscoveryTask
                  0x012c60                  _GenericTCPClient
                  0x012dba                  _ReadStringUART
                  0x012e02                  _putsUART2
                  0x012e50                  _getsUART2
                  0x012eb8                  _DataRdyUART2
                  0x012ec4                  _BusyUART2
                  0x012ed2                  _ReadUART2
                  0x012ef0                  _WriteUART2
                  0x012f0c                  _BerkeleyTCPServerDemo
                  0x01305c                  _RebootTask
                  0x0131aa                  _BerkeleyTCPClientDemo
                  0x0132c8                  _SMTPDemo
                  0x0133ce                  _TickInit
                  0x01344a                  _TickGet
                  0x013456                  _TickGetDiv256
                  0x013470                  _TickGetDiv64K
                  0x01348a                  _TickConvertToMilliseconds
                  0x0134b0                  __T1Interrupt
                  0x0134c8                  _PingDemo
                  0x0135b2                  _GenericTCPServer
                  0x013682                  _DelayMs
                  0x0136ac                  _Delay10us
                  0x0136d8                  __DefaultInterrupt

External Symbols in Program Memory (by name):

                  0x010988                  _ARPInit
                  0x010b8a                  _ARPIsResolved
                  0x0109be                  _ARPProcess
                  0x010abe                  _ARPResolve
                  0x012afa                  _AnnounceIP
                  0x00d9da                  _Base64Decode
                  0x00db40                  _Base64Encode
                  0x011e1c                  _BerkeleySNTPGetUTCSeconds
                  0x00c454                  _BerkeleySocketInit
                  0x0131aa                  _BerkeleyTCPClientDemo
                  0x012f0c                  _BerkeleyTCPServerDemo
                  0x011bd6                  _BerkeleyUDPClientDemo
                  0x012ec4                  _BusyUART2
                  0x00a7b0                  _CalcIPBufferChecksum
                  0x00df9e                  _CalcIPChecksum
                  0x00d6f6                  _DDNSForceUpdate
                  0x00d72c                  _DDNSGetLastIP
                  0x00d738                  _DDNSGetLastStatus
                  0x00cddc                  _DDNSInit
                  0x00d70c                  _DDNSSetService
                  0x00ce1e                  _DDNSTask
                  0x00e0b8                  _DHCPDisable
                  0x00e0d4                  _DHCPEnable
                  0x00e096                  _DHCPReset
                  0x00f62c                  _DHCPServerTask
                  0x00e0ec                  _DHCPTask
                  0x00e968                  _DNSBeginUsage
                  0x00e984                  _DNSEndUsage
                  0x00e9da                  _DNSIsResolved
                  0x00e9aa                  _DNSResolve
                  0x012eb8                  _DataRdyUART2
                  0x0136ac                  _Delay10us
                  0x013682                  _DelayMs
                  0x012b7c                  _DiscoveryTask
                  0x01060a                  _DisplayIPValue
                  0x012364                  _DoUARTConfig
                  0x00e04e                  _FormatNetBIOSName
                  0x00d740                  _GenerateRandomDWORD
                  0x012c60                  _GenericTCPClient
                  0x0135b2                  _GenericTCPServer
                  0x00af10                  _GetCLKOUT
                  0x0012b4                  _HTML_DOWN_ARROW
                  0x0012b1                  _HTML_UP_ARROW
                  0x0079d4                  _HTTPCheckAuth
                  0x007a2c                  _HTTPExecuteGet
                  0x007c56                  _HTTPExecutePost
                  0x00744e                  _HTTPGetArg
                  0x0078c2                  _HTTPIncFile
                  0x0061e8                  _HTTPInit
                  0x00798a                  _HTTPNeedsAuth
                  0x005f58                  _HTTPPrint
                  0x008df2                  _HTTPPrintIP
                  0x0061ce                  _HTTPPrint_
                  0x008966                  _HTTPPrint_btn
                  0x00890a                  _HTTPPrint_builddate
                  0x008e60                  _HTTPPrint_config_dhcpchecked
                  0x008ef6                  _HTTPPrint_config_dns1
                  0x008f1c                  _HTTPPrint_config_dns2
                  0x008eaa                  _HTTPPrint_config_gw
                  0x008e46                  _HTTPPrint_config_hostname
                  0x008e84                  _HTTPPrint_config_ip
                  0x008f42                  _HTTPPrint_config_mac
                  0x008ed0                  _HTTPPrint_config_subnet
                  0x008cd8                  _HTTPPrint_cookiename
                  0x00910e                  _HTTPPrint_ddns_host
                  0x0090b6                  _HTTPPrint_ddns_pass
                  0x009166                  _HTTPPrint_ddns_service
                  0x0091a6                  _HTTPPrint_ddns_status
                  0x00920e                  _HTTPPrint_ddns_status_msg
                  0x00905e                  _HTTPPrint_ddns_user
                  0x008c9a                  _HTTPPrint_hellomsg
                  0x008bb6                  _HTTPPrint_lcdtext
                  0x0089e6                  _HTTPPrint_led
                  0x008ab6                  _HTTPPrint_ledSelected
                  0x008b90                  _HTTPPrint_pot
                  0x008fe0                  _HTTPPrint_read_comm
                  0x00903c                  _HTTPPrint_reboot
                  0x009044                  _HTTPPrint_rebootaddr
                  0x009300                  _HTTPPrint_smtps_en
                  0x00931c                  _HTTPPrint_snmp_en
                  0x009376                  _HTTPPrint_status_fail
                  0x009338                  _HTTPPrint_status_ok
                  0x008d18                  _HTTPPrint_uploadedmd5
                  0x00894a                  _HTTPPrint_version
                  0x00900e                  _HTTPPrint_write_comm
                  0x007496                  _HTTPReadPostName
                  0x0074be                  _HTTPReadPostValue
                  0x006258                  _HTTPServer
                  0x007388                  _HTTPURLDecode
                  0x00fb46                  _HashAddData
                  0x012340                  _ICMPBeginUsage
                  0x01235c                  _ICMPEndUsage
                  0x0121e8                  _ICMPGetReply
                  0x0120f0                  _ICMPProcess
                  0x0121b0                  _ICMPSendPing
                  0x0121cc                  _ICMPSendPingToHost
                  0x0127a6                  _IPGetHeader
                  0x012870                  _IPPutHeader
                  0x01290e                  _IPSetRxBuffer
                  0x012ade                  _LCDErase
                  0x012996                  _LCDInit
                  0x012a22                  _LCDUpdate
                  0x00a758                  _MACCalcRxChecksum
                  0x00a3c0                  _MACDiscardRx
                  0x00a5b2                  _MACFlush
                  0x00aa2a                  _MACGet
                  0x00aa5c                  _MACGetArray
                  0x00a3f4                  _MACGetFreeRxSize
                  0x00a47c                  _MACGetHeader
                  0x00a274                  _MACInit
                  0x00a394                  _MACIsLinked
                  0x00aa12                  _MACIsMemCopyDone
                  0x00a3a8                  _MACIsTxReady
                  0x00a864                  _MACMemCopyAsync
                  0x00aeac                  _MACPowerDown
                  0x00aeda                  _MACPowerUp
                  0x00ab36                  _MACPut
                  0x00ab6e                  _MACPutArray
                  0x00a55e                  _MACPutHeader
                  0x00a72a                  _MACSetReadPtr
                  0x00a6ce                  _MACSetReadPtrInRx
                  0x00a6fc                  _MACSetWritePtr
                  0x00fb9e                  _MD5AddData
                  0x00fe9e                  _MD5Calculate
                  0x00fb62                  _MD5Initialize
                  0x00b132                  _MPFSClose
                  0x00b56a                  _MPFSFormat
                  0x00b154                  _MPFSGet
                  0x00b25a                  _MPFSGetArray
                  0x00b832                  _MPFSGetBytesRem
                  0x00b8ca                  _MPFSGetEndAddr
                  0x00b924                  _MPFSGetFilename
                  0x00b7a0                  _MPFSGetFlags
                  0x00b9ac                  _MPFSGetID
                  0x00b36e                  _MPFSGetLong
                  0x00b752                  _MPFSGetMicrotime
                  0x00b98c                  _MPFSGetPosition
                  0x00b7e4                  _MPFSGetSize
                  0x00b87a                  _MPFSGetStartAddr
                  0x00b704                  _MPFSGetTimestamp
                  0x00af2a                  _MPFSInit
                  0x00af60                  _MPFSOpen
                  0x00b0ae                  _MPFSOpenID
                  0x00b604                  _MPFSPutArray
                  0x00b6a8                  _MPFSPutEnd
                  0x00b38e                  _MPFSSeek
                  0x010cb6                  _NBNSTask
                  0x0134c8                  _PingDemo
                  0x00ad2a                  _ReadPHYReg
                  0x012dba                  _ReadStringUART
                  0x012ed2                  _ReadUART2
                  0x01305c                  _RebootTask
                  0x0093b4                  _SMTPBeginUsage
                  0x0132c8                  _SMTPDemo
                  0x009408                  _SMTPEndUsage
                  0x00a0f8                  _SMTPFlush
                  0x009fb4                  _SMTPIsBusy
                  0x009fca                  _SMTPIsPutReady
                  0x009fe6                  _SMTPPut
                  0x00a086                  _SMTPPutArray
                  0x00a104                  _SMTPPutDone
                  0x00a0c2                  _SMTPPutString
                  0x009fac                  _SMTPSendMail
                  0x009450                  _SMTPTask
                  0x00bfbe                  _SNMPGetNextIndex
                  0x00c016                  _SNMPGetVar
                  0x004048                  _SNMPInit
                  0x004128                  _SNMPIsNotifyReady
                  0x00bdc0                  _SNMPIsValidSetLen
                  0x00416c                  _SNMPNotify
                  0x0040ee                  _SNMPNotifyPrepare
                  0x00bbe8                  _SNMPSendTrap
                  0x00bdfc                  _SNMPSetVar
                  0x00405e                  _SNMPTask
                  0x00bab8                  _SNMPTrapDemo
                  0x00bd1c                  _SNMPValidateCommunity
                  0x011644                  _SNTPClient
                  0x0118b8                  _SNTPGetUTCSeconds
                  0x0108f4                  _SaveAppConfig
                  0x00aefa                  _SetCLKOUT
                  0x0120ba                  _StackApplications
                  0x011e74                  _StackInit
                  0x011eb4                  _StackTask
                  0x00d85a                  _StringToIPAddress
                  0x003e2e                  _TCPAdjustFIFOSize
                  0x002500                  _TCPDiscard
                  0x002266                  _TCPDisconnect
                  0x002692                  _TCPFindArrayEx
                  0x002916                  _TCPFindEx
                  0x002304                  _TCPFlush
                  0x002550                  _TCPGet
                  0x0025ba                  _TCPGetArray
                  0x0022e8                  _TCPGetRemoteInfo
                  0x002676                  _TCPGetRxFIFOFree
                  0x0024e2                  _TCPGetTxFIFOFull
                  0x00201a                  _TCPInit
                  0x00224a                  _TCPIsConnected
                  0x00251e                  _TCPIsGetReady
                  0x002320                  _TCPIsPutReady
                  0x0020e0                  _TCPOpen
                  0x01136a                  _TCPPerformanceTask
                  0x002da2                  _TCPProcess
                  0x00236a                  _TCPPut
                  0x0023f6                  _TCPPutArray
                  0x0024c4                  _TCPPutString
                  0x011532                  _TCPRXPerformanceTask
                  0x001ed4                  _TCPSocketInitializer
                  0x011374                  _TCPTXPerformanceTask
                  0x002934                  _TCPTick
                  0x002226                  _TCPWasReset
                  0x01000a                  _TelnetTask
                  0x01348a                  _TickConvertToMilliseconds
                  0x01344a                  _TickGet
                  0x013456                  _TickGetDiv256
                  0x013470                  _TickGetDiv64K
                  0x0133ce                  _TickInit
                  0x0125c6                  _UART2TCPBridgeInit
                  0x0125dc                  _UART2TCPBridgeTask
                  0x00f1ac                  _UDPClose
                  0x00f43c                  _UDPDiscard
                  0x00f2b6                  _UDPFlush
                  0x00f3bc                  _UDPGet
                  0x00f3f2                  _UDPGetArray
                  0x00f0fa                  _UDPInit
                  0x00f38c                  _UDPIsGetReady
                  0x00f1fe                  _UDPIsPutReady
                  0x00f11e                  _UDPOpen
                  0x00f458                  _UDPProcess
                  0x00f234                  _UDPPut
                  0x00f268                  _UDPPutArray
                  0x00f2a0                  _UDPPutString
                  0x00f1ea                  _UDPSetRxBuffer
                  0x00f1d6                  _UDPSetTxBuffer
                  0x00f114                  _UDPTask
                  0x00ae5c                  _WritePHYReg
                  0x012ef0                  _WriteUART2
                  0x01105a                  _XEEBeginRead
                  0x011180                  _XEEBeginWrite
                  0x0110ac                  _XEEEndRead
                  0x0111f2                  _XEEEndWrite
                  0x01103c                  _XEEInit
                  0x0112fe                  _XEEIsBusy
                  0x01106e                  _XEERead
                  0x0110b4                  _XEEReadArray
                  0x011194                  _XEEWrite
                  0x0111d0                  _XEEWriteArray
                  0x0104a2                  __AddressError
                  0x0136d8                  __DefaultInterrupt
                  0x000586                  __Geterrno
                  0x0104ac                  __StackError
                  0x0002f4                  __Stoul
                  0x0134b0                  __T1Interrupt
                  0x012738                  __U2RXInterrupt
                  0x012776                  __U2TXInterrupt
                  0x00069c                  ___divdi3
                  0x0006d6                  ___moddi3
                  0x0007c8                  ___muldi3
                  0x000868                  ___mulsi3
                  0x000686                  ___udivdi3
                  0x0005b8                  ___udivmoddi3
                  0x0007a8                  ___udivsi3
                  0x000694                  ___umoddi3
                  0x000824                  ___umuldi3
                  0x00022e                  __data_init
                  0x00021e                  __psv_init
                  0x000200                  __resetPRI
                  0x00c68a                  _accept
                  0x00c518                  _bind
                  0x00de40                  _btohexa_high
                  0x00de68                  _btohexa_low
                  0x00cd78                  _closesocket
                  0x00c76c                  _connect
                  0x00cd14                  _gethostname
                  0x012e50                  _getsUART2
                  0x00ddca                  _hexatob
                  0x000554                  _isspace
                  0x00c58c                  _listen
                  0x0104b6                  _main
                  0x000572                  _memchr
                  0x0002a6                  _memcmp
                  0x000522                  _memcpy
                  0x0002e6                  _memset
                  0x012e02                  _putsUART2
                  0x00041c                  _rand
                  0x00cb2e                  _recv
                  0x00cc5a                  _recvfrom
                  0x00c8aa                  _send
                  0x00c9ec                  _sendto
                  0x00c49a                  _socket
                  0x0004c6                  _srand
                  0x0004e8                  _strchr
                  0x0002c2                  _strcmp
                  0x000296                  _strcpy
                  0x00de8e                  _stricmppgm2ram
                  0x000288                  _strlen
                  0x000530                  _strncmp
                  0x0004fa                  _strstr
                  0x00e014                  _strupr
                  0x00df40                  _swapl
                  0x00df26                  _swaps
                  0x000564                  _tolower
                  0x00dc9c                  _uitoa
                  0x00dd1a                  _ultoa

Memory Configuration

Name             Origin             Length             Attributes
data             0x000800           0x002000           a !xr
reset            0x000000           0x000004  
ivt              0x000004           0x0000fc  
aivt             0x000104           0x0000fc  
program          0x000200           0x0155fc           xr
config2          0x0157fc           0x000002  
config1          0x0157fe           0x000002  
*default*        0x000000           0xffffffff  

Linker script and memory map

LOAD Objects - TCPIP Demo App-C30\MainDemo.o
LOAD Objects - TCPIP Demo App-C30\CustomHTTPApp.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Tick.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UART2TCPBridge.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UART.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UDP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UDPPerformanceTest.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Announce.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ARP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Delay.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DHCP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DHCPs.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DNS.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DynDNS.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\FTP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Hashes.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Helpers.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\HTTP2.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\HTTP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ICMP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\IP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\LCDBlocking.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\MPFS2.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\MPFS.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\NBNS.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Reboot.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SMTP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SNMP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SNTP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SPIEEPROM.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SPIFlash.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SPIRAM.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\StackTsk.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCPPerformanceTest.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Telnet.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TFTPc.o
LOAD Objects - TCPIP Demo App-C30\CustomSNMPApp.o
LOAD Objects - TCPIP Demo App-C30\UARTConfig.o
LOAD Objects - TCPIP Demo App-C30\GenericTCPClient.o
LOAD Objects - TCPIP Demo App-C30\GenericTCPServer.o
LOAD Objects - TCPIP Demo App-C30\PingDemo.o
LOAD Objects - TCPIP Demo App-C30\SMTPDemo.o
LOAD Objects - TCPIP Demo App-C30\LegacyHTTPApp.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\BerkeleyAPI.o
LOAD Objects - TCPIP Demo App-C30\BerkeleyUDPClientDemo.o
LOAD Objects - TCPIP Demo App-C30\BerkeleyTCPClientDemo.o
LOAD Objects - TCPIP Demo App-C30\BerkeleyTCPServerDemo.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ENCX24J600.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ENC28J60.o
LOAD Objects - TCPIP Demo App-C30\CustomSSLCert.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SSL.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ARCFOUR.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\BigInt.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Random.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\RSA.o
LOAD C:\Microchip Solutions\Microchip\TCPIP Stack\BigInt_helper_coff.a
LOAD C:\Microchip Solutions\Microchip\TCPIP Stack\BigInt_helper_elf.a
LOAD c:/program files/microchip/mplab c30/bin/bin/../../lib/PIC24F\libpPIC24Fxxx-coff.a
                    0x157fc                  __CONFIG2 = 0x157fc
                    0x157fe                  __CONFIG1 = 0x157fe
                    0x0004                  __IVT_BASE = 0x4
                    0x0104                  __AIVT_BASE = 0x104
                    0x0800                  __DATA_BASE = 0x800
                    0x0200                  __CODE_BASE = 0x200

.reset            0x000000          0x4
                  0x000000          0x2 SHORT 0x200 <code 337> (__reset)
                  0x000001          0x2 SHORT 0x4
                  0x000002          0x2 SHORT 0x0 ((<code 337> (__reset) >> 0x10) & 0x7f)
                  0x000003          0x2 SHORT 0x0

.text             0x000200        0x674
 *(.init)
 .init            0x000200         0x88 c:/program files/microchip/mplab c30/bin/bin/../../lib\libpic30-coff.a(crt0.o)
                  0x000200                  _resetPRI
                  0x000200                  _reset
                  0x00021e                  _psv_init
                  0x00022e                  _data_init
 *(.user_init)
 *(.handle)
 *(.libc)
 .libc            0x000288          0xe c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strlen.o)
                  0x000288                  strlen
 .libc            0x000296         0x10 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strcpy.o)
                  0x000296                  strcpy
 .libc            0x0002a6         0x1c c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memcmp.o)
                  0x0002a6                  memcmp
 .libc            0x0002c2         0x24 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strcmp.o)
                  0x0002c2                  strcmp
 .libc            0x0002e6          0xe c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memset.o)
                  0x0002e6                  memset
 .libc            0x0002f4        0x128 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xstoul.o)
                  0x0002f4                  _Stoul
 .libc            0x00041c         0xaa c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(rand.o)
                  0x00041c                  rand
 .libc            0x0004c6         0x22 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(srand.o)
                  0x0004c6                  srand
 .libc            0x0004e8         0x12 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strchr.o)
                  0x0004e8                  strchr
 .libc            0x0004fa         0x28 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strstr.o)
                  0x0004fa                  strstr
 .libc            0x000522          0xe c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memcpy.o)
                  0x000522                  memcpy
 .libc            0x000530         0x24 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strncmp.o)
                  0x000530                  strncmp
 .libc            0x000554         0x10 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(isspace.os)
                  0x000554                  isspace
 .libc            0x000564          0xe c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(tolower.os)
                  0x000564                  tolower
 .libc            0x000572         0x14 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memchr.o)
                  0x000572                  memchr
 .libc            0x000586          0xc c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(errno.o)
                  0x000586                  _Geterrno
 *(.libm)
 .libm            0x000592        0x216 c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(divmoddi3.o)
                  0x0005b8                  __udivmoddi3
                  0x000686                  __udivdi3
                  0x000694                  __umoddi3
                  0x00069c                  __divdi3
                  0x0006d6                  __moddi3
 .libm            0x0007a8         0x20 c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(udivsi3.o)
                  0x0007a8                  __udivsi3
 .libm            0x0007c8         0x5c c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(muldi3.o)
                  0x0007c8                  __muldi3
 .libm            0x000824         0x44 c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(umuldi3.o)
                  0x000824                  __umuldi3
 .libm            0x000868          0xc c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(mulsi3.o)
                  0x000868                  __mulsi3
 *(.libdsp)
 *(.lib*)

__CONFIG2         0x0157fc          0x2
 *(__CONFIG2.sec)
 __CONFIG2.sec    0x0157fc          0x2 Objects - TCPIP Demo App-C30\MainDemo.o

__CONFIG1         0x0157fe          0x2
 *(__CONFIG1.sec)
 __CONFIG1.sec    0x0157fe          0x2 Objects - TCPIP Demo App-C30\MainDemo.o

.comment
 *(.comment)

.debug_info
 *(.debug_info)
 *(.gnu.linkonce.wi.*)

.debug_abbrev
 *(.debug_abbrev)

.debug_line
 *(.debug_line)

.debug_frame
 *(.debug_frame)

.debug_str
 *(.debug_str)

.debug_loc
 *(.debug_loc)

.debug_macinfo
 *(.debug_macinfo)

.debug_pubnames
 *(.debug_pubnames)

.debug_ranges
 *(.debug_ranges)

.debug_aranges
 *(.debug_aranges)

.ivt              0x000004         0xfc
                  0x000004          0x4 LONG 0x136d8 DEFINED (__ReservedTrap0)?<code 337> (__ReservedTrap0):<code 337> (__DefaultInterrupt)
                  0x000006          0x4 LONG 0x136d8 DEFINED (__OscillatorFail)?<code 337> (__OscillatorFail):<code 337> (__DefaultInterrupt)
                  0x000008          0x4 LONG 0x104a2 DEFINED (__AddressError)?<code 337> (__AddressError):<code 337> (__DefaultInterrupt)
                  0x00000a          0x4 LONG 0x104ac DEFINED (__StackError)?<code 337> (__StackError):<code 337> (__DefaultInterrupt)
                  0x00000c          0x4 LONG 0x136d8 DEFINED (__MathError)?<code 337> (__MathError):<code 337> (__DefaultInterrupt)
                  0x00000e          0x4 LONG 0x136d8 DEFINED (__ReservedTrap5)?<code 337> (__ReservedTrap5):<code 337> (__DefaultInterrupt)
                  0x000010          0x4 LONG 0x136d8 DEFINED (__ReservedTrap6)?<code 337> (__ReservedTrap6):<code 337> (__DefaultInterrupt)
                  0x000012          0x4 LONG 0x136d8 DEFINED (__ReservedTrap7)?<code 337> (__ReservedTrap7):<code 337> (__DefaultInterrupt)
                  0x000014          0x4 LONG 0x136d8 DEFINED (__INT0Interrupt)?<code 337> (__INT0Interrupt):<code 337> (__DefaultInterrupt)
                  0x000016          0x4 LONG 0x136d8 DEFINED (__IC1Interrupt)?<code 337> (__IC1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000018          0x4 LONG 0x136d8 DEFINED (__OC1Interrupt)?<code 337> (__OC1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00001a          0x4 LONG 0x134b0 DEFINED (__T1Interrupt)?<code 337> (__T1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00001c          0x4 LONG 0x136d8 DEFINED (__Interrupt4)?<code 337> (__Interrupt4):<code 337> (__DefaultInterrupt)
                  0x00001e          0x4 LONG 0x136d8 DEFINED (__IC2Interrupt)?<code 337> (__IC2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000020          0x4 LONG 0x136d8 DEFINED (__OC2Interrupt)?<code 337> (__OC2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000022          0x4 LONG 0x136d8 DEFINED (__T2Interrupt)?<code 337> (__T2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000024          0x4 LONG 0x136d8 DEFINED (__T3Interrupt)?<code 337> (__T3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000026          0x4 LONG 0x136d8 DEFINED (__SPI1ErrInterrupt)?<code 337> (__SPI1ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x000028          0x4 LONG 0x136d8 DEFINED (__SPI1Interrupt)?<code 337> (__SPI1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00002a          0x4 LONG 0x136d8 DEFINED (__U1RXInterrupt)?<code 337> (__U1RXInterrupt):<code 337> (__DefaultInterrupt)
                  0x00002c          0x4 LONG 0x136d8 DEFINED (__U1TXInterrupt)?<code 337> (__U1TXInterrupt):<code 337> (__DefaultInterrupt)
                  0x00002e          0x4 LONG 0x136d8 DEFINED (__ADC1Interrupt)?<code 337> (__ADC1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000030          0x4 LONG 0x136d8 DEFINED (__Interrupt14)?<code 337> (__Interrupt14):<code 337> (__DefaultInterrupt)
                  0x000032          0x4 LONG 0x136d8 DEFINED (__Interrupt15)?<code 337> (__Interrupt15):<code 337> (__DefaultInterrupt)
                  0x000034          0x4 LONG 0x136d8 DEFINED (__SI2C1Interrupt)?<code 337> (__SI2C1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000036          0x4 LONG 0x136d8 DEFINED (__MI2C1Interrupt)?<code 337> (__MI2C1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000038          0x4 LONG 0x136d8 DEFINED (__CompInterrupt)?<code 337> (__CompInterrupt):<code 337> (__DefaultInterrupt)
                  0x00003a          0x4 LONG 0x136d8 DEFINED (__CNInterrupt)?<code 337> (__CNInterrupt):<code 337> (__DefaultInterrupt)
                  0x00003c          0x4 LONG 0x136d8 DEFINED (__INT1Interrupt)?<code 337> (__INT1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00003e          0x4 LONG 0x136d8 DEFINED (__Interrupt21)?<code 337> (__Interrupt21):<code 337> (__DefaultInterrupt)
                  0x000040          0x4 LONG 0x136d8 DEFINED (__Interrupt22)?<code 337> (__Interrupt22):<code 337> (__DefaultInterrupt)
                  0x000042          0x4 LONG 0x136d8 DEFINED (__Interrupt23)?<code 337> (__Interrupt23):<code 337> (__DefaultInterrupt)
                  0x000044          0x4 LONG 0x136d8 DEFINED (__Interrupt24)?<code 337> (__Interrupt24):<code 337> (__DefaultInterrupt)
                  0x000046          0x4 LONG 0x136d8 DEFINED (__OC3Interrupt)?<code 337> (__OC3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000048          0x4 LONG 0x136d8 DEFINED (__OC4Interrupt)?<code 337> (__OC4Interrupt):<code 337> (__DefaultInterrupt)
                  0x00004a          0x4 LONG 0x136d8 DEFINED (__T4Interrupt)?<code 337> (__T4Interrupt):<code 337> (__DefaultInterrupt)
                  0x00004c          0x4 LONG 0x136d8 DEFINED (__T5Interrupt)?<code 337> (__T5Interrupt):<code 337> (__DefaultInterrupt)
                  0x00004e          0x4 LONG 0x136d8 DEFINED (__INT2Interrupt)?<code 337> (__INT2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000050          0x4 LONG 0x12738 DEFINED (__U2RXInterrupt)?<code 337> (__U2RXInterrupt):<code 337> (__DefaultInterrupt)
                  0x000052          0x4 LONG 0x12776 DEFINED (__U2TXInterrupt)?<code 337> (__U2TXInterrupt):<code 337> (__DefaultInterrupt)
                  0x000054          0x4 LONG 0x136d8 DEFINED (__SPI2ErrInterrupt)?<code 337> (__SPI2ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x000056          0x4 LONG 0x136d8 DEFINED (__SPI2Interrupt)?<code 337> (__SPI2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000058          0x4 LONG 0x136d8 DEFINED (__Interrupt34)?<code 337> (__Interrupt34):<code 337> (__DefaultInterrupt)
                  0x00005a          0x4 LONG 0x136d8 DEFINED (__Interrupt35)?<code 337> (__Interrupt35):<code 337> (__DefaultInterrupt)
                  0x00005c          0x4 LONG 0x136d8 DEFINED (__Interrupt36)?<code 337> (__Interrupt36):<code 337> (__DefaultInterrupt)
                  0x00005e          0x4 LONG 0x136d8 DEFINED (__IC3Interrupt)?<code 337> (__IC3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000060          0x4 LONG 0x136d8 DEFINED (__IC4Interrupt)?<code 337> (__IC4Interrupt):<code 337> (__DefaultInterrupt)
                  0x000062          0x4 LONG 0x136d8 DEFINED (__IC5Interrupt)?<code 337> (__IC5Interrupt):<code 337> (__DefaultInterrupt)
                  0x000064          0x4 LONG 0x136d8 DEFINED (__Interrupt40)?<code 337> (__Interrupt40):<code 337> (__DefaultInterrupt)
                  0x000066          0x4 LONG 0x136d8 DEFINED (__OC5Interrupt)?<code 337> (__OC5Interrupt):<code 337> (__DefaultInterrupt)
                  0x000068          0x4 LONG 0x136d8 DEFINED (__Interrupt42)?<code 337> (__Interrupt42):<code 337> (__DefaultInterrupt)
                  0x00006a          0x4 LONG 0x136d8 DEFINED (__Interrupt43)?<code 337> (__Interrupt43):<code 337> (__DefaultInterrupt)
                  0x00006c          0x4 LONG 0x136d8 DEFINED (__Interrupt44)?<code 337> (__Interrupt44):<code 337> (__DefaultInterrupt)
                  0x00006e          0x4 LONG 0x136d8 DEFINED (__PMPInterrupt)?<code 337> (__PMPInterrupt):<code 337> (__DefaultInterrupt)
                  0x000070          0x4 LONG 0x136d8 DEFINED (__Interrupt46)?<code 337> (__Interrupt46):<code 337> (__DefaultInterrupt)
                  0x000072          0x4 LONG 0x136d8 DEFINED (__Interrupt47)?<code 337> (__Interrupt47):<code 337> (__DefaultInterrupt)
                  0x000074          0x4 LONG 0x136d8 DEFINED (__Interrupt48)?<code 337> (__Interrupt48):<code 337> (__DefaultInterrupt)
                  0x000076          0x4 LONG 0x136d8 DEFINED (__SI2C2Interrupt)?<code 337> (__SI2C2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000078          0x4 LONG 0x136d8 DEFINED (__MI2C2Interrupt)?<code 337> (__MI2C2Interrupt):<code 337> (__DefaultInterrupt)
                  0x00007a          0x4 LONG 0x136d8 DEFINED (__Interrupt51)?<code 337> (__Interrupt51):<code 337> (__DefaultInterrupt)
                  0x00007c          0x4 LONG 0x136d8 DEFINED (__Interrupt52)?<code 337> (__Interrupt52):<code 337> (__DefaultInterrupt)
                  0x00007e          0x4 LONG 0x136d8 DEFINED (__INT3Interrupt)?<code 337> (__INT3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000080          0x4 LONG 0x136d8 DEFINED (__INT4Interrupt)?<code 337> (__INT4Interrupt):<code 337> (__DefaultInterrupt)
                  0x000082          0x4 LONG 0x136d8 DEFINED (__Interrupt55)?<code 337> (__Interrupt55):<code 337> (__DefaultInterrupt)
                  0x000084          0x4 LONG 0x136d8 DEFINED (__Interrupt56)?<code 337> (__Interrupt56):<code 337> (__DefaultInterrupt)
                  0x000086          0x4 LONG 0x136d8 DEFINED (__Interrupt57)?<code 337> (__Interrupt57):<code 337> (__DefaultInterrupt)
                  0x000088          0x4 LONG 0x136d8 DEFINED (__Interrupt58)?<code 337> (__Interrupt58):<code 337> (__DefaultInterrupt)
                  0x00008a          0x4 LONG 0x136d8 DEFINED (__Interrupt59)?<code 337> (__Interrupt59):<code 337> (__DefaultInterrupt)
                  0x00008c          0x4 LONG 0x136d8 DEFINED (__Interrupt60)?<code 337> (__Interrupt60):<code 337> (__DefaultInterrupt)
                  0x00008e          0x4 LONG 0x136d8 DEFINED (__Interrupt61)?<code 337> (__Interrupt61):<code 337> (__DefaultInterrupt)
                  0x000090          0x4 LONG 0x136d8 DEFINED (__RTCCInterrupt)?<code 337> (__RTCCInterrupt):<code 337> (__DefaultInterrupt)
                  0x000092          0x4 LONG 0x136d8 DEFINED (__Interrupt63)?<code 337> (__Interrupt63):<code 337> (__DefaultInterrupt)
                  0x000094          0x4 LONG 0x136d8 DEFINED (__Interrupt64)?<code 337> (__Interrupt64):<code 337> (__DefaultInterrupt)
                  0x000096          0x4 LONG 0x136d8 DEFINED (__U1ErrInterrupt)?<code 337> (__U1ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x000098          0x4 LONG 0x136d8 DEFINED (__U2ErrInterrupt)?<code 337> (__U2ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x00009a          0x4 LONG 0x136d8 DEFINED (__CRCInterrupt)?<code 337> (__CRCInterrupt):<code 337> (__DefaultInterrupt)
                  0x00009c          0x4 LONG 0x136d8 DEFINED (__Interrupt68)?<code 337> (__Interrupt68):<code 337> (__DefaultInterrupt)
                  0x00009e          0x4 LONG 0x136d8 DEFINED (__Interrupt69)?<code 337> (__Interrupt69):<code 337> (__DefaultInterrupt)
                  0x0000a0          0x4 LONG 0x136d8 DEFINED (__Interrupt70)?<code 337> (__Interrupt70):<code 337> (__DefaultInterrupt)
                  0x0000a2          0x4 LONG 0x136d8 DEFINED (__Interrupt71)?<code 337> (__Interrupt71):<code 337> (__DefaultInterrupt)
                  0x0000a4          0x4 LONG 0x136d8 DEFINED (__Interrupt72)?<code 337> (__Interrupt72):<code 337> (__DefaultInterrupt)
                  0x0000a6          0x4 LONG 0x136d8 DEFINED (__Interrupt73)?<code 337> (__Interrupt73):<code 337> (__DefaultInterrupt)
                  0x0000a8          0x4 LONG 0x136d8 DEFINED (__Interrupt74)?<code 337> (__Interrupt74):<code 337> (__DefaultInterrupt)
                  0x0000aa          0x4 LONG 0x136d8 DEFINED (__Interrupt75)?<code 337> (__Interrupt75):<code 337> (__DefaultInterrupt)
                  0x0000ac          0x4 LONG 0x136d8 DEFINED (__Interrupt76)?<code 337> (__Interrupt76):<code 337> (__DefaultInterrupt)
                  0x0000ae          0x4 LONG 0x136d8 DEFINED (__Interrupt77)?<code 337> (__Interrupt77):<code 337> (__DefaultInterrupt)
                  0x0000b0          0x4 LONG 0x136d8 DEFINED (__Interrupt78)?<code 337> (__Interrupt78):<code 337> (__DefaultInterrupt)
                  0x0000b2          0x4 LONG 0x136d8 DEFINED (__Interrupt79)?<code 337> (__Interrupt79):<code 337> (__DefaultInterrupt)
                  0x0000b4          0x4 LONG 0x136d8 DEFINED (__Interrupt80)?<code 337> (__Interrupt80):<code 337> (__DefaultInterrupt)
                  0x0000b6          0x4 LONG 0x136d8 DEFINED (__Interrupt81)?<code 337> (__Interrupt81):<code 337> (__DefaultInterrupt)
                  0x0000b8          0x4 LONG 0x136d8 DEFINED (__Interrupt82)?<code 337> (__Interrupt82):<code 337> (__DefaultInterrupt)
                  0x0000ba          0x4 LONG 0x136d8 DEFINED (__Interrupt83)?<code 337> (__Interrupt83):<code 337> (__DefaultInterrupt)
                  0x0000bc          0x4 LONG 0x136d8 DEFINED (__Interrupt84)?<code 337> (__Interrupt84):<code 337> (__DefaultInterrupt)
                  0x0000be          0x4 LONG 0x136d8 DEFINED (__Interrupt85)?<code 337> (__Interrupt85):<code 337> (__DefaultInterrupt)
                  0x0000c0          0x4 LONG 0x136d8 DEFINED (__Interrupt86)?<code 337> (__Interrupt86):<code 337> (__DefaultInterrupt)
                  0x0000c2          0x4 LONG 0x136d8 DEFINED (__Interrupt87)?<code 337> (__Interrupt87):<code 337> (__DefaultInterrupt)
                  0x0000c4          0x4 LONG 0x136d8 DEFINED (__Interrupt88)?<code 337> (__Interrupt88):<code 337> (__DefaultInterrupt)
                  0x0000c6          0x4 LONG 0x136d8 DEFINED (__Interrupt89)?<code 337> (__Interrupt89):<code 337> (__DefaultInterrupt)
                  0x0000c8          0x4 LONG 0x136d8 DEFINED (__Interrupt90)?<code 337> (__Interrupt90):<code 337> (__DefaultInterrupt)
                  0x0000ca          0x4 LONG 0x136d8 DEFINED (__Interrupt91)?<code 337> (__Interrupt91):<code 337> (__DefaultInterrupt)
                  0x0000cc          0x4 LONG 0x136d8 DEFINED (__Interrupt92)?<code 337> (__Interrupt92):<code 337> (__DefaultInterrupt)
                  0x0000ce          0x4 LONG 0x136d8 DEFINED (__Interrupt93)?<code 337> (__Interrupt93):<code 337> (__DefaultInterrupt)
                  0x0000d0          0x4 LONG 0x136d8 DEFINED (__Interrupt94)?<code 337> (__Interrupt94):<code 337> (__DefaultInterrupt)
                  0x0000d2          0x4 LONG 0x136d8 DEFINED (__Interrupt95)?<code 337> (__Interrupt95):<code 337> (__DefaultInterrupt)
                  0x0000d4          0x4 LONG 0x136d8 DEFINED (__Interrupt96)?<code 337> (__Interrupt96):<code 337> (__DefaultInterrupt)
                  0x0000d6          0x4 LONG 0x136d8 DEFINED (__Interrupt97)?<code 337> (__Interrupt97):<code 337> (__DefaultInterrupt)
                  0x0000d8          0x4 LONG 0x136d8 DEFINED (__Interrupt98)?<code 337> (__Interrupt98):<code 337> (__DefaultInterrupt)
                  0x0000da          0x4 LONG 0x136d8 DEFINED (__Interrupt99)?<code 337> (__Interrupt99):<code 337> (__DefaultInterrupt)
                  0x0000dc          0x4 LONG 0x136d8 DEFINED (__Interrupt100)?<code 337> (__Interrupt100):<code 337> (__DefaultInterrupt)
                  0x0000de          0x4 LONG 0x136d8 DEFINED (__Interrupt101)?<code 337> (__Interrupt101):<code 337> (__DefaultInterrupt)
                  0x0000e0          0x4 LONG 0x136d8 DEFINED (__Interrupt102)?<code 337> (__Interrupt102):<code 337> (__DefaultInterrupt)
                  0x0000e2          0x4 LONG 0x136d8 DEFINED (__Interrupt103)?<code 337> (__Interrupt103):<code 337> (__DefaultInterrupt)
                  0x0000e4          0x4 LONG 0x136d8 DEFINED (__Interrupt104)?<code 337> (__Interrupt104):<code 337> (__DefaultInterrupt)
                  0x0000e6          0x4 LONG 0x136d8 DEFINED (__Interrupt105)?<code 337> (__Interrupt105):<code 337> (__DefaultInterrupt)
                  0x0000e8          0x4 LONG 0x136d8 DEFINED (__Interrupt106)?<code 337> (__Interrupt106):<code 337> (__DefaultInterrupt)
                  0x0000ea          0x4 LONG 0x136d8 DEFINED (__Interrupt107)?<code 337> (__Interrupt107):<code 337> (__DefaultInterrupt)
                  0x0000ec          0x4 LONG 0x136d8 DEFINED (__Interrupt108)?<code 337> (__Interrupt108):<code 337> (__DefaultInterrupt)
                  0x0000ee          0x4 LONG 0x136d8 DEFINED (__Interrupt109)?<code 337> (__Interrupt109):<code 337> (__DefaultInterrupt)
                  0x0000f0          0x4 LONG 0x136d8 DEFINED (__Interrupt110)?<code 337> (__Interrupt110):<code 337> (__DefaultInterrupt)
                  0x0000f2          0x4 LONG 0x136d8 DEFINED (__Interrupt111)?<code 337> (__Interrupt111):<code 337> (__DefaultInterrupt)
                  0x0000f4          0x4 LONG 0x136d8 DEFINED (__Interrupt112)?<code 337> (__Interrupt112):<code 337> (__DefaultInterrupt)
                  0x0000f6          0x4 LONG 0x136d8 DEFINED (__Interrupt113)?<code 337> (__Interrupt113):<code 337> (__DefaultInterrupt)
                  0x0000f8          0x4 LONG 0x136d8 DEFINED (__Interrupt114)?<code 337> (__Interrupt114):<code 337> (__DefaultInterrupt)
                  0x0000fa          0x4 LONG 0x136d8 DEFINED (__Interrupt115)?<code 337> (__Interrupt115):<code 337> (__DefaultInterrupt)
                  0x0000fc          0x4 LONG 0x136d8 DEFINED (__Interrupt116)?<code 337> (__Interrupt116):<code 337> (__DefaultInterrupt)
                  0x0000fe          0x4 LONG 0x136d8 DEFINED (__Interrupt117)?<code 337> (__Interrupt117):<code 337> (__DefaultInterrupt)

.aivt             0x000104         0xfc
                  0x000104          0x4 LONG 0x136d8 DEFINED (__AltReservedTrap0)?<code 337> (__AltReservedTrap0):DEFINED (__ReservedTrap0)?<code 337> (__ReservedTrap0):<code 337> (__DefaultInterrupt)
                  0x000106          0x4 LONG 0x136d8 DEFINED (__AltOscillatorFail)?<code 337> (__AltOscillatorFail):DEFINED (__OscillatorFail)?<code 337> (__OscillatorFail):<code 337> (__DefaultInterrupt)
                  0x000108          0x4 LONG 0x104a2 DEFINED (__AltAddressError)?<code 337> (__AltAddressError):DEFINED (__AddressError)?<code 337> (__AddressError):<code 337> (__DefaultInterrupt)
                  0x00010a          0x4 LONG 0x104ac DEFINED (__AltStackError)?<code 337> (__AltStackError):DEFINED (__StackError)?<code 337> (__StackError):<code 337> (__DefaultInterrupt)
                  0x00010c          0x4 LONG 0x136d8 DEFINED (__AltMathError)?<code 337> (__AltMathError):DEFINED (__MathError)?<code 337> (__MathError):<code 337> (__DefaultInterrupt)
                  0x00010e          0x4 LONG 0x136d8 DEFINED (__AltReservedTrap5)?<code 337> (__AltReservedTrap5):DEFINED (__ReservedTrap5)?<code 337> (__ReservedTrap5):<code 337> (__DefaultInterrupt)
                  0x000110          0x4 LONG 0x136d8 DEFINED (__AltReservedTrap6)?<code 337> (__AltReservedTrap6):DEFINED (__ReservedTrap6)?<code 337> (__ReservedTrap6):<code 337> (__DefaultInterrupt)
                  0x000112          0x4 LONG 0x136d8 DEFINED (__AltReservedTrap7)?<code 337> (__AltReservedTrap7):DEFINED (__ReservedTrap7)?<code 337> (__ReservedTrap7):<code 337> (__DefaultInterrupt)
                  0x000114          0x4 LONG 0x136d8 DEFINED (__AltINT0Interrupt)?<code 337> (__AltINT0Interrupt):DEFINED (__INT0Interrupt)?<code 337> (__INT0Interrupt):<code 337> (__DefaultInterrupt)
                  0x000116          0x4 LONG 0x136d8 DEFINED (__AltIC1Interrupt)?<code 337> (__AltIC1Interrupt):DEFINED (__IC1Interrupt)?<code 337> (__IC1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000118          0x4 LONG 0x136d8 DEFINED (__AltOC1Interrupt)?<code 337> (__AltOC1Interrupt):DEFINED (__OC1Interrupt)?<code 337> (__OC1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00011a          0x4 LONG 0x134b0 DEFINED (__AltT1Interrupt)?<code 337> (__AltT1Interrupt):DEFINED (__T1Interrupt)?<code 337> (__T1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00011c          0x4 LONG 0x136d8 DEFINED (__AltInterrupt4)?<code 337> (__AltInterrupt4):DEFINED (__Interrupt4)?<code 337> (__Interrupt4):<code 337> (__DefaultInterrupt)
                  0x00011e          0x4 LONG 0x136d8 DEFINED (__AltIC2Interrupt)?<code 337> (__AltIC2Interrupt):DEFINED (__IC2Interrupt)?<code 337> (__IC2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000120          0x4 LONG 0x136d8 DEFINED (__AltOC2Interrupt)?<code 337> (__AltOC2Interrupt):DEFINED (__OC2Interrupt)?<code 337> (__OC2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000122          0x4 LONG 0x136d8 DEFINED (__AltT2Interrupt)?<code 337> (__AltT2Interrupt):DEFINED (__T2Interrupt)?<code 337> (__T2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000124          0x4 LONG 0x136d8 DEFINED (__AltT3Interrupt)?<code 337> (__AltT3Interrupt):DEFINED (__T3Interrupt)?<code 337> (__T3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000126          0x4 LONG 0x136d8 DEFINED (__AltSPI1ErrInterrupt)?<code 337> (__AltSPI1ErrInterrupt):DEFINED (__SPI1ErrInterrupt)?<code 337> (__SPI1ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x000128          0x4 LONG 0x136d8 DEFINED (__AltSPI1Interrupt)?<code 337> (__AltSPI1Interrupt):DEFINED (__SPI1Interrupt)?<code 337> (__SPI1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00012a          0x4 LONG 0x136d8 DEFINED (__AltU1RXInterrupt)?<code 337> (__AltU1RXInterrupt):DEFINED (__U1RXInterrupt)?<code 337> (__U1RXInterrupt):<code 337> (__DefaultInterrupt)
                  0x00012c          0x4 LONG 0x136d8 DEFINED (__AltU1TXInterrupt)?<code 337> (__AltU1TXInterrupt):DEFINED (__U1TXInterrupt)?<code 337> (__U1TXInterrupt):<code 337> (__DefaultInterrupt)
                  0x00012e          0x4 LONG 0x136d8 DEFINED (__AltADC1Interrupt)?<code 337> (__AltADC1Interrupt):DEFINED (__ADC1Interrupt)?<code 337> (__ADC1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000130          0x4 LONG 0x136d8 DEFINED (__AltInterrupt14)?<code 337> (__AltInterrupt14):DEFINED (__Interrupt14)?<code 337> (__Interrupt14):<code 337> (__DefaultInterrupt)
                  0x000132          0x4 LONG 0x136d8 DEFINED (__AltInterrupt15)?<code 337> (__AltInterrupt15):DEFINED (__Interrupt15)?<code 337> (__Interrupt15):<code 337> (__DefaultInterrupt)
                  0x000134          0x4 LONG 0x136d8 DEFINED (__AltSI2C1Interrupt)?<code 337> (__AltSI2C1Interrupt):DEFINED (__SI2C1Interrupt)?<code 337> (__SI2C1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000136          0x4 LONG 0x136d8 DEFINED (__AltMI2C1Interrupt)?<code 337> (__AltMI2C1Interrupt):DEFINED (__MI2C1Interrupt)?<code 337> (__MI2C1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000138          0x4 LONG 0x136d8 DEFINED (__AltCompInterrupt)?<code 337> (__AltCompInterrupt):DEFINED (__CompInterrupt)?<code 337> (__CompInterrupt):<code 337> (__DefaultInterrupt)
                  0x00013a          0x4 LONG 0x136d8 DEFINED (__AltCNInterrupt)?<code 337> (__AltCNInterrupt):DEFINED (__CNInterrupt)?<code 337> (__CNInterrupt):<code 337> (__DefaultInterrupt)
                  0x00013c          0x4 LONG 0x136d8 DEFINED (__AltINT1Interrupt)?<code 337> (__AltINT1Interrupt):DEFINED (__INT1Interrupt)?<code 337> (__INT1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00013e          0x4 LONG 0x136d8 DEFINED (__AltInterrupt21)?<code 337> (__AltInterrupt21):DEFINED (__Interrupt21)?<code 337> (__Interrupt21):<code 337> (__DefaultInterrupt)
                  0x000140          0x4 LONG 0x136d8 DEFINED (__AltInterrupt22)?<code 337> (__AltInterrupt22):DEFINED (__Interrupt22)?<code 337> (__Interrupt22):<code 337> (__DefaultInterrupt)
                  0x000142          0x4 LONG 0x136d8 DEFINED (__AltInterrupt23)?<code 337> (__AltInterrupt23):DEFINED (__Interrupt23)?<code 337> (__Interrupt23):<code 337> (__DefaultInterrupt)
                  0x000144          0x4 LONG 0x136d8 DEFINED (__AltInterrupt24)?<code 337> (__AltInterrupt24):DEFINED (__Interrupt24)?<code 337> (__Interrupt24):<code 337> (__DefaultInterrupt)
                  0x000146          0x4 LONG 0x136d8 DEFINED (__AltOC3Interrupt)?<code 337> (__AltOC3Interrupt):DEFINED (__OC3Interrupt)?<code 337> (__OC3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000148          0x4 LONG 0x136d8 DEFINED (__AltOC4Interrupt)?<code 337> (__AltOC4Interrupt):DEFINED (__OC4Interrupt)?<code 337> (__OC4Interrupt):<code 337> (__DefaultInterrupt)
                  0x00014a          0x4 LONG 0x136d8 DEFINED (__AltT4Interrupt)?<code 337> (__AltT4Interrupt):DEFINED (__T4Interrupt)?<code 337> (__T4Interrupt):<code 337> (__DefaultInterrupt)
                  0x00014c          0x4 LONG 0x136d8 DEFINED (__AltT5Interrupt)?<code 337> (__AltT5Interrupt):DEFINED (__T5Interrupt)?<code 337> (__T5Interrupt):<code 337> (__DefaultInterrupt)
                  0x00014e          0x4 LONG 0x136d8 DEFINED (__AltINT2Interrupt)?<code 337> (__AltINT2Interrupt):DEFINED (__INT2Interrupt)?<code 337> (__INT2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000150          0x4 LONG 0x12738 DEFINED (__AltU2RXInterrupt)?<code 337> (__AltU2RXInterrupt):DEFINED (__U2RXInterrupt)?<code 337> (__U2RXInterrupt):<code 337> (__DefaultInterrupt)
                  0x000152          0x4 LONG 0x12776 DEFINED (__AltU2TXInterrupt)?<code 337> (__AltU2TXInterrupt):DEFINED (__U2TXInterrupt)?<code 337> (__U2TXInterrupt):<code 337> (__DefaultInterrupt)
                  0x000154          0x4 LONG 0x136d8 DEFINED (__AltSPI2ErrInterrupt)?<code 337> (__AltSPI2ErrInterrupt):DEFINED (__SPI2ErrInterrupt)?<code 337> (__SPI2ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x000156          0x4 LONG 0x136d8 DEFINED (__AltSPI2Interrupt)?<code 337> (__AltSPI2Interrupt):DEFINED (__SPI2Interrupt)?<code 337> (__SPI2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000158          0x4 LONG 0x136d8 DEFINED (__AltInterrupt34)?<code 337> (__AltInterrupt34):DEFINED (__Interrupt34)?<code 337> (__Interrupt34):<code 337> (__DefaultInterrupt)
                  0x00015a          0x4 LONG 0x136d8 DEFINED (__AltInterrupt35)?<code 337> (__AltInterrupt35):DEFINED (__Interrupt35)?<code 337> (__Interrupt35):<code 337> (__DefaultInterrupt)
                  0x00015c          0x4 LONG 0x136d8 DEFINED (__AltInterrupt36)?<code 337> (__AltInterrupt36):DEFINED (__Interrupt36)?<code 337> (__Interrupt36):<code 337> (__DefaultInterrupt)
                  0x00015e          0x4 LONG 0x136d8 DEFINED (__AltIC3Interrupt)?<code 337> (__AltIC3Interrupt):DEFINED (__IC3Interrupt)?<code 337> (__IC3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000160          0x4 LONG 0x136d8 DEFINED (__AltIC4Interrupt)?<code 337> (__AltIC4Interrupt):DEFINED (__IC4Interrupt)?<code 337> (__IC4Interrupt):<code 337> (__DefaultInterrupt)
                  0x000162          0x4 LONG 0x136d8 DEFINED (__AltIC5Interrupt)?<code 337> (__AltIC5Interrupt):DEFINED (__IC5Interrupt)?<code 337> (__IC5Interrupt):<code 337> (__DefaultInterrupt)
                  0x000164          0x4 LONG 0x136d8 DEFINED (__AltInterrupt40)?<code 337> (__AltInterrupt40):DEFINED (__Interrupt40)?<code 337> (__Interrupt40):<code 337> (__DefaultInterrupt)
                  0x000166          0x4 LONG 0x136d8 DEFINED (__AltOC5Interrupt)?<code 337> (__AltOC5Interrupt):DEFINED (__OC5Interrupt)?<code 337> (__OC5Interrupt):<code 337> (__DefaultInterrupt)
                  0x000168          0x4 LONG 0x136d8 DEFINED (__AltInterrupt42)?<code 337> (__AltInterrupt42):DEFINED (__Interrupt42)?<code 337> (__Interrupt42):<code 337> (__DefaultInterrupt)
                  0x00016a          0x4 LONG 0x136d8 DEFINED (__AltInterrupt43)?<code 337> (__AltInterrupt43):DEFINED (__Interrupt43)?<code 337> (__Interrupt43):<code 337> (__DefaultInterrupt)
                  0x00016c          0x4 LONG 0x136d8 DEFINED (__AltInterrupt44)?<code 337> (__AltInterrupt44):DEFINED (__Interrupt44)?<code 337> (__Interrupt44):<code 337> (__DefaultInterrupt)
                  0x00016e          0x4 LONG 0x136d8 DEFINED (__AltPMPInterrupt)?<code 337> (__AltPMPInterrupt):DEFINED (__PMPInterrupt)?<code 337> (__PMPInterrupt):<code 337> (__DefaultInterrupt)
                  0x000170          0x4 LONG 0x136d8 DEFINED (__AltInterrupt46)?<code 337> (__AltInterrupt46):DEFINED (__Interrupt46)?<code 337> (__Interrupt46):<code 337> (__DefaultInterrupt)
                  0x000172          0x4 LONG 0x136d8 DEFINED (__AltInterrupt47)?<code 337> (__AltInterrupt47):DEFINED (__Interrupt47)?<code 337> (__Interrupt47):<code 337> (__DefaultInterrupt)
                  0x000174          0x4 LONG 0x136d8 DEFINED (__AltInterrupt48)?<code 337> (__AltInterrupt48):DEFINED (__Interrupt48)?<code 337> (__Interrupt48):<code 337> (__DefaultInterrupt)
                  0x000176          0x4 LONG 0x136d8 DEFINED (__AltSI2C2Interrupt)?<code 337> (__AltSI2C2Interrupt):DEFINED (__SI2C2Interrupt)?<code 337> (__SI2C2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000178          0x4 LONG 0x136d8 DEFINED (__AltMI2C2Interrupt)?<code 337> (__AltMI2C2Interrupt):DEFINED (__MI2C2Interrupt)?<code 337> (__MI2C2Interrupt):<code 337> (__DefaultInterrupt)
                  0x00017a          0x4 LONG 0x136d8 DEFINED (__AltInterrupt51)?<code 337> (__AltInterrupt51):DEFINED (__Interrupt51)?<code 337> (__Interrupt51):<code 337> (__DefaultInterrupt)
                  0x00017c          0x4 LONG 0x136d8 DEFINED (__AltInterrupt52)?<code 337> (__AltInterrupt52):DEFINED (__Interrupt52)?<code 337> (__Interrupt52):<code 337> (__DefaultInterrupt)
                  0x00017e          0x4 LONG 0x136d8 DEFINED (__AltINT3Interrupt)?<code 337> (__AltINT3Interrupt):DEFINED (__INT3Interrupt)?<code 337> (__INT3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000180          0x4 LONG 0x136d8 DEFINED (__AltINT4Interrupt)?<code 337> (__AltINT4Interrupt):DEFINED (__INT4Interrupt)?<code 337> (__INT4Interrupt):<code 337> (__DefaultInterrupt)
                  0x000182          0x4 LONG 0x136d8 DEFINED (__AltInterrupt55)?<code 337> (__AltInterrupt55):DEFINED (__Interrupt55)?<code 337> (__Interrupt55):<code 337> (__DefaultInterrupt)
                  0x000184          0x4 LONG 0x136d8 DEFINED (__AltInterrupt56)?<code 337> (__AltInterrupt56):DEFINED (__Interrupt56)?<code 337> (__Interrupt56):<code 337> (__DefaultInterrupt)
                  0x000186          0x4 LONG 0x136d8 DEFINED (__AltInterrupt57)?<code 337> (__AltInterrupt57):DEFINED (__Interrupt57)?<code 337> (__Interrupt57):<code 337> (__DefaultInterrupt)
                  0x000188          0x4 LONG 0x136d8 DEFINED (__AltInterrupt58)?<code 337> (__AltInterrupt58):DEFINED (__Interrupt58)?<code 337> (__Interrupt58):<code 337> (__DefaultInterrupt)
                  0x00018a          0x4 LONG 0x136d8 DEFINED (__AltInterrupt59)?<code 337> (__AltInterrupt59):DEFINED (__Interrupt59)?<code 337> (__Interrupt59):<code 337> (__DefaultInterrupt)
                  0x00018c          0x4 LONG 0x136d8 DEFINED (__AltInterrupt60)?<code 337> (__AltInterrupt60):DEFINED (__Interrupt60)?<code 337> (__Interrupt60):<code 337> (__DefaultInterrupt)
                  0x00018e          0x4 LONG 0x136d8 DEFINED (__AltInterrupt61)?<code 337> (__AltInterrupt61):DEFINED (__Interrupt61)?<code 337> (__Interrupt61):<code 337> (__DefaultInterrupt)
                  0x000190          0x4 LONG 0x136d8 DEFINED (__AltRTCCInterrupt)?<code 337> (__AltRTCCInterrupt):DEFINED (__RTCCInterrupt)?<code 337> (__RTCCInterrupt):<code 337> (__DefaultInterrupt)
                  0x000192          0x4 LONG 0x136d8 DEFINED (__AltInterrupt63)?<code 337> (__AltInterrupt63):DEFINED (__Interrupt63)?<code 337> (__Interrupt63):<code 337> (__DefaultInterrupt)
                  0x000194          0x4 LONG 0x136d8 DEFINED (__AltInterrupt64)?<code 337> (__AltInterrupt64):DEFINED (__Interrupt64)?<code 337> (__Interrupt64):<code 337> (__DefaultInterrupt)
                  0x000196          0x4 LONG 0x136d8 DEFINED (__AltU1ErrInterrupt)?<code 337> (__AltU1ErrInterrupt):DEFINED (__U1ErrInterrupt)?<code 337> (__U1ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x000198          0x4 LONG 0x136d8 DEFINED (__AltU2ErrInterrupt)?<code 337> (__AltU2ErrInterrupt):DEFINED (__U2ErrInterrupt)?<code 337> (__U2ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x00019a          0x4 LONG 0x136d8 DEFINED (__AltCRCInterrupt)?<code 337> (__AltCRCInterrupt):DEFINED (__CRCInterrupt)?<code 337> (__CRCInterrupt):<code 337> (__DefaultInterrupt)
                  0x00019c          0x4 LONG 0x136d8 DEFINED (__AltInterrupt68)?<code 337> (__AltInterrupt68):DEFINED (__Interrupt68)?<code 337> (__Interrupt68):<code 337> (__DefaultInterrupt)
                  0x00019e          0x4 LONG 0x136d8 DEFINED (__AltInterrupt69)?<code 337> (__AltInterrupt69):DEFINED (__Interrupt69)?<code 337> (__Interrupt69):<code 337> (__DefaultInterrupt)
                  0x0001a0          0x4 LONG 0x136d8 DEFINED (__AltInterrupt70)?<code 337> (__AltInterrupt70):DEFINED (__Interrupt70)?<code 337> (__Interrupt70):<code 337> (__DefaultInterrupt)
                  0x0001a2          0x4 LONG 0x136d8 DEFINED (__AltInterrupt71)?<code 337> (__AltInterrupt71):DEFINED (__Interrupt71)?<code 337> (__Interrupt71):<code 337> (__DefaultInterrupt)
                  0x0001a4          0x4 LONG 0x136d8 DEFINED (__AltInterrupt72)?<code 337> (__AltInterrupt72):DEFINED (__Interrupt72)?<code 337> (__Interrupt72):<code 337> (__DefaultInterrupt)
                  0x0001a6          0x4 LONG 0x136d8 DEFINED (__AltInterrupt73)?<code 337> (__AltInterrupt73):DEFINED (__Interrupt73)?<code 337> (__Interrupt73):<code 337> (__DefaultInterrupt)
                  0x0001a8          0x4 LONG 0x136d8 DEFINED (__AltInterrupt74)?<code 337> (__AltInterrupt74):DEFINED (__Interrupt74)?<code 337> (__Interrupt74):<code 337> (__DefaultInterrupt)
                  0x0001aa          0x4 LONG 0x136d8 DEFINED (__AltInterrupt75)?<code 337> (__AltInterrupt75):DEFINED (__Interrupt75)?<code 337> (__Interrupt75):<code 337> (__DefaultInterrupt)
                  0x0001ac          0x4 LONG 0x136d8 DEFINED (__AltInterrupt76)?<code 337> (__AltInterrupt76):DEFINED (__Interrupt76)?<code 337> (__Interrupt76):<code 337> (__DefaultInterrupt)
                  0x0001ae          0x4 LONG 0x136d8 DEFINED (__AltInterrupt77)?<code 337> (__AltInterrupt77):DEFINED (__Interrupt77)?<code 337> (__Interrupt77):<code 337> (__DefaultInterrupt)
                  0x0001b0          0x4 LONG 0x136d8 DEFINED (__AltInterrupt78)?<code 337> (__AltInterrupt78):DEFINED (__Interrupt78)?<code 337> (__Interrupt78):<code 337> (__DefaultInterrupt)
                  0x0001b2          0x4 LONG 0x136d8 DEFINED (__AltInterrupt79)?<code 337> (__AltInterrupt79):DEFINED (__Interrupt79)?<code 337> (__Interrupt79):<code 337> (__DefaultInterrupt)
                  0x0001b4          0x4 LONG 0x136d8 DEFINED (__AltInterrupt80)?<code 337> (__AltInterrupt80):DEFINED (__Interrupt80)?<code 337> (__Interrupt80):<code 337> (__DefaultInterrupt)
                  0x0001b6          0x4 LONG 0x136d8 DEFINED (__AltInterrupt81)?<code 337> (__AltInterrupt81):DEFINED (__Interrupt81)?<code 337> (__Interrupt81):<code 337> (__DefaultInterrupt)
                  0x0001b8          0x4 LONG 0x136d8 DEFINED (__AltInterrupt82)?<code 337> (__AltInterrupt82):DEFINED (__Interrupt82)?<code 337> (__Interrupt82):<code 337> (__DefaultInterrupt)
                  0x0001ba          0x4 LONG 0x136d8 DEFINED (__AltInterrupt83)?<code 337> (__AltInterrupt83):DEFINED (__Interrupt83)?<code 337> (__Interrupt83):<code 337> (__DefaultInterrupt)
                  0x0001bc          0x4 LONG 0x136d8 DEFINED (__AltInterrupt84)?<code 337> (__AltInterrupt84):DEFINED (__Interrupt84)?<code 337> (__Interrupt84):<code 337> (__DefaultInterrupt)
                  0x0001be          0x4 LONG 0x136d8 DEFINED (__AltInterrupt85)?<code 337> (__AltInterrupt85):DEFINED (__Interrupt85)?<code 337> (__Interrupt85):<code 337> (__DefaultInterrupt)
                  0x0001c0          0x4 LONG 0x136d8 DEFINED (__AltInterrupt86)?<code 337> (__AltInterrupt86):DEFINED (__Interrupt86)?<code 337> (__Interrupt86):<code 337> (__DefaultInterrupt)
                  0x0001c2          0x4 LONG 0x136d8 DEFINED (__AltInterrupt87)?<code 337> (__AltInterrupt87):DEFINED (__Interrupt87)?<code 337> (__Interrupt87):<code 337> (__DefaultInterrupt)
                  0x0001c4          0x4 LONG 0x136d8 DEFINED (__AltInterrupt88)?<code 337> (__AltInterrupt88):DEFINED (__Interrupt88)?<code 337> (__Interrupt88):<code 337> (__DefaultInterrupt)
                  0x0001c6          0x4 LONG 0x136d8 DEFINED (__AltInterrupt89)?<code 337> (__AltInterrupt89):DEFINED (__Interrupt89)?<code 337> (__Interrupt89):<code 337> (__DefaultInterrupt)
                  0x0001c8          0x4 LONG 0x136d8 DEFINED (__AltInterrupt90)?<code 337> (__AltInterrupt90):DEFINED (__Interrupt90)?<code 337> (__Interrupt90):<code 337> (__DefaultInterrupt)
                  0x0001ca          0x4 LONG 0x136d8 DEFINED (__AltInterrupt91)?<code 337> (__AltInterrupt91):DEFINED (__Interrupt91)?<code 337> (__Interrupt91):<code 337> (__DefaultInterrupt)
                  0x0001cc          0x4 LONG 0x136d8 DEFINED (__AltInterrupt92)?<code 337> (__AltInterrupt92):DEFINED (__Interrupt92)?<code 337> (__Interrupt92):<code 337> (__DefaultInterrupt)
                  0x0001ce          0x4 LONG 0x136d8 DEFINED (__AltInterrupt93)?<code 337> (__AltInterrupt93):DEFINED (__Interrupt93)?<code 337> (__Interrupt93):<code 337> (__DefaultInterrupt)
                  0x0001d0          0x4 LONG 0x136d8 DEFINED (__AltInterrupt94)?<code 337> (__AltInterrupt94):DEFINED (__Interrupt94)?<code 337> (__Interrupt94):<code 337> (__DefaultInterrupt)
                  0x0001d2          0x4 LONG 0x136d8 DEFINED (__AltInterrupt95)?<code 337> (__AltInterrupt95):DEFINED (__Interrupt95)?<code 337> (__Interrupt95):<code 337> (__DefaultInterrupt)
                  0x0001d4          0x4 LONG 0x136d8 DEFINED (__AltInterrupt96)?<code 337> (__AltInterrupt96):DEFINED (__Interrupt96)?<code 337> (__Interrupt96):<code 337> (__DefaultInterrupt)
                  0x0001d6          0x4 LONG 0x136d8 DEFINED (__AltInterrupt97)?<code 337> (__AltInterrupt97):DEFINED (__Interrupt97)?<code 337> (__Interrupt97):<code 337> (__DefaultInterrupt)
                  0x0001d8          0x4 LONG 0x136d8 DEFINED (__AltInterrupt98)?<code 337> (__AltInterrupt98):DEFINED (__Interrupt98)?<code 337> (__Interrupt98):<code 337> (__DefaultInterrupt)
                  0x0001da          0x4 LONG 0x136d8 DEFINED (__AltInterrupt99)?<code 337> (__AltInterrupt99):DEFINED (__Interrupt99)?<code 337> (__Interrupt99):<code 337> (__DefaultInterrupt)
                  0x0001dc          0x4 LONG 0x136d8 DEFINED (__AltInterrupt100)?<code 337> (__AltInterrupt100):DEFINED (__Interrupt100)?<code 337> (__Interrupt100):<code 337> (__DefaultInterrupt)
                  0x0001de          0x4 LONG 0x136d8 DEFINED (__AltInterrupt101)?<code 337> (__AltInterrupt101):DEFINED (__Interrupt101)?<code 337> (__Interrupt101):<code 337> (__DefaultInterrupt)
                  0x0001e0          0x4 LONG 0x136d8 DEFINED (__AltInterrupt102)?<code 337> (__AltInterrupt102):DEFINED (__Interrupt102)?<code 337> (__Interrupt102):<code 337> (__DefaultInterrupt)
                  0x0001e2          0x4 LONG 0x136d8 DEFINED (__AltInterrupt103)?<code 337> (__AltInterrupt103):DEFINED (__Interrupt103)?<code 337> (__Interrupt103):<code 337> (__DefaultInterrupt)
                  0x0001e4          0x4 LONG 0x136d8 DEFINED (__AltInterrupt104)?<code 337> (__AltInterrupt104):DEFINED (__Interrupt104)?<code 337> (__Interrupt104):<code 337> (__DefaultInterrupt)
                  0x0001e6          0x4 LONG 0x136d8 DEFINED (__AltInterrupt105)?<code 337> (__AltInterrupt105):DEFINED (__Interrupt105)?<code 337> (__Interrupt105):<code 337> (__DefaultInterrupt)
                  0x0001e8          0x4 LONG 0x136d8 DEFINED (__AltInterrupt106)?<code 337> (__AltInterrupt106):DEFINED (__Interrupt106)?<code 337> (__Interrupt106):<code 337> (__DefaultInterrupt)
                  0x0001ea          0x4 LONG 0x136d8 DEFINED (__AltInterrupt107)?<code 337> (__AltInterrupt107):DEFINED (__Interrupt107)?<code 337> (__Interrupt107):<code 337> (__DefaultInterrupt)
                  0x0001ec          0x4 LONG 0x136d8 DEFINED (__AltInterrupt108)?<code 337> (__AltInterrupt108):DEFINED (__Interrupt108)?<code 337> (__Interrupt108):<code 337> (__DefaultInterrupt)
                  0x0001ee          0x4 LONG 0x136d8 DEFINED (__AltInterrupt109)?<code 337> (__AltInterrupt109):DEFINED (__Interrupt109)?<code 337> (__Interrupt109):<code 337> (__DefaultInterrupt)
                  0x0001f0          0x4 LONG 0x136d8 DEFINED (__AltInterrupt110)?<code 337> (__AltInterrupt110):DEFINED (__Interrupt110)?<code 337> (__Interrupt110):<code 337> (__DefaultInterrupt)
                  0x0001f2          0x4 LONG 0x136d8 DEFINED (__AltInterrupt111)?<code 337> (__AltInterrupt111):DEFINED (__Interrupt111)?<code 337> (__Interrupt111):<code 337> (__DefaultInterrupt)
                  0x0001f4          0x4 LONG 0x136d8 DEFINED (__AltInterrupt112)?<code 337> (__AltInterrupt112):DEFINED (__Interrupt112)?<code 337> (__Interrupt112):<code 337> (__DefaultInterrupt)
                  0x0001f6          0x4 LONG 0x136d8 DEFINED (__AltInterrupt113)?<code 337> (__AltInterrupt113):DEFINED (__Interrupt113)?<code 337> (__Interrupt113):<code 337> (__DefaultInterrupt)
                  0x0001f8          0x4 LONG 0x136d8 DEFINED (__AltInterrupt114)?<code 337> (__AltInterrupt114):DEFINED (__Interrupt114)?<code 337> (__Interrupt114):<code 337> (__DefaultInterrupt)
                  0x0001fa          0x4 LONG 0x136d8 DEFINED (__AltInterrupt115)?<code 337> (__AltInterrupt115):DEFINED (__Interrupt115)?<code 337> (__Interrupt115):<code 337> (__DefaultInterrupt)
                  0x0001fc          0x4 LONG 0x136d8 DEFINED (__AltInterrupt116)?<code 337> (__AltInterrupt116):DEFINED (__Interrupt116)?<code 337> (__Interrupt116):<code 337> (__DefaultInterrupt)
                  0x0001fe          0x4 LONG 0x136d8 DEFINED (__AltInterrupt117)?<code 337> (__AltInterrupt117):DEFINED (__Interrupt117)?<code 337> (__Interrupt117):<code 337> (__DefaultInterrupt)
                    0x0000                  WREG0 = 0x0
                    0x0000                  _WREG0 = 0x0
                    0x0002                  WREG1 = 0x2
                    0x0002                  _WREG1 = 0x2
                    0x0004                  WREG2 = 0x4
                    0x0004                  _WREG2 = 0x4
                    0x0006                  WREG3 = 0x6
                    0x0006                  _WREG3 = 0x6
                    0x0008                  WREG4 = 0x8
                    0x0008                  _WREG4 = 0x8
                    0x000a                  WREG5 = 0xa
                    0x000a                  _WREG5 = 0xa
                    0x000c                  WREG6 = 0xc
                    0x000c                  _WREG6 = 0xc
                    0x000e                  WREG7 = 0xe
                    0x000e                  _WREG7 = 0xe
                    0x0010                  WREG8 = 0x10
                    0x0010                  _WREG8 = 0x10
                    0x0012                  WREG9 = 0x12
                    0x0012                  _WREG9 = 0x12
                    0x0014                  WREG10 = 0x14
                    0x0014                  _WREG10 = 0x14
                    0x0016                  WREG11 = 0x16
                    0x0016                  _WREG11 = 0x16
                    0x0018                  WREG12 = 0x18
                    0x0018                  _WREG12 = 0x18
                    0x001a                  WREG13 = 0x1a
                    0x001a                  _WREG13 = 0x1a
                    0x001c                  WREG14 = 0x1c
                    0x001c                  _WREG14 = 0x1c
                    0x001e                  WREG15 = 0x1e
                    0x001e                  _WREG15 = 0x1e
                    0x0020                  SPLIM = 0x20
                    0x0020                  _SPLIM = 0x20
                    0x002e                  PCL = 0x2e
                    0x002e                  _PCL = 0x2e
                    0x0030                  PCH = 0x30
                    0x0030                  _PCH = 0x30
                    0x0032                  TBLPAG = 0x32
                    0x0032                  _TBLPAG = 0x32
                    0x0034                  PSVPAG = 0x34
                    0x0034                  _PSVPAG = 0x34
                    0x0036                  RCOUNT = 0x36
                    0x0036                  _RCOUNT = 0x36
                    0x0042                  SR = 0x42
                    0x0042                  _SR = 0x42
                    0x0042                  _SRbits = 0x42
                    0x0044                  CORCON = 0x44
                    0x0044                  _CORCON = 0x44
                    0x0044                  _CORCONbits = 0x44
                    0x0052                  DISICNT = 0x52
                    0x0052                  _DISICNT = 0x52
                    0x0060                  CNEN1 = 0x60
                    0x0060                  _CNEN1 = 0x60
                    0x0060                  _CNEN1bits = 0x60
                    0x0062                  CNEN2 = 0x62
                    0x0062                  _CNEN2 = 0x62
                    0x0062                  _CNEN2bits = 0x62
                    0x0068                  CNPU1 = 0x68
                    0x0068                  _CNPU1 = 0x68
                    0x0068                  _CNPU1bits = 0x68
                    0x006a                  CNPU2 = 0x6a
                    0x006a                  _CNPU2 = 0x6a
                    0x006a                  _CNPU2bits = 0x6a
                    0x0080                  INTCON1 = 0x80
                    0x0080                  _INTCON1 = 0x80
                    0x0080                  _INTCON1bits = 0x80
                    0x0082                  INTCON2 = 0x82
                    0x0082                  _INTCON2 = 0x82
                    0x0082                  _INTCON2bits = 0x82
                    0x0084                  IFS0 = 0x84
                    0x0084                  _IFS0 = 0x84
                    0x0084                  _IFS0bits = 0x84
                    0x0086                  IFS1 = 0x86
                    0x0086                  _IFS1 = 0x86
                    0x0086                  _IFS1bits = 0x86
                    0x0088                  IFS2 = 0x88
                    0x0088                  _IFS2 = 0x88
                    0x0088                  _IFS2bits = 0x88
                    0x008a                  IFS3 = 0x8a
                    0x008a                  _IFS3 = 0x8a
                    0x008a                  _IFS3bits = 0x8a
                    0x008c                  IFS4 = 0x8c
                    0x008c                  _IFS4 = 0x8c
                    0x008c                  _IFS4bits = 0x8c
                    0x0094                  IEC0 = 0x94
                    0x0094                  _IEC0 = 0x94
                    0x0094                  _IEC0bits = 0x94
                    0x0096                  IEC1 = 0x96
                    0x0096                  _IEC1 = 0x96
                    0x0096                  _IEC1bits = 0x96
                    0x0098                  IEC2 = 0x98
                    0x0098                  _IEC2 = 0x98
                    0x0098                  _IEC2bits = 0x98
                    0x009a                  IEC3 = 0x9a
                    0x009a                  _IEC3 = 0x9a
                    0x009a                  _IEC3bits = 0x9a
                    0x009c                  IEC4 = 0x9c
                    0x009c                  _IEC4 = 0x9c
                    0x009c                  _IEC4bits = 0x9c
                    0x00a4                  IPC0 = 0xa4
                    0x00a4                  _IPC0 = 0xa4
                    0x00a4                  _IPC0bits = 0xa4
                    0x00a6                  IPC1 = 0xa6
                    0x00a6                  _IPC1 = 0xa6
                    0x00a6                  _IPC1bits = 0xa6
                    0x00a8                  IPC2 = 0xa8
                    0x00a8                  _IPC2 = 0xa8
                    0x00a8                  _IPC2bits = 0xa8
                    0x00aa                  IPC3 = 0xaa
                    0x00aa                  _IPC3 = 0xaa
                    0x00aa                  _IPC3bits = 0xaa
                    0x00ac                  IPC4 = 0xac
                    0x00ac                  _IPC4 = 0xac
                    0x00ac                  _IPC4bits = 0xac
                    0x00ae                  IPC5 = 0xae
                    0x00ae                  _IPC5 = 0xae
                    0x00ae                  _IPC5bits = 0xae
                    0x00b0                  IPC6 = 0xb0
                    0x00b0                  _IPC6 = 0xb0
                    0x00b0                  _IPC6bits = 0xb0
                    0x00b2                  IPC7 = 0xb2
                    0x00b2                  _IPC7 = 0xb2
                    0x00b2                  _IPC7bits = 0xb2
                    0x00b4                  IPC8 = 0xb4
                    0x00b4                  _IPC8 = 0xb4
                    0x00b4                  _IPC8bits = 0xb4
                    0x00b6                  IPC9 = 0xb6
                    0x00b6                  _IPC9 = 0xb6
                    0x00b6                  _IPC9bits = 0xb6
                    0x00b8                  IPC10 = 0xb8
                    0x00b8                  _IPC10 = 0xb8
                    0x00b8                  _IPC10bits = 0xb8
                    0x00ba                  IPC11 = 0xba
                    0x00ba                  _IPC11 = 0xba
                    0x00ba                  _IPC11bits = 0xba
                    0x00bc                  IPC12 = 0xbc
                    0x00bc                  _IPC12 = 0xbc
                    0x00bc                  _IPC12bits = 0xbc
                    0x00be                  IPC13 = 0xbe
                    0x00be                  _IPC13 = 0xbe
                    0x00be                  _IPC13bits = 0xbe
                    0x00c2                  IPC15 = 0xc2
                    0x00c2                  _IPC15 = 0xc2
                    0x00c2                  _IPC15bits = 0xc2
                    0x00c4                  IPC16 = 0xc4
                    0x00c4                  _IPC16 = 0xc4
                    0x00c4                  _IPC16bits = 0xc4
                    0x0100                  TMR1 = 0x100
                    0x0100                  _TMR1 = 0x100
                    0x0102                  PR1 = 0x102
                    0x0102                  _PR1 = 0x102
                    0x0104                  T1CON = 0x104
                    0x0104                  _T1CON = 0x104
                    0x0104                  _T1CONbits = 0x104
                    0x0106                  TMR2 = 0x106
                    0x0106                  _TMR2 = 0x106
                    0x0108                  TMR3HLD = 0x108
                    0x0108                  _TMR3HLD = 0x108
                    0x010a                  TMR3 = 0x10a
                    0x010a                  _TMR3 = 0x10a
                    0x010c                  PR2 = 0x10c
                    0x010c                  _PR2 = 0x10c
                    0x010e                  PR3 = 0x10e
                    0x010e                  _PR3 = 0x10e
                    0x0110                  T2CON = 0x110
                    0x0110                  _T2CON = 0x110
                    0x0110                  _T2CONbits = 0x110
                    0x0112                  T3CON = 0x112
                    0x0112                  _T3CON = 0x112
                    0x0112                  _T3CONbits = 0x112
                    0x0114                  TMR4 = 0x114
                    0x0114                  _TMR4 = 0x114
                    0x0116                  TMR5HLD = 0x116
                    0x0116                  _TMR5HLD = 0x116
                    0x0118                  TMR5 = 0x118
                    0x0118                  _TMR5 = 0x118
                    0x011a                  PR4 = 0x11a
                    0x011a                  _PR4 = 0x11a
                    0x011c                  PR5 = 0x11c
                    0x011c                  _PR5 = 0x11c
                    0x011e                  T4CON = 0x11e
                    0x011e                  _T4CON = 0x11e
                    0x011e                  _T4CONbits = 0x11e
                    0x0120                  T5CON = 0x120
                    0x0120                  _T5CON = 0x120
                    0x0120                  _T5CONbits = 0x120
                    0x0140                  IC1BUF = 0x140
                    0x0140                  _IC1BUF = 0x140
                    0x0142                  IC1CON = 0x142
                    0x0142                  _IC1CON = 0x142
                    0x0142                  _IC1CONbits = 0x142
                    0x0144                  IC2BUF = 0x144
                    0x0144                  _IC2BUF = 0x144
                    0x0146                  IC2CON = 0x146
                    0x0146                  _IC2CON = 0x146
                    0x0146                  _IC2CONbits = 0x146
                    0x0148                  IC3BUF = 0x148
                    0x0148                  _IC3BUF = 0x148
                    0x014a                  IC3CON = 0x14a
                    0x014a                  _IC3CON = 0x14a
                    0x014a                  _IC3CONbits = 0x14a
                    0x014c                  IC4BUF = 0x14c
                    0x014c                  _IC4BUF = 0x14c
                    0x014e                  IC4CON = 0x14e
                    0x014e                  _IC4CON = 0x14e
                    0x014e                  _IC4CONbits = 0x14e
                    0x0150                  IC5BUF = 0x150
                    0x0150                  _IC5BUF = 0x150
                    0x0152                  IC5CON = 0x152
                    0x0152                  _IC5CON = 0x152
                    0x0152                  _IC5CONbits = 0x152
                    0x0180                  OC1RS = 0x180
                    0x0180                  _OC1RS = 0x180
                    0x0182                  OC1R = 0x182
                    0x0182                  _OC1R = 0x182
                    0x0184                  OC1CON = 0x184
                    0x0184                  _OC1CON = 0x184
                    0x0184                  _OC1CONbits = 0x184
                    0x0186                  OC2RS = 0x186
                    0x0186                  _OC2RS = 0x186
                    0x0188                  OC2R = 0x188
                    0x0188                  _OC2R = 0x188
                    0x018a                  OC2CON = 0x18a
                    0x018a                  _OC2CON = 0x18a
                    0x018a                  _OC2CONbits = 0x18a
                    0x018c                  OC3RS = 0x18c
                    0x018c                  _OC3RS = 0x18c
                    0x018e                  OC3R = 0x18e
                    0x018e                  _OC3R = 0x18e
                    0x0190                  OC3CON = 0x190
                    0x0190                  _OC3CON = 0x190
                    0x0190                  _OC3CONbits = 0x190
                    0x0192                  OC4RS = 0x192
                    0x0192                  _OC4RS = 0x192
                    0x0194                  OC4R = 0x194
                    0x0194                  _OC4R = 0x194
                    0x0196                  OC4CON = 0x196
                    0x0196                  _OC4CON = 0x196
                    0x0196                  _OC4CONbits = 0x196
                    0x0198                  OC5RS = 0x198
                    0x0198                  _OC5RS = 0x198
                    0x019a                  OC5R = 0x19a
                    0x019a                  _OC5R = 0x19a
                    0x019c                  OC5CON = 0x19c
                    0x019c                  _OC5CON = 0x19c
                    0x019c                  _OC5CONbits = 0x19c
                    0x0200                  I2C1RCV = 0x200
                    0x0200                  _I2C1RCV = 0x200
                    0x0202                  I2C1TRN = 0x202
                    0x0202                  _I2C1TRN = 0x202
                    0x0204                  I2C1BRG = 0x204
                    0x0204                  _I2C1BRG = 0x204
                    0x0206                  I2C1CON = 0x206
                    0x0206                  _I2C1CON = 0x206
                    0x0206                  _I2C1CONbits = 0x206
                    0x0208                  I2C1STAT = 0x208
                    0x0208                  _I2C1STAT = 0x208
                    0x0208                  _I2C1STATbits = 0x208
                    0x020a                  I2C1ADD = 0x20a
                    0x020a                  _I2C1ADD = 0x20a
                    0x020c                  I2C1MSK = 0x20c
                    0x020c                  _I2C1MSK = 0x20c
                    0x0210                  I2C2RCV = 0x210
                    0x0210                  _I2C2RCV = 0x210
                    0x0212                  I2C2TRN = 0x212
                    0x0212                  _I2C2TRN = 0x212
                    0x0214                  I2C2BRG = 0x214
                    0x0214                  _I2C2BRG = 0x214
                    0x0216                  I2C2CON = 0x216
                    0x0216                  _I2C2CON = 0x216
                    0x0216                  _I2C2CONbits = 0x216
                    0x0218                  I2C2STAT = 0x218
                    0x0218                  _I2C2STAT = 0x218
                    0x0218                  _I2C2STATbits = 0x218
                    0x021a                  I2C2ADD = 0x21a
                    0x021a                  _I2C2ADD = 0x21a
                    0x021c                  I2C2MSK = 0x21c
                    0x021c                  _I2C2MSK = 0x21c
                    0x0220                  U1MODE = 0x220
                    0x0220                  _U1MODE = 0x220
                    0x0220                  _U1MODEbits = 0x220
                    0x0222                  U1STA = 0x222
                    0x0222                  _U1STA = 0x222
                    0x0222                  _U1STAbits = 0x222
                    0x0224                  U1TXREG = 0x224
                    0x0224                  _U1TXREG = 0x224
                    0x0226                  U1RXREG = 0x226
                    0x0226                  _U1RXREG = 0x226
                    0x0228                  U1BRG = 0x228
                    0x0228                  _U1BRG = 0x228
                    0x0230                  U2MODE = 0x230
                    0x0230                  _U2MODE = 0x230
                    0x0230                  _U2MODEbits = 0x230
                    0x0232                  U2STA = 0x232
                    0x0232                  _U2STA = 0x232
                    0x0232                  _U2STAbits = 0x232
                    0x0234                  U2TXREG = 0x234
                    0x0234                  _U2TXREG = 0x234
                    0x0236                  U2RXREG = 0x236
                    0x0236                  _U2RXREG = 0x236
                    0x0238                  U2BRG = 0x238
                    0x0238                  _U2BRG = 0x238
                    0x0240                  SPI1STAT = 0x240
                    0x0240                  _SPI1STAT = 0x240
                    0x0240                  _SPI1STATbits = 0x240
                    0x0242                  SPI1CON1 = 0x242
                    0x0242                  _SPI1CON1 = 0x242
                    0x0242                  _SPI1CON1bits = 0x242
                    0x0244                  SPI1CON2 = 0x244
                    0x0244                  _SPI1CON2 = 0x244
                    0x0244                  _SPI1CON2bits = 0x244
                    0x0248                  SPI1BUF = 0x248
                    0x0248                  _SPI1BUF = 0x248
                    0x0260                  SPI2STAT = 0x260
                    0x0260                  _SPI2STAT = 0x260
                    0x0260                  _SPI2STATbits = 0x260
                    0x0262                  SPI2CON1 = 0x262
                    0x0262                  _SPI2CON1 = 0x262
                    0x0262                  _SPI2CON1bits = 0x262
                    0x0264                  SPI2CON2 = 0x264
                    0x0264                  _SPI2CON2 = 0x264
                    0x0264                  _SPI2CON2bits = 0x264
                    0x0268                  SPI2BUF = 0x268
                    0x0268                  _SPI2BUF = 0x268
                    0x02c0                  TRISA = 0x2c0
                    0x02c0                  _TRISA = 0x2c0
                    0x02c0                  _TRISAbits = 0x2c0
                    0x02c2                  PORTA = 0x2c2
                    0x02c2                  _PORTA = 0x2c2
                    0x02c2                  _PORTAbits = 0x2c2
                    0x02c4                  LATA = 0x2c4
                    0x02c4                  _LATA = 0x2c4
                    0x02c4                  _LATAbits = 0x2c4
                    0x02c6                  TRISB = 0x2c6
                    0x02c6                  _TRISB = 0x2c6
                    0x02c6                  _TRISBbits = 0x2c6
                    0x02c8                  PORTB = 0x2c8
                    0x02c8                  _PORTB = 0x2c8
                    0x02c8                  _PORTBbits = 0x2c8
                    0x02ca                  LATB = 0x2ca
                    0x02ca                  _LATB = 0x2ca
                    0x02ca                  _LATBbits = 0x2ca
                    0x02cc                  TRISC = 0x2cc
                    0x02cc                  _TRISC = 0x2cc
                    0x02cc                  _TRISCbits = 0x2cc
                    0x02ce                  PORTC = 0x2ce
                    0x02ce                  _PORTC = 0x2ce
                    0x02ce                  _PORTCbits = 0x2ce
                    0x02d0                  LATC = 0x2d0
                    0x02d0                  _LATC = 0x2d0
                    0x02d0                  _LATCbits = 0x2d0
                    0x02d2                  TRISD = 0x2d2
                    0x02d2                  _TRISD = 0x2d2
                    0x02d2                  _TRISDbits = 0x2d2
                    0x02d4                  PORTD = 0x2d4
                    0x02d4                  _PORTD = 0x2d4
                    0x02d4                  _PORTDbits = 0x2d4
                    0x02d6                  LATD = 0x2d6
                    0x02d6                  _LATD = 0x2d6
                    0x02d6                  _LATDbits = 0x2d6
                    0x02d8                  TRISE = 0x2d8
                    0x02d8                  _TRISE = 0x2d8
                    0x02d8                  _TRISEbits = 0x2d8
                    0x02da                  PORTE = 0x2da
                    0x02da                  _PORTE = 0x2da
                    0x02da                  _PORTEbits = 0x2da
                    0x02dc                  LATE = 0x2dc
                    0x02dc                  _LATE = 0x2dc
                    0x02dc                  _LATEbits = 0x2dc
                    0x02de                  TRISF = 0x2de
                    0x02de                  _TRISF = 0x2de
                    0x02de                  _TRISFbits = 0x2de
                    0x02e0                  PORTF = 0x2e0
                    0x02e0                  _PORTF = 0x2e0
                    0x02e0                  _PORTFbits = 0x2e0
                    0x02e2                  LATF = 0x2e2
                    0x02e2                  _LATF = 0x2e2
                    0x02e2                  _LATFbits = 0x2e2
                    0x02e4                  TRISG = 0x2e4
                    0x02e4                  _TRISG = 0x2e4
                    0x02e4                  _TRISGbits = 0x2e4
                    0x02e6                  PORTG = 0x2e6
                    0x02e6                  _PORTG = 0x2e6
                    0x02e6                  _PORTGbits = 0x2e6
                    0x02e8                  LATG = 0x2e8
                    0x02e8                  _LATG = 0x2e8
                    0x02e8                  _LATGbits = 0x2e8
                    0x02fc                  PADCFG1 = 0x2fc
                    0x02fc                  _PADCFG1 = 0x2fc
                    0x02fc                  _PADCFG1bits = 0x2fc
                    0x0300                  ADC1BUF0 = 0x300
                    0x0300                  _ADC1BUF0 = 0x300
                    0x0302                  ADC1BUF1 = 0x302
                    0x0302                  _ADC1BUF1 = 0x302
                    0x0304                  ADC1BUF2 = 0x304
                    0x0304                  _ADC1BUF2 = 0x304
                    0x0306                  ADC1BUF3 = 0x306
                    0x0306                  _ADC1BUF3 = 0x306
                    0x0308                  ADC1BUF4 = 0x308
                    0x0308                  _ADC1BUF4 = 0x308
                    0x030a                  ADC1BUF5 = 0x30a
                    0x030a                  _ADC1BUF5 = 0x30a
                    0x030c                  ADC1BUF6 = 0x30c
                    0x030c                  _ADC1BUF6 = 0x30c
                    0x030e                  ADC1BUF7 = 0x30e
                    0x030e                  _ADC1BUF7 = 0x30e
                    0x0310                  ADC1BUF8 = 0x310
                    0x0310                  _ADC1BUF8 = 0x310
                    0x0312                  ADC1BUF9 = 0x312
                    0x0312                  _ADC1BUF9 = 0x312
                    0x0314                  ADC1BUFA = 0x314
                    0x0314                  _ADC1BUFA = 0x314
                    0x0316                  ADC1BUFB = 0x316
                    0x0316                  _ADC1BUFB = 0x316
                    0x0318                  ADC1BUFC = 0x318
                    0x0318                  _ADC1BUFC = 0x318
                    0x031a                  ADC1BUFD = 0x31a
                    0x031a                  _ADC1BUFD = 0x31a
                    0x031c                  ADC1BUFE = 0x31c
                    0x031c                  _ADC1BUFE = 0x31c
                    0x031e                  ADC1BUFF = 0x31e
                    0x031e                  _ADC1BUFF = 0x31e
                    0x0320                  AD1CON1 = 0x320
                    0x0320                  _AD1CON1 = 0x320
                    0x0320                  _AD1CON1bits = 0x320
                    0x0322                  AD1CON2 = 0x322
                    0x0322                  _AD1CON2 = 0x322
                    0x0322                  _AD1CON2bits = 0x322
                    0x0324                  AD1CON3 = 0x324
                    0x0324                  _AD1CON3 = 0x324
                    0x0324                  _AD1CON3bits = 0x324
                    0x0328                  AD1CHS = 0x328
                    0x0328                  _AD1CHS = 0x328
                    0x0328                  _AD1CHSbits = 0x328
                    0x032c                  AD1PCFG = 0x32c
                    0x032c                  _AD1PCFG = 0x32c
                    0x032c                  _AD1PCFGbits = 0x32c
                    0x0330                  AD1CSSL = 0x330
                    0x0330                  _AD1CSSL = 0x330
                    0x0330                  _AD1CSSLbits = 0x330
                    0x0600                  PMCON = 0x600
                    0x0600                  _PMCON = 0x600
                    0x0600                  _PMCONbits = 0x600
                    0x0602                  PMMODE = 0x602
                    0x0602                  _PMMODE = 0x602
                    0x0602                  _PMMODEbits = 0x602
                    0x0604                  PMADDR = 0x604
                    0x0604                  _PMADDR = 0x604
                    0x0604                  _PMADDRbits = 0x604
                    0x0604                  PMDOUT1 = 0x604
                    0x0604                  _PMDOUT1 = 0x604
                    0x0604                  _PMDOUT1bits = 0x604
                    0x0606                  PMDOUT2 = 0x606
                    0x0606                  _PMDOUT2 = 0x606
                    0x0608                  PMDIN1 = 0x608
                    0x0608                  _PMDIN1 = 0x608
                    0x060a                  PMDIN2 = 0x60a
                    0x060a                  _PMDIN2 = 0x60a
                    0x060c                  PMAEN = 0x60c
                    0x060c                  _PMAEN = 0x60c
                    0x060c                  _PMAENbits = 0x60c
                    0x060e                  PMSTAT = 0x60e
                    0x060e                  _PMSTAT = 0x60e
                    0x060e                  _PMSTATbits = 0x60e
                    0x0620                  ALRMVAL = 0x620
                    0x0620                  _ALRMVAL = 0x620
                    0x0622                  ALCFGRPT = 0x622
                    0x0622                  _ALCFGRPT = 0x622
                    0x0622                  _ALCFGRPTbits = 0x622
                    0x0624                  RTCVAL = 0x624
                    0x0624                  _RTCVAL = 0x624
                    0x0626                  RCFGCAL = 0x626
                    0x0626                  _RCFGCAL = 0x626
                    0x0626                  _RCFGCALbits = 0x626
                    0x0630                  CMCON = 0x630
                    0x0630                  _CMCON = 0x630
                    0x0630                  _CMCONbits = 0x630
                    0x0632                  CVRCON = 0x632
                    0x0632                  _CVRCON = 0x632
                    0x0632                  _CVRCONbits = 0x632
                    0x0640                  CRCCON = 0x640
                    0x0640                  _CRCCON = 0x640
                    0x0640                  _CRCCONbits = 0x640
                    0x0642                  CRCXOR = 0x642
                    0x0642                  _CRCXOR = 0x642
                    0x0642                  _CRCXORbits = 0x642
                    0x0644                  CRCDAT = 0x644
                    0x0644                  _CRCDAT = 0x644
                    0x0646                  CRCWDAT = 0x646
                    0x0646                  _CRCWDAT = 0x646
                    0x06c0                  ODCA = 0x6c0
                    0x06c0                  _ODCA = 0x6c0
                    0x06c0                  _ODCAbits = 0x6c0
                    0x06c6                  ODCB = 0x6c6
                    0x06c6                  _ODCB = 0x6c6
                    0x06c6                  _ODCBbits = 0x6c6
                    0x06cc                  ODCC = 0x6cc
                    0x06cc                  _ODCC = 0x6cc
                    0x06cc                  _ODCCbits = 0x6cc
                    0x06d2                  ODCD = 0x6d2
                    0x06d2                  _ODCD = 0x6d2
                    0x06d2                  _ODCDbits = 0x6d2
                    0x06d8                  ODCE = 0x6d8
                    0x06d8                  _ODCE = 0x6d8
                    0x06d8                  _ODCEbits = 0x6d8
                    0x06de                  ODCF = 0x6de
                    0x06de                  _ODCF = 0x6de
                    0x06de                  _ODCFbits = 0x6de
                    0x06e4                  ODCG = 0x6e4
                    0x06e4                  _ODCG = 0x6e4
                    0x06e4                  _ODCGbits = 0x6e4
                    0x0740                  RCON = 0x740
                    0x0740                  _RCON = 0x740
                    0x0740                  _RCONbits = 0x740
                    0x0742                  OSCCON = 0x742
                    0x0742                  _OSCCON = 0x742
                    0x0742                  _OSCCONbits = 0x742
                    0x0742                  OSCCONL = 0x742
                    0x0742                  _OSCCONL = 0x742
                    0x0743                  OSCCONH = 0x743
                    0x0743                  _OSCCONH = 0x743
                    0x0744                  CLKDIV = 0x744
                    0x0744                  _CLKDIV = 0x744
                    0x0744                  _CLKDIVbits = 0x744
                    0x0748                  OSCTUN = 0x748
                    0x0748                  _OSCTUN = 0x748
                    0x0748                  _OSCTUNbits = 0x748
                    0x0760                  NVMCON = 0x760
                    0x0760                  _NVMCON = 0x760
                    0x0760                  _NVMCONbits = 0x760
                    0x0766                  NVMKEY = 0x766
                    0x0766                  _NVMKEY = 0x766
                    0x0770                  PMD1 = 0x770
                    0x0770                  _PMD1 = 0x770
                    0x0770                  _PMD1bits = 0x770
                    0x0772                  PMD2 = 0x772
                    0x0772                  _PMD2 = 0x772
                    0x0772                  _PMD2bits = 0x772
                    0x0774                  PMD3 = 0x774
                    0x0774                  _PMD3 = 0x774
                    0x0774                  _PMD3bits = 0x774
                    0x0140                  IC1 = 0x140
                    0x0140                  _IC1 = 0x140
                    0x0144                  IC2 = 0x144
                    0x0144                  _IC2 = 0x144
                    0x0148                  IC3 = 0x148
                    0x0148                  _IC3 = 0x148
                    0x014c                  IC4 = 0x14c
                    0x014c                  _IC4 = 0x14c
                    0x0150                  IC5 = 0x150
                    0x0150                  _IC5 = 0x150
                    0x0180                  OC1 = 0x180
                    0x0180                  _OC1 = 0x180
                    0x0186                  OC2 = 0x186
                    0x0186                  _OC2 = 0x186
                    0x018c                  OC3 = 0x18c
                    0x018c                  _OC3 = 0x18c
                    0x0192                  OC4 = 0x192
                    0x0192                  _OC4 = 0x192
                    0x0198                  OC5 = 0x198
                    0x0198                  _OC5 = 0x198
                    0x0240                  SPI1 = 0x240
                    0x0240                  _SPI1 = 0x240
                    0x0260                  SPI2 = 0x260
                    0x0260                  _SPI2 = 0x260
                    0x0220                  UART1 = 0x220
                    0x0220                  _UART1 = 0x220
                    0x0230                  UART2 = 0x230
                    0x0230                  _UART2 = 0x230
                    0x0001                  __MPLAB_BUILD = 0x1
START GROUP
LOAD c:/program files/microchip/mplab c30/bin/bin/../../lib\libpic30-coff.a
LOAD c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a
LOAD c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a
END GROUP
OUTPUT(TCPIP Demo App-C30.cof coff-pic30)
LOAD data_init
LOAD default_isr

.nbss               0x0800        0x3fc
 .nbss              0x0800        0x19a ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCP.o
 .nbss              0x099a         0xc8 Objects - TCPIP Demo App-C30\CustomHTTPApp.o
 .nbss              0x0a62         0x98 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UDP.o
                    0x0a68                  UDPSocketInfo
                    0x0af4                  activeUDPSocket
                    0x0af6                  UDPTxCount
                    0x0af8                  UDPRxCount
 .nbss              0x0afa         0x8c ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\HTTP2.o
                    0x0afa                  curHTTP
                    0x0b7c                  httpStubs
                    0x0b84                  curHTTPID
 .nbss              0x0b86         0x76 Objects - TCPIP Demo App-C30\MainDemo.o
                    0x0b8a                  AppConfig
                    0x0bf3                  AN0String

.ndata              0x0bfc         0x72
 .ndata             0x0bfc         0x72 Objects - TCPIP Demo App-C30\BerkeleyTCPClientDemo.o

.nbss               0x0c6e        0x12a
 .nbss              0x0c6e         0x70 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\MPFS2.o
                    0x0cda                  lastRead
 .nbss              0x0cde         0x66 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\BerkeleyAPI.o
 .nbss              0x0d44         0x54 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UART2TCPBridge.o

.ndata              0x0d98         0x98
 .ndata             0x0d98         0x50 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\HTTP2.o
 .ndata             0x0de8         0x48 Objects - TCPIP Demo App-C30\SMTPDemo.o

.nbss               0x0e30        0x130
 .nbss              0x0e30         0x40 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Hashes.o
                    0x0e30                  lastBlock
 .nbss              0x0e70         0x3a ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DynDNS.o
                    0x0e9a                  DDNSClient
 .nbss              0x0eaa         0x3a ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SMTP.o
                    0x0ecc                  SMTPClient
 .nbss              0x0ee4         0x2e ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SNMP.o
                    0x0f0a                  snmpReqVarErrStatus
 .nbss              0x0f12         0x28 Objects - TCPIP Demo App-C30\BerkeleyUDPClientDemo.o
 .nbss              0x0f3a         0x26 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SPIEEPROM.o

.ndata              0x0f60         0x26
 .ndata             0x0f60         0x26 Objects - TCPIP Demo App-C30\CustomSNMPApp.o
                    0x0f60                  gSendTrapFlag
                    0x0f61                  gOIDCorrespondingSnmpMibID
                    0x0f62                  gGenericTrapNotification
                    0x0f63                  gSpecificTrapNotification
                    0x0f64                  trapInfo

.nbss               0x0f86         0x22
 .nbss              0x0f86         0x22 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DHCP.o

.ndata              0x0fa8         0x22
 .ndata             0x0fa8         0x22 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DynDNS.o
                    0x0fc2                  ddnsServiceHosts

.nbss               0x0fca         0xaa
 .nbss              0x0fca         0x22 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\LCDBlocking.o
                    0x0fca                  LCDText
 .nbss              0x0fec         0x20 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCPPerformanceTest.o
 .nbss              0x100c         0x20 Objects - TCPIP Demo App-C30\CustomSNMPApp.o
 .nbss              0x102c         0x1a ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SNTP.o
 .nbss              0x1046         0x18 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DNS.o
 .nbss              0x105e         0x16 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ARP.o

.ndata              0x1074         0x16
 .ndata             0x1074         0x16 Objects - TCPIP Demo App-C30\GenericTCPClient.o

.nbss               0x108a         0x4e
 .nbss              0x108a         0x14 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ICMP.o
 .nbss              0x109e         0x14 Objects - TCPIP Demo App-C30\BerkeleyTCPServerDemo.o
 .nbss              0x10b2         0x10 Objects - TCPIP Demo App-C30\BerkeleyTCPClientDemo.o
 .nbss              0x10c2          0xc ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\StackTsk.o
                    0x10c4                  remoteNode
 .nbss              0x10ce          0xa ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Tick.o

.ndata              0x10d8          0xa
 .ndata             0x10d8          0xa ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UART2TCPBridge.o

.nbss               0x10e2         0x18
 .nbss              0x10e2          0x8 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DHCPs.o
 .nbss              0x10ea          0x8 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Telnet.o
 .nbss              0x10f2          0x8 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ENC28J60.o

.ndata              0x10fa          0x6
 .ndata             0x10fa          0x6 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DHCP.o
                    0x10fa                  smDHCPState
                    0x10fc                  DHCPFlags
                    0x10fe                  DHCPBindCount

.nbss               0x1100          0xc
 .nbss              0x1100          0x6 Objects - TCPIP Demo App-C30\PingDemo.o
 .nbss              0x1106          0x6 Objects - TCPIP Demo App-C30\SMTPDemo.o

.ndata              0x110c          0x4
 .ndata             0x110c          0x4 Objects - TCPIP Demo App-C30\MainDemo.o
                    0x110c                  myDHCPBindCount
                    0x110e                  __C30_UART

.nbss               0x1110          0x4
 .nbss              0x1110          0x4 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Announce.o

.ndata              0x1114          0x4
 .ndata             0x1114          0x4 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DNS.o

.nbss               0x1118         0x10
 .nbss              0x1118          0x4 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\IP.o
 .nbss              0x111c          0x4 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\NBNS.o
 .nbss              0x1120          0x4 Objects - TCPIP Demo App-C30\GenericTCPClient.o
 .nbss              0x1124          0x4 Objects - TCPIP Demo App-C30\GenericTCPServer.o

.ndata              0x1128          0x6
 .ndata             0x1128          0x4 Objects - TCPIP Demo App-C30\BerkeleyTCPServerDemo.o
 .ndata             0x112c          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UDP.o

_0185a7004a392480
                    0x112e          0x2
 _0185a7004a392480
                    0x112e          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UDP.o

.ndata              0x1130          0x2
 .ndata             0x1130          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DHCPs.o
                    0x1130                  bDHCPServerEnabled

_018768504a392489
                    0x1132          0x2
 _018768504a392489
                    0x1132          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DNS.o

.ndata              0x1134          0x8
 .ndata             0x1134          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Reboot.o
 .ndata             0x1136          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SMTP.o
 .ndata             0x1138          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SNMP.o
 .ndata             0x113a          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCP.o

_0189f7704a3924a4
                    0x113c          0x2
 _0189f7704a3924a4
                    0x113c          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCP.o

.ndata              0x113e          0x6
 .ndata             0x113e          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCPPerformanceTest.o
 .ndata             0x1140          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\BerkeleyAPI.o
 .ndata             0x1142          0x2 Objects - TCPIP Demo App-C30\BerkeleyUDPClientDemo.o

.bss                0x1144         0x88
 .bss               0x1144         0x88 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(rand.o)

.data               0x11cc         0x58
 .data              0x11cc         0x4a c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xstoul.o)
 .data              0x1216          0xa c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(rand.o)
                    0x1216                  _Tls_setup__Randseed
                    0x1218                  _Randseed
                    0x121c                  _Tls_setup__Randinit
                    0x121e                  _Randinit
 .data              0x1220          0x4 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(errno.o)
                    0x1220                  _Tls_setup_errno
                    0x1222                  errno

.const              0x8874       0x170a load address 0x000874  
 .const             0x8874        0x72a ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\HTTP2.o
 .const             0x8f9e        0x4bc Objects - TCPIP Demo App-C30\CustomHTTPApp.o
                    0x92b1                  HTML_UP_ARROW
                    0x92b4                  HTML_DOWN_ARROW
 .const             0x945a        0x1fe Objects - TCPIP Demo App-C30\UARTConfig.o
 .const             0x9658        0x1c2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Telnet.o
 .const             0x981a        0x1a4 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DynDNS.o
 .const             0x99be        0x140 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Hashes.o
 .const             0x9afe        0x12e Objects - TCPIP Demo App-C30\BerkeleyTCPClientDemo.o
 .const             0x9c2c         0xb8 Objects - TCPIP Demo App-C30\MainDemo.o
 .const             0x9ce4         0x8e Objects - TCPIP Demo App-C30\GenericTCPClient.o
 .const             0x9d72         0x86 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SMTP.o
 .const             0x9df8         0x58 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCPPerformanceTest.o
 .const             0x9e50         0x4a Objects - TCPIP Demo App-C30\SMTPDemo.o
 .const             0x9e9a         0x3a Objects - TCPIP Demo App-C30\PingDemo.o
 .const             0x9ed4         0x36 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCP.o
                    0x9ed4                  TCPSocketInitializer
 .const             0x9f0a         0x22 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SNMP.o
 .const             0x9f2c         0x1c ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Announce.o
 .const             0x9f48         0x12 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Reboot.o
 .const             0x9f5a          0xe ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SNTP.o
 .const             0x9f68          0xe Objects - TCPIP Demo App-C30\BerkeleyUDPClientDemo.o
 .const             0x9f76          0x8 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\MPFS2.o

.text             0x001f7e       0x20ca
 .text            0x001f7e       0x20ca ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCP.o
                  0x00201a                  TCPInit
                  0x0020e0                  TCPOpen
                  0x002226                  TCPWasReset
                  0x00224a                  TCPIsConnected
                  0x002266                  TCPDisconnect
                  0x0022e8                  TCPGetRemoteInfo
                  0x002304                  TCPFlush
                  0x002320                  TCPIsPutReady
                  0x00236a                  TCPPut
                  0x0023f6                  TCPPutArray
                  0x0024c4                  TCPPutString
                  0x0024e2                  TCPGetTxFIFOFull
                  0x002500                  TCPDiscard
                  0x00251e                  TCPIsGetReady
                  0x002550                  TCPGet
                  0x0025ba                  TCPGetArray
                  0x002676                  TCPGetRxFIFOFree
                  0x002692                  TCPFindArrayEx
                  0x002916                  TCPFindEx
                  0x002934                  TCPTick
                  0x002da2                  TCPProcess
                  0x003e2e                  TCPAdjustFIFOSize

.text             0x004048       0x1f10
 .text            0x004048       0x1f10 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SNMP.o
                  0x004048                  SNMPInit
                  0x00405e                  SNMPTask
                  0x0040ee                  SNMPNotifyPrepare
                  0x004128                  SNMPIsNotifyReady
                  0x00416c                  SNMPNotify

.text             0x005f58       0x1a32
 .text            0x005f58       0x1a32 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\HTTP2.o
                  0x005f58                  HTTPPrint
                  0x0061ce                  HTTPPrint_
                  0x0061e8                  HTTPInit
                  0x006258                  HTTPServer
                  0x007388                  HTTPURLDecode
                  0x00744e                  HTTPGetArg
                  0x007496                  HTTPReadPostName
                  0x0074be                  HTTPReadPostValue
                  0x0078c2                  HTTPIncFile

.text             0x00798a       0x1a2a
 .text            0x00798a       0x1a2a Objects - TCPIP Demo App-C30\CustomHTTPApp.o
                  0x00798a                  HTTPNeedsAuth
                  0x0079d4                  HTTPCheckAuth
                  0x007a2c                  HTTPExecuteGet
                  0x007c56                  HTTPExecutePost
                  0x00890a                  HTTPPrint_builddate
                  0x00894a                  HTTPPrint_version
                  0x008966                  HTTPPrint_btn
                  0x0089e6                  HTTPPrint_led
                  0x008ab6                  HTTPPrint_ledSelected
                  0x008b90                  HTTPPrint_pot
                  0x008bb6                  HTTPPrint_lcdtext
                  0x008c9a                  HTTPPrint_hellomsg
                  0x008cd8                  HTTPPrint_cookiename
                  0x008d18                  HTTPPrint_uploadedmd5
                  0x008df2                  HTTPPrintIP
                  0x008e46                  HTTPPrint_config_hostname
                  0x008e60                  HTTPPrint_config_dhcpchecked
                  0x008e84                  HTTPPrint_config_ip
                  0x008eaa                  HTTPPrint_config_gw
                  0x008ed0                  HTTPPrint_config_subnet
                  0x008ef6                  HTTPPrint_config_dns1
                  0x008f1c                  HTTPPrint_config_dns2
                  0x008f42                  HTTPPrint_config_mac
                  0x008fe0                  HTTPPrint_read_comm
                  0x00900e                  HTTPPrint_write_comm
                  0x00903c                  HTTPPrint_reboot
                  0x009044                  HTTPPrint_rebootaddr
                  0x00905e                  HTTPPrint_ddns_user
                  0x0090b6                  HTTPPrint_ddns_pass
                  0x00910e                  HTTPPrint_ddns_host
                  0x009166                  HTTPPrint_ddns_service
                  0x0091a6                  HTTPPrint_ddns_status
                  0x00920e                  HTTPPrint_ddns_status_msg
                  0x009300                  HTTPPrint_smtps_en
                  0x00931c                  HTTPPrint_snmp_en
                  0x009338                  HTTPPrint_status_ok
                  0x009376                  HTTPPrint_status_fail

.text             0x0093b4        0xec0
 .text            0x0093b4        0xec0 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SMTP.o
                  0x0093b4                  SMTPBeginUsage
                  0x009408                  SMTPEndUsage
                  0x009450                  SMTPTask
                  0x009fac                  SMTPSendMail
                  0x009fb4                  SMTPIsBusy
                  0x009fca                  SMTPIsPutReady
                  0x009fe6                  SMTPPut
                  0x00a086                  SMTPPutArray
                  0x00a0c2                  SMTPPutString
                  0x00a0f8                  SMTPFlush
                  0x00a104                  SMTPPutDone

.text             0x00a274        0xcb6
 .text            0x00a274        0xcb6 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ENC28J60.o
                  0x00a274                  MACInit
                  0x00a394                  MACIsLinked
                  0x00a3a8                  MACIsTxReady
                  0x00a3c0                  MACDiscardRx
                  0x00a3f4                  MACGetFreeRxSize
                  0x00a47c                  MACGetHeader
                  0x00a55e                  MACPutHeader
                  0x00a5b2                  MACFlush
                  0x00a6ce                  MACSetReadPtrInRx
                  0x00a6fc                  MACSetWritePtr
                  0x00a72a                  MACSetReadPtr
                  0x00a758                  MACCalcRxChecksum
                  0x00a7b0                  CalcIPBufferChecksum
                  0x00a864                  MACMemCopyAsync
                  0x00aa12                  MACIsMemCopyDone
                  0x00aa2a                  MACGet
                  0x00aa5c                  MACGetArray
                  0x00ab36                  MACPut
                  0x00ab6e                  MACPutArray
                  0x00ad2a                  ReadPHYReg
                  0x00ae5c                  WritePHYReg
                  0x00aeac                  MACPowerDown
                  0x00aeda                  MACPowerUp
                  0x00aefa                  SetCLKOUT
                  0x00af10                  GetCLKOUT

.text             0x00af2a        0xad2
 .text            0x00af2a        0xad2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\MPFS2.o
                  0x00af2a                  MPFSInit
                  0x00af60                  MPFSOpen
                  0x00b0ae                  MPFSOpenID
                  0x00b132                  MPFSClose
                  0x00b154                  MPFSGet
                  0x00b25a                  MPFSGetArray
                  0x00b36e                  MPFSGetLong
                  0x00b38e                  MPFSSeek
                  0x00b56a                  MPFSFormat
                  0x00b604                  MPFSPutArray
                  0x00b6a8                  MPFSPutEnd
                  0x00b704                  MPFSGetTimestamp
                  0x00b752                  MPFSGetMicrotime
                  0x00b7a0                  MPFSGetFlags
                  0x00b7e4                  MPFSGetSize
                  0x00b832                  MPFSGetBytesRem
                  0x00b87a                  MPFSGetStartAddr
                  0x00b8ca                  MPFSGetEndAddr
                  0x00b924                  MPFSGetFilename
                  0x00b98c                  MPFSGetPosition
                  0x00b9ac                  MPFSGetID

.text             0x00b9fc        0xa58
 .text            0x00b9fc        0xa58 Objects - TCPIP Demo App-C30\CustomSNMPApp.o
                  0x00bab8                  SNMPTrapDemo
                  0x00bbe8                  SNMPSendTrap
                  0x00bd1c                  SNMPValidateCommunity
                  0x00bdc0                  SNMPIsValidSetLen
                  0x00bdfc                  SNMPSetVar
                  0x00bfbe                  SNMPGetNextIndex
                  0x00c016                  SNMPGetVar

.text             0x00c454        0x988
 .text            0x00c454        0x988 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\BerkeleyAPI.o
                  0x00c454                  BerkeleySocketInit
                  0x00c49a                  socket
                  0x00c518                  bind
                  0x00c58c                  listen
                  0x00c68a                  accept
                  0x00c76c                  connect
                  0x00c8aa                  send
                  0x00c9ec                  sendto
                  0x00cb2e                  recv
                  0x00cc5a                  recvfrom
                  0x00cd14                  gethostname
                  0x00cd78                  closesocket

.text             0x00cddc        0x964
 .text            0x00cddc        0x964 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DynDNS.o
                  0x00cddc                  DDNSInit
                  0x00ce1e                  DDNSTask
                  0x00d6f6                  DDNSForceUpdate
                  0x00d70c                  DDNSSetService
                  0x00d72c                  DDNSGetLastIP
                  0x00d738                  DDNSGetLastStatus

.text             0x00d740        0x956
 .text            0x00d740        0x956 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Helpers.o
                  0x00d740                  GenerateRandomDWORD
                  0x00d85a                  StringToIPAddress
                  0x00d9da                  Base64Decode
                  0x00db40                  Base64Encode
                  0x00dc9c                  uitoa
                  0x00dd1a                  ultoa
                  0x00ddca                  hexatob
                  0x00de40                  btohexa_high
                  0x00de68                  btohexa_low
                  0x00de8e                  stricmppgm2ram
                  0x00df26                  swaps
                  0x00df40                  swapl
                  0x00df9e                  CalcIPChecksum
                  0x00e014                  strupr
                  0x00e04e                  FormatNetBIOSName

.text             0x00e096        0x8d2
 .text            0x00e096        0x8d2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DHCP.o
                  0x00e096                  DHCPReset
                  0x00e0b8                  DHCPDisable
                  0x00e0d4                  DHCPEnable
                  0x00e0ec                  DHCPTask

.text             0x00e968        0x792
 .text            0x00e968        0x792 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DNS.o
                  0x00e968                  DNSBeginUsage
                  0x00e984                  DNSEndUsage
                  0x00e9aa                  DNSResolve
                  0x00e9da                  DNSIsResolved

.text             0x00f0fa        0x532
 .text            0x00f0fa        0x532 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UDP.o
                  0x00f0fa                  UDPInit
                  0x00f114                  UDPTask
                  0x00f11e                  UDPOpen
                  0x00f1ac                  UDPClose
                  0x00f1d6                  UDPSetTxBuffer
                  0x00f1ea                  UDPSetRxBuffer
                  0x00f1fe                  UDPIsPutReady
                  0x00f234                  UDPPut
                  0x00f268                  UDPPutArray
                  0x00f2a0                  UDPPutString
                  0x00f2b6                  UDPFlush
                  0x00f38c                  UDPIsGetReady
                  0x00f3bc                  UDPGet
                  0x00f3f2                  UDPGetArray
                  0x00f43c                  UDPDiscard
                  0x00f458                  UDPProcess

.text             0x00f62c        0x51a
 .text            0x00f62c        0x51a ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DHCPs.o
                  0x00f62c                  DHCPServerTask

.text             0x00fb46        0x4c4
 .text            0x00fb46        0x4c4 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Hashes.o
                  0x00fb46                  HashAddData
                  0x00fb62                  MD5Initialize
                  0x00fb9e                  MD5AddData
                  0x00fe9e                  MD5Calculate

.text             0x01000a        0x498
 .text            0x01000a        0x498 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Telnet.o
                  0x01000a                  TelnetTask

.text             0x0104a2        0x46c
 .text            0x0104a2        0x46c Objects - TCPIP Demo App-C30\MainDemo.o
                  0x0104a2                  _AddressError
                  0x0104ac                  _StackError
                  0x0104b6                  main
                  0x01060a                  DisplayIPValue
                  0x0108f4                  SaveAppConfig

.text             0x01090e        0x3a8
 .text            0x01090e        0x3a8 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ARP.o
                  0x010988                  ARPInit
                  0x0109be                  ARPProcess
                  0x010abe                  ARPResolve
                  0x010b8a                  ARPIsResolved

.text             0x010cb6        0x386
 .text            0x010cb6        0x386 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\NBNS.o
                  0x010cb6                  NBNSTask

.text             0x01103c        0x32e
 .text            0x01103c        0x32e ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SPIEEPROM.o
                  0x01103c                  XEEInit
                  0x01105a                  XEEBeginRead
                  0x01106e                  XEERead
                  0x0110ac                  XEEEndRead
                  0x0110b4                  XEEReadArray
                  0x011180                  XEEBeginWrite
                  0x011194                  XEEWrite
                  0x0111d0                  XEEWriteArray
                  0x0111f2                  XEEEndWrite
                  0x0112fe                  XEEIsBusy

.text             0x01136a        0x2da
 .text            0x01136a        0x2da ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCPPerformanceTest.o
                  0x01136a                  TCPPerformanceTask
                  0x011374                  TCPTXPerformanceTask
                  0x011532                  TCPRXPerformanceTask

.text             0x011644        0x2cc
 .text            0x011644        0x2cc ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SNTP.o
                  0x011644                  SNTPClient
                  0x0118b8                  SNTPGetUTCSeconds

.dinit            0x011910        0x2c6
 .dinit           0x011910        0x2c6 data_init

.text             0x011bd6        0x29e
 .text            0x011bd6        0x29e Objects - TCPIP Demo App-C30\BerkeleyUDPClientDemo.o
                  0x011bd6                  BerkeleyUDPClientDemo
                  0x011e1c                  BerkeleySNTPGetUTCSeconds

.text             0x011e74        0x27c
 .text            0x011e74        0x27c ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\StackTsk.o
                  0x011e74                  StackInit
                  0x011eb4                  StackTask
                  0x0120ba                  StackApplications

.text             0x0120f0        0x274
 .text            0x0120f0        0x274 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ICMP.o
                  0x0120f0                  ICMPProcess
                  0x0121b0                  ICMPSendPing
                  0x0121cc                  ICMPSendPingToHost
                  0x0121e8                  ICMPGetReply
                  0x012340                  ICMPBeginUsage
                  0x01235c                  ICMPEndUsage

.text             0x012364        0x262
 .text            0x012364        0x262 Objects - TCPIP Demo App-C30\UARTConfig.o
                  0x012364                  DoUARTConfig

.text             0x0125c6        0x1e0
 .text            0x0125c6        0x1e0 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UART2TCPBridge.o
                  0x0125c6                  UART2TCPBridgeInit
                  0x0125dc                  UART2TCPBridgeTask
                  0x012738                  _U2RXInterrupt
                  0x012776                  _U2TXInterrupt

.text             0x0127a6        0x1ac
 .text            0x0127a6        0x1ac ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\IP.o
                  0x0127a6                  IPGetHeader
                  0x012870                  IPPutHeader
                  0x01290e                  IPSetRxBuffer

.text             0x012952        0x1a8
 .text            0x012952        0x1a8 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\LCDBlocking.o
                  0x012996                  LCDInit
                  0x012a22                  LCDUpdate
                  0x012ade                  LCDErase

.text             0x012afa        0x166
 .text            0x012afa        0x166 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Announce.o
                  0x012afa                  AnnounceIP
                  0x012b7c                  DiscoveryTask

.text             0x012c60        0x15a
 .text            0x012c60        0x15a Objects - TCPIP Demo App-C30\GenericTCPClient.o
                  0x012c60                  GenericTCPClient

.text             0x012dba        0x152
 .text            0x012dba        0x152 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UART.o
                  0x012dba                  ReadStringUART
                  0x012e02                  putsUART2
                  0x012e50                  getsUART2
                  0x012eb8                  DataRdyUART2
                  0x012ec4                  BusyUART2
                  0x012ed2                  ReadUART2
                  0x012ef0                  WriteUART2

.text             0x012f0c        0x150
 .text            0x012f0c        0x150 Objects - TCPIP Demo App-C30\BerkeleyTCPServerDemo.o
                  0x012f0c                  BerkeleyTCPServerDemo

.text             0x01305c        0x14e
 .text            0x01305c        0x14e ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Reboot.o
                  0x01305c                  RebootTask

.text             0x0131aa        0x11e
 .text            0x0131aa        0x11e Objects - TCPIP Demo App-C30\BerkeleyTCPClientDemo.o
                  0x0131aa                  BerkeleyTCPClientDemo

.text             0x0132c8        0x106
 .text            0x0132c8        0x106 Objects - TCPIP Demo App-C30\SMTPDemo.o
                  0x0132c8                  SMTPDemo

.text             0x0133ce         0xfa
 .text            0x0133ce         0xfa ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Tick.o
                  0x0133ce                  TickInit
                  0x01344a                  TickGet
                  0x013456                  TickGetDiv256
                  0x013470                  TickGetDiv64K
                  0x01348a                  TickConvertToMilliseconds
                  0x0134b0                  _T1Interrupt

.text             0x0134c8         0xea
 .text            0x0134c8         0xea Objects - TCPIP Demo App-C30\PingDemo.o
                  0x0134c8                  PingDemo

.text             0x0135b2         0xd0
 .text            0x0135b2         0xd0 Objects - TCPIP Demo App-C30\GenericTCPServer.o
                  0x0135b2                  GenericTCPServer

.text             0x013682         0x56
 .text            0x013682         0x56 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Delay.o
                  0x013682                  DelayMs
                  0x0136ac                  Delay10us

.isr              0x0136d8          0x2
 .isr             0x0136d8          0x2 default_isr
                  0x0136d8                  _DefaultInterrupt
