Archive member included because of file (symbol)

C:\Microchip Solutions\Microchip\TCPIP Stack\BigInt_helper_coff.a(BigInt_helper.o)
                              ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\BigInt.o (_iA)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libpic30-coff.a(crt1.o)
                              (_resetALT)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libpic30-coff.a(crt0.o)
                              (_resetPRI)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(divmoddi3.o)
                              ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Tick.o (__udivdi3)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(udivsi3.o)
                              ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Helpers.o (__udivsi3)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(mulsi3.o)
                              ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Helpers.o (__mulsi3)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(muldi3.o)
                              ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCPPerformanceTest.o (__muldi3)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(umuldi3.o)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(muldi3.o) (__umuldi3)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strlen.o)
                              Objects - TCPIP Demo App-C30\MainDemo.o (strlen)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strcpy.o)
                              Objects - TCPIP Demo App-C30\MainDemo.o (strcpy)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memcmp.o)
                              Objects - TCPIP Demo App-C30\CustomHTTPApp.o (memcmp)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strcmp.o)
                              Objects - TCPIP Demo App-C30\CustomHTTPApp.o (strcmp)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xstoul.o)
                              Objects - TCPIP Demo App-C30\CustomHTTPApp.o (_Stoul)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memset.o)
                              Objects - TCPIP Demo App-C30\CustomHTTPApp.o (memset)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(rand.o)
                              ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Helpers.o (rand)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(srand.o)
                              ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Helpers.o (srand)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strchr.o)
                              ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SMTP.o (strchr)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strstr.o)
                              ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SMTP.o (strstr)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memcpy.o)
                              ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCP.o (memcpy)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strncmp.o)
                              Objects - TCPIP Demo App-C30\CustomSNMPApp.o (strncmp)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strcat.o)
                              Objects - TCPIP Demo App-C30\PingDemo.o (strcat)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(isspace.os)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xstoul.o) (isspace)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(tolower.os)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xstoul.o) (tolower)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memchr.o)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xstoul.o) (memchr)
c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(errno.o)
                              c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xstoul.o) (errno)


Program Memory Usage

section                    address   length (PC units)   length (bytes) (dec)
-------                    -------   -----------------   --------------------
.reset                           0                 0x4             0x6  (6)
.ivt                           0x4                0xfc           0x17a  (378)
.aivt                        0x104                0xfc           0x17a  (378)
.text                        0x200               0x692           0x9db  (2523)
.const                       0x892              0x19dc          0x26ca  (9930)
.text                       0x226e              0x1a94          0x27de  (10206)
.text                       0x3d02              0x14a2          0x1ef3  (7923)
.text                       0x51a4              0x12fe          0x1c7d  (7293)
.text                       0x64a2              0x1210          0x1b18  (6936)
.text                       0x76b2              0x1140          0x19e0  (6624)
.text                       0x87f2               0xade          0x104d  (4173)
.text                       0x92d0               0x8e2           0xd53  (3411)
.text                       0x9bb2               0x71c           0xaaa  (2730)
.text                       0xa2ce               0x63c           0x95a  (2394)
.text                       0xa90a               0x632           0x94b  (2379)
.text                       0xaf3c               0x620           0x930  (2352)
.text                       0xb55c               0x5da           0x8c7  (2247)
.text                       0xbb36               0x5a0           0x870  (2160)
.text                       0xc0d6               0x526           0x7b9  (1977)
.text                       0xc5fc               0x524           0x7b6  (1974)
.text                       0xcb20               0x478           0x6b4  (1716)
.text                       0xcf98               0x46c           0x6a2  (1698)
.text                       0xd404               0x44c           0x672  (1650)
.text                       0xd850               0x3ce           0x5b5  (1461)
.text                       0xdc1e               0x382           0x543  (1347)
.dinit                      0xdfa0               0x2de           0x44d  (1101)
.text                       0xe27e               0x280           0x3c0  (960)
.text                       0xe4fe               0x27c           0x3ba  (954)
.text                       0xe77a               0x252           0x37b  (891)
.text                       0xe9cc               0x23c           0x35a  (858)
.text                       0xec08               0x238           0x354  (852)
.text                       0xee40               0x236           0x351  (849)
.text                       0xf076               0x204           0x306  (774)
.text                       0xf27a               0x1fe           0x2fd  (765)
.text                       0xf478               0x1d0           0x2b8  (696)
.text                       0xf648               0x1b0           0x288  (648)
.text                       0xf7f8               0x154           0x1fe  (510)
.text                       0xf94c               0x140           0x1e0  (480)
.text                       0xfa8c               0x138           0x1d4  (468)
.text                       0xfbc4               0x12e           0x1c5  (453)
.text                       0xfcf2               0x122           0x1b3  (435)
.text                       0xfe14                0xec           0x162  (354)
.text                       0xff00                0xe8           0x15c  (348)
.text                       0xffe8                0xe6           0x159  (345)
.text                      0x100ce                0xdc           0x14a  (330)
.text                      0x101aa                0xce           0x135  (309)
.text                      0x10278                0xce           0x135  (309)
.text                      0x10346                0xb8           0x114  (276)
.text                      0x103fe                0xa0            0xf0  (240)
.text                      0x1049e                0xa0            0xf0  (240)
.text                      0x1053e                0x80            0xc0  (192)
.text                      0x105be                0x60            0x90  (144)
.text                      0x1061e                0x4e            0x75  (117)
.isr                       0x1066c                 0x2             0x3  (3)
__CONFIG2                  0x157fc                 0x2             0x3  (3)
__CONFIG1                  0x157fe                 0x2             0x3  (3)

                     Total program memory used (bytes):        0x189a5  (100773) 76%


Data Memory Usage

section                    address      alignment gaps    total length  (dec)
-------                    -------      --------------    -------------------
.nbss                        0x800                   0           0x65a  (1626)
.ndata                       0xe5a                   0            0x72  (114)
.nbss                        0xecc                   0           0x1ee  (494)
.ndata                      0x10ba                   0            0x98  (152)
.nbss                       0x1152                   0           0x130  (304)
.ndata                      0x1282                   0            0x26  (38)
.nbss                       0x12a8                   0            0x22  (34)
.ndata                      0x12ca                   0            0x22  (34)
.nbss                       0x12ec                   0            0xaa  (170)
.ndata                      0x1396                   0            0x16  (22)
.nbss                       0x13ac                   0            0x4e  (78)
.ndata                      0x13fa                   0             0xa  (10)
.nbss                       0x1404                   0            0x18  (24)
.ndata                      0x141c                   0             0x6  (6)
.nbss                       0x1422                   0             0xc  (12)
.ndata                      0x142e                   0             0x4  (4)
.nbss                       0x1432                   0             0x4  (4)
.ndata                      0x1436                   0             0x4  (4)
.nbss                       0x143a                   0            0x10  (16)
.ndata                      0x144a                   0             0x6  (6)
_018770704a24403d           0x1450                   0             0x2  (2)
.ndata                      0x1452                   0             0x2  (2)
_0188b5404a244046           0x1454                   0             0x2  (2)
.ndata                      0x1456                   0             0x8  (8)
_018aebd04a244061           0x145e                   0             0x2  (2)
.ndata                      0x1460                   0             0x6  (6)
.bss                        0x1466                   0            0x88  (136)
.data                       0x14ee                   0            0x4a  (74)
.bss                        0x1538                   0             0xc  (12)
.data                       0x1544                   0             0xe  (14)

                        Total data memory used (bytes):          0xd52  (3410) 41%


Dynamic Memory Usage

region                     address                      maximum length  (dec)
------                     -------                      ---------------------
heap                             0                                   0  (0)
stack                       0x1552                              0x12ae  (4782)

                        Maximum dynamic memory (bytes):         0x12ae  (4782)


External Symbols in Data Memory (by address):

                    0x0800                  _isBufferUsed
                    0x0802                  _isHashUsed
                    0x0804                  _isStubUsed
                    0x0806                  _ptrHS
                    0x0808                  _sslSessionStubs
                    0x0818                  _sslSession
                    0x0868                  _sslHash
                    0x08c2                  _sslBuffer
                    0x0cc0                  _UDPRxCount
                    0x0cc2                  _UDPTxCount
                    0x0cc4                  _activeUDPSocket
                    0x0cc6                  _UDPSocketInfo
                    0x0d58                  _curHTTPID
                    0x0d5a                  _httpStubs
                    0x0d62                  _curHTTP
                    0x0de8                  _AppConfig
                    0x0e51                  _AN0String
                    0x0ecc                  _lastRead
                    0x107c                  _qInv
                    0x1084                  _dQ
                    0x108c                  _dP
                    0x1094                  _Q
                    0x109c                  _P
                    0x1152                  _lastBlock
                    0x11b0                  _DDNSClient
                    0x11e0                  _SMTPClient
                    0x1214                  _snmpReqVarErrStatus
                    0x1282                  _trapInfo
                    0x12a4                  _gSpecificTrapNotification
                    0x12a5                  _gGenericTrapNotification
                    0x12a6                  _gOIDCorrespondingSnmpMibID
                    0x12a7                  _gSendTrapFlag
                    0x12ca                  _ddnsServiceHosts
                    0x12ec                  _LCDText
                    0x13e4                  _remoteNode
                    0x141c                  _DHCPBindCount
                    0x141d                  _DHCPFlags
                    0x141e                  _smDHCPState
                    0x142e                  _myDHCPBindCount
                    0x1430                  ___C30_UART
                    0x1452                  _bDHCPServerEnabled
                    0x1538                  __iA
                    0x153a                  __xA
                    0x153c                  __iB
                    0x153e                  __xB
                    0x1540                  __iR
                    0x1542                  __wC
                    0x1544                  __Tls_setup__Randseed
                    0x1546                  __Randseed
                    0x154a                  __Tls_setup__Randinit
                    0x154c                  __Randinit
                    0x154e                  __Tls_setup_errno
                    0x1550                  _errno

External Symbols in Data Memory (by name):

                    0x0e51                  _AN0String
                    0x0de8                  _AppConfig
                    0x11b0                  _DDNSClient
                    0x141c                  _DHCPBindCount
                    0x141d                  _DHCPFlags
                    0x12ec                  _LCDText
                    0x109c                  _P
                    0x1094                  _Q
                    0x11e0                  _SMTPClient
                    0x0cc0                  _UDPRxCount
                    0x0cc6                  _UDPSocketInfo
                    0x0cc2                  _UDPTxCount
                    0x154c                  __Randinit
                    0x1546                  __Randseed
                    0x154a                  __Tls_setup__Randinit
                    0x1544                  __Tls_setup__Randseed
                    0x154e                  __Tls_setup_errno
                    0x1430                  ___C30_UART
                    0x1538                  __iA
                    0x153c                  __iB
                    0x1540                  __iR
                    0x1542                  __wC
                    0x153a                  __xA
                    0x153e                  __xB
                    0x0cc4                  _activeUDPSocket
                    0x1452                  _bDHCPServerEnabled
                    0x0d62                  _curHTTP
                    0x0d58                  _curHTTPID
                    0x108c                  _dP
                    0x1084                  _dQ
                    0x12ca                  _ddnsServiceHosts
                    0x1550                  _errno
                    0x12a5                  _gGenericTrapNotification
                    0x12a6                  _gOIDCorrespondingSnmpMibID
                    0x12a7                  _gSendTrapFlag
                    0x12a4                  _gSpecificTrapNotification
                    0x0d5a                  _httpStubs
                    0x0800                  _isBufferUsed
                    0x0802                  _isHashUsed
                    0x0804                  _isStubUsed
                    0x1152                  _lastBlock
                    0x0ecc                  _lastRead
                    0x142e                  _myDHCPBindCount
                    0x0806                  _ptrHS
                    0x107c                  _qInv
                    0x13e4                  _remoteNode
                    0x141e                  _smDHCPState
                    0x1214                  _snmpReqVarErrStatus
                    0x08c2                  _sslBuffer
                    0x0868                  _sslHash
                    0x0818                  _sslSession
                    0x0808                  _sslSessionStubs
                    0x1282                  _trapInfo

External Symbols in Program Memory (by address):

                  0x000200                  __resetPRI
                  0x00021e                  __psv_init
                  0x00022e                  __data_init
                  0x000288                  _strlen
                  0x000296                  _strcpy
                  0x0002a6                  _memcmp
                  0x0002c2                  _strcmp
                  0x0002e6                  __Stoul
                  0x00040e                  _memset
                  0x00041c                  _rand
                  0x0004c6                  _srand
                  0x0004e8                  _strchr
                  0x0004fa                  _strstr
                  0x000522                  _memcpy
                  0x000530                  _strncmp
                  0x000554                  _strcat
                  0x000572                  _isspace
                  0x000582                  _tolower
                  0x000590                  _memchr
                  0x0005a4                  __Geterrno
                  0x0005d6                  ___udivmoddi3
                  0x0006a4                  ___udivdi3
                  0x0006b2                  ___umoddi3
                  0x0006ba                  ___divdi3
                  0x0006f4                  ___moddi3
                  0x0007c6                  ___udivsi3
                  0x0007e6                  ___mulsi3
                  0x0007f2                  ___muldi3
                  0x00084e                  ___umuldi3
                  0x000fbc                  _HTML_DOWN_ARROW
                  0x000fbf                  _HTML_UP_ARROW
                  0x001460                  _SSL_CERT_LEN
                  0x001462                  _SSL_CERT
                  0x00166e                  _SSL_qInv
                  0x00168e                  _SSL_dQ
                  0x0016ae                  _SSL_dP
                  0x0016ce                  _SSL_Q
                  0x0016ee                  _SSL_P
                  0x0021c4                  _TCPSocketInitializer
                  0x0022a8                  _TCPWasReset
                  0x0022b8                  _TCPIsConnected
                  0x0022c8                  _TCPIsPutReady
                  0x002312                  _TCPGetTxFIFOFull
                  0x002328                  _TCPIsGetReady
                  0x002344                  _TCPGetRxFIFOFree
                  0x00236e                  _TCPSSLGetPendingTxSize
                  0x0023d0                  _TCPIsSSL
                  0x002506                  _TCPGetRemoteInfo
                  0x00251a                  _TCPInit
                  0x00289e                  _TCPAdjustFIFOSize
                  0x0029ae                  _TCPDiscard
                  0x0029ca                  _TCPFlush
                  0x0029de                  _TCPDisconnect
                  0x002a56                  _TCPOpen
                  0x002b4c                  _TCPFindArrayEx
                  0x002cbe                  _TCPFindEx
                  0x002cd2                  _TCPGetArray
                  0x002d4e                  _TCPGet
                  0x002da6                  _TCPPutArray
                  0x002e7a                  _TCPPutString
                  0x002e94                  _TCPPut
                  0x002f2a                  _TCPStartSSLServer
                  0x002f7c                  _TCPTick
                  0x0032e6                  _TCPAddSSLListener
                  0x003302                  _TCPRequestSSLMessage
                  0x003322                  _TCPSSLIsHandshaking
                  0x00332c                  _TCPSSLHandshakeComplete
                  0x003332                  _TCPSSLDecryptMAC
                  0x003414                  _TCPSSLInPlaceMACEncrypt
                  0x0034f0                  _TCPSSLPutRecordHeader
                  0x003552                  _TCPSSLHandleIncoming
                  0x00363a                  _TCPProcess
                  0x003d02                  _SNMPInit
                  0x003d12                  _SNMPNotifyPrepare
                  0x003d46                  _SNMPIsNotifyReady
                  0x004282                  _SNMPNotify
                  0x00456a                  _SNMPTask
                  0x0051a4                  _HTTPPrint_
                  0x0051b4                  _HTTPInit
                  0x005262                  _HTTPURLDecode
                  0x0052d0                  _HTTPGetArg
                  0x005430                  _HTTPReadPostName
                  0x005450                  _HTTPReadPostValue
                  0x0054a2                  _HTTPIncFile
                  0x005546                  _HTTPPrint
                  0x0056f2                  _HTTPServer
                  0x0064a2                  _HTTPNeedsAuth
                  0x0064ca                  _HTTPCheckAuth
                  0x0064ee                  _HTTPExecuteGet
                  0x006776                  _HTTPExecutePost
                  0x006fd2                  _HTTPPrint_builddate
                  0x007006                  _HTTPPrint_version
                  0x007016                  _HTTPPrint_btn
                  0x007054                  _HTTPPrint_led
                  0x0070b8                  _HTTPPrint_ledSelected
                  0x007128                  _HTTPPrint_pot
                  0x007146                  _HTTPPrint_lcdtext
                  0x0071d8                  _HTTPPrint_hellomsg
                  0x00720e                  _HTTPPrint_cookiename
                  0x00723e                  _HTTPPrint_uploadedmd5
                  0x0072e2                  _HTTPPrintIP
                  0x00732c                  _HTTPPrint_config_hostname
                  0x00733c                  _HTTPPrint_config_dhcpchecked
                  0x007352                  _HTTPPrint_config_ip
                  0x007370                  _HTTPPrint_config_gw
                  0x00738e                  _HTTPPrint_config_subnet
                  0x0073ac                  _HTTPPrint_config_dns1
                  0x0073ca                  _HTTPPrint_config_dns2
                  0x0073e8                  _HTTPPrint_config_mac
                  0x007460                  _HTTPPrint_read_comm
                  0x00747a                  _HTTPPrint_write_comm
                  0x007494                  _HTTPPrint_reboot
                  0x007498                  _HTTPPrint_rebootaddr
                  0x0074a8                  _HTTPPrint_ddns_user
                  0x0074e2                  _HTTPPrint_ddns_pass
                  0x00751c                  _HTTPPrint_ddns_host
                  0x007556                  _HTTPPrint_ddns_service
                  0x00757c                  _HTTPPrint_ddns_status
                  0x0075ba                  _HTTPPrint_ddns_status_msg
                  0x00764a                  _HTTPPrint_smtps_en
                  0x00765a                  _HTTPPrint_snmp_en
                  0x00766a                  _HTTPPrint_status_ok
                  0x00768e                  _HTTPPrint_status_fail
                  0x0076b2                  _SSLInit
                  0x007734                  _SSLMACBegin
                  0x007796                  _SSLMACCalc
                  0x007c64                  _SSLRxHandshake
                  0x00801a                  _SSLStartSession
                  0x008126                  _SSLStartPartialRecord
                  0x008158                  _SSLTxRecord
                  0x0081d0                  _SSLRxRecord
                  0x0083ce                  _SSLTerminate
                  0x0083fc                  _SSLPeriodic
                  0x0084a4                  _SSLTxMessage
                  0x0087e8                  _SSLMACAdd
                  0x0087f2                  _MACGet
                  0x008818                  _MACGetArray
                  0x0088aa                  _MACPut
                  0x0088d8                  _MACPutArray
                  0x0089f0                  _MACSetReadPtrInRx
                  0x008a12                  _MACPutHeader
                  0x008a92                  _MACDiscardRx
                  0x008b06                  _SetCLKOUT
                  0x008b1c                  _WritePHYReg
                  0x008b54                  _ReadPHYReg
                  0x008bb2                  _MACIsLinked
                  0x008bf2                  _GetCLKOUT
                  0x008c10                  _MACPowerUp
                  0x008c2e                  _MACPowerDown
                  0x008c58                  _MACIsMemCopyDone
                  0x008c6e                  _MACMemCopyAsync
                  0x008dee                  _CalcIPBufferChecksum
                  0x008e7c                  _MACCalcRxChecksum
                  0x008ed8                  _MACSetReadPtr
                  0x008f12                  _MACSetWritePtr
                  0x008f4c                  _MACFlush
                  0x009062                  _MACGetHeader
                  0x0090fe                  _MACGetFreeRxSize
                  0x009180                  _MACIsTxReady
                  0x009196                  _MACInit
                  0x0092d0                  _SMTPBeginUsage
                  0x0092fa                  _SMTPEndUsage
                  0x0093d2                  _SMTPTask
                  0x009ae2                  _SMTPSendMail
                  0x009ae6                  _SMTPIsBusy
                  0x009af0                  _SMTPIsPutReady
                  0x009b04                  _SMTPPut
                  0x009b6a                  _SMTPPutArray
                  0x009b8c                  _SMTPPutString
                  0x009ba8                  _SMTPFlush
                  0x009bae                  _SMTPPutDone
                  0x009bb2                  _MD5Initialize
                  0x009d2c                  _MD5AddData
                  0x009d76                  _MD5Calculate
                  0x009e70                  _SHA1Initialize
                  0x00a0f0                  _SHA1AddData
                  0x00a13c                  _HashAddData
                  0x00a164                  _SHA1Calculate
                  0x00a2ce                  _DHCPReset
                  0x00a2e8                  _DHCPDisable
                  0x00a2fa                  _DHCPEnable
                  0x00a6e2                  _DHCPTask
                  0x00a90a                  _SNMPValidateCommunity
                  0x00a96e                  _SNMPIsValidSetLen
                  0x00a988                  _SNMPSetVar
                  0x00aa72                  _SNMPGetNextIndex
                  0x00ab5e                  _SNMPSendTrap
                  0x00acb4                  _SNMPTrapDemo
                  0x00ad98                  _SNMPGetVar
                  0x00af3c                  _DDNSInit
                  0x00af6a                  _DDNSTask
                  0x00b52c                  _DDNSForceUpdate
                  0x00b53e                  _DDNSSetService
                  0x00b550                  _DDNSGetLastIP
                  0x00b558                  _DDNSGetLastStatus
                  0x00b55c                  _MPFSClose
                  0x00b574                  _MPFSGet
                  0x00b5fa                  _MPFSGetArray
                  0x00b6a2                  _MPFSOpenID
                  0x00b6fc                  _MPFSOpen
                  0x00b7e0                  _MPFSGetLong
                  0x00b7ee                  _MPFSGetSize
                  0x00b816                  _MPFSGetStartAddr
                  0x00b844                  _MPFSGetEndAddr
                  0x00b876                  _MPFSSeek
                  0x00b928                  _MPFSFormat
                  0x00b968                  _MPFSGetTimestamp
                  0x00b990                  _MPFSGetMicrotime
                  0x00b9b8                  _MPFSGetFlags
                  0x00b9dc                  _MPFSGetBytesRem
                  0x00b9fc                  _MPFSGetFilename
                  0x00ba40                  _MPFSGetPosition
                  0x00ba58                  _MPFSGetID
                  0x00ba92                  _MPFSPutEnd
                  0x00baae                  _MPFSPutArray
                  0x00bb1a                  _MPFSInit
                  0x00bb36                  _BerkeleySocketInit
                  0x00bb56                  _socket
                  0x00bb90                  _bind
                  0x00bbca                  _listen
                  0x00bc4c                  _accept
                  0x00bcc0                  _connect
                  0x00bd52                  _send
                  0x00be2a                  _sendto
                  0x00bf04                  _recv
                  0x00bfdc                  _recvfrom
                  0x00c058                  _gethostname
                  0x00c090                  _closesocket
                  0x00c0d6                  _GenerateRandomDWORD
                  0x00c1ac                  _StringToIPAddress
                  0x00c252                  _Base64Decode
                  0x00c318                  _Base64Encode
                  0x00c3d8                  _uitoa
                  0x00c414                  _ultoa
                  0x00c472                  _hexatob
                  0x00c4ce                  _btohexa_high
                  0x00c4e2                  _btohexa_low
                  0x00c4f4                  _stricmppgm2ram
                  0x00c536                  _swaps
                  0x00c548                  _swapl
                  0x00c576                  _CalcIPChecksum
                  0x00c5ae                  _strupr
                  0x00c5cc                  _FormatNetBIOSName
                  0x00c5fc                  _DNSBeginUsage
                  0x00c608                  _DNSEndUsage
                  0x00c622                  _DNSResolve
                  0x00c6b2                  _DNSIsResolved
                  0x00cb20                  _DHCPServerTask
                  0x00cf98                  __AddressError
                  0x00cfa2                  __StackError
                  0x00cfac                  _main
                  0x00d100                  _DisplayIPValue
                  0x00d3ea                  _SaveAppConfig
                  0x00d404                  _RSAInit
                  0x00d444                  _RSABeginUsage
                  0x00d460                  _RSAEndUsage
                  0x00d464                  _RSASetData
                  0x00d758                  _RSAStep
                  0x00d850                  _UDPClose
                  0x00d868                  _UDPTask
                  0x00d86c                  _UDPOpen
                  0x00d8cc                  _UDPSetTxBuffer
                  0x00d8de                  _UDPSetRxBuffer
                  0x00d8ee                  _UDPIsPutReady
                  0x00d918                  _UDPPut
                  0x00d93e                  _UDPPutArray
                  0x00d96a                  _UDPPutString
                  0x00d980                  _UDPFlush
                  0x00da40                  _UDPIsGetReady
                  0x00da5c                  _UDPGet
                  0x00da80                  _UDPGetArray
                  0x00daa8                  _UDPDiscard
                  0x00dab8                  _UDPProcess
                  0x00dc08                  _UDPInit
                  0x00dc1e                  _TelnetTask
                  0x00e27e                  _NBNSTask
                  0x00e4fe                  _ARPInit
                  0x00e518                  _ARPIsResolved
                  0x00e63e                  _ARPResolve
                  0x00e6c4                  _ARPProcess
                  0x00e77a                  _XEEInit
                  0x00e792                  _XEEBeginRead
                  0x00e79a                  _XEEEndRead
                  0x00e79c                  _XEEBeginWrite
                  0x00e7a4                  _XEEReadArray
                  0x00e838                  _XEERead
                  0x00e870                  _XEEIsBusy
                  0x00e986                  _XEEEndWrite
                  0x00e98e                  _XEEWrite
                  0x00e9ae                  _XEEWriteArray
                  0x00e9cc                  _BigInt
                  0x00e9de                  _BigIntZero
                  0x00ea2a                  _BigIntMagnitude
                  0x00ea38                  _BigIntMagnitudeDifference
                  0x00ea4c                  _BigIntCompare
                  0x00ea94                  _BigIntMod
                  0x00eb38                  _BigIntMultiply
                  0x00eb6c                  _BigIntSquare
                  0x00eb90                  _BigIntAdd
                  0x00ebb2                  _BigIntSubtract
                  0x00ebd4                  _BigIntCopy
                  0x00ebf4                  _BigIntSwapEndianness
                  0x00ec08                  _DoUARTConfig
                  0x00ee40                  _TCPTXPerformanceTask
                  0x00ef9c                  _TCPRXPerformanceTask
                  0x00f072                  _TCPPerformanceTask
                  0x00f076                  _ICMPProcess
                  0x00f130                  _ICMPSendPing
                  0x00f14a                  _ICMPSendPingToHost
                  0x00f164                  _ICMPGetReply
                  0x00f26a                  _ICMPBeginUsage
                  0x00f276                  _ICMPEndUsage
                  0x00f27a                  _SNTPClient
                  0x00f440                  _SNTPGetUTCSeconds
                  0x00f478                  _BerkeleyUDPClientDemo
                  0x00f610                  _BerkeleySNTPGetUTCSeconds
                  0x00f648                  _StackInit
                  0x00f684                  _StackTask
                  0x00f7c8                  _StackApplications
                  0x00f7f8                  _UART2TCPBridgeInit
                  0x00f80a                  _UART2TCPBridgeTask
                  0x00f8f4                  __U2RXInterrupt
                  0x00f928                  __U2TXInterrupt
                  0x00f982                  _LCDInit
                  0x00f9fe                  _LCDUpdate
                  0x00fa76                  _LCDErase
                  0x00fa8c                  _IPSetRxBuffer
                  0x00fab8                  _IPPutHeader
                  0x00fb40                  _IPGetHeader
                  0x00fbc4                  _AnnounceIP
                  0x00fc2c                  _DiscoveryTask
                  0x00fcf2                  _GenericTCPClient
                  0x00fe14                  _BerkeleyTCPServerDemo
                  0x00ff00                  _BerkeleyTCPClientDemo
                  0x00ffe8                  _TickInit
                  0x01003e                  _TickGet
                  0x010046                  _TickGetDiv256
                  0x010076                  _TickGetDiv64K
                  0x0100a6                  _TickConvertToMilliseconds
                  0x0100ba                  __T1Interrupt
                  0x0100ce                  __addBI
                  0x0100ee                  __subBI
                  0x01010e                  __zeroBI
                  0x01011a                  __msbBI
                  0x01012a                  __mulBI
                  0x010160                  __sqrBI
                  0x01016a                  __masBI
                  0x01018c                  __copyBI
                  0x0101aa                  _DataRdyUART2
                  0x0101b0                  _ReadUART2
                  0x0101c2                  _putsUART2
                  0x0101f6                  _BusyUART2
                  0x0101fe                  _WriteUART2
                  0x01020e                  _getsUART2
                  0x010246                  _ReadStringUART
                  0x010278                  _SMTPDemo
                  0x010346                  _RebootTask
                  0x0103fe                  _GenericTCPServer
                  0x01049e                  _PingDemo
                  0x01053e                  _ARCFOURInitialize
                  0x01057c                  _ARCFOURCrypt
                  0x0105be                  _RandomInit
                  0x0105ca                  _RandomAdd
                  0x0105f2                  _RandomGet
                  0x01061e                  _Delay10us
                  0x010646                  _DelayMs
                  0x01066c                  __DefaultInterrupt

External Symbols in Program Memory (by name):

                  0x01057c                  _ARCFOURCrypt
                  0x01053e                  _ARCFOURInitialize
                  0x00e4fe                  _ARPInit
                  0x00e518                  _ARPIsResolved
                  0x00e6c4                  _ARPProcess
                  0x00e63e                  _ARPResolve
                  0x00fbc4                  _AnnounceIP
                  0x00c252                  _Base64Decode
                  0x00c318                  _Base64Encode
                  0x00f610                  _BerkeleySNTPGetUTCSeconds
                  0x00bb36                  _BerkeleySocketInit
                  0x00ff00                  _BerkeleyTCPClientDemo
                  0x00fe14                  _BerkeleyTCPServerDemo
                  0x00f478                  _BerkeleyUDPClientDemo
                  0x00e9cc                  _BigInt
                  0x00eb90                  _BigIntAdd
                  0x00ea4c                  _BigIntCompare
                  0x00ebd4                  _BigIntCopy
                  0x00ea2a                  _BigIntMagnitude
                  0x00ea38                  _BigIntMagnitudeDifference
                  0x00ea94                  _BigIntMod
                  0x00eb38                  _BigIntMultiply
                  0x00eb6c                  _BigIntSquare
                  0x00ebb2                  _BigIntSubtract
                  0x00ebf4                  _BigIntSwapEndianness
                  0x00e9de                  _BigIntZero
                  0x0101f6                  _BusyUART2
                  0x008dee                  _CalcIPBufferChecksum
                  0x00c576                  _CalcIPChecksum
                  0x00b52c                  _DDNSForceUpdate
                  0x00b550                  _DDNSGetLastIP
                  0x00b558                  _DDNSGetLastStatus
                  0x00af3c                  _DDNSInit
                  0x00b53e                  _DDNSSetService
                  0x00af6a                  _DDNSTask
                  0x00a2e8                  _DHCPDisable
                  0x00a2fa                  _DHCPEnable
                  0x00a2ce                  _DHCPReset
                  0x00cb20                  _DHCPServerTask
                  0x00a6e2                  _DHCPTask
                  0x00c5fc                  _DNSBeginUsage
                  0x00c608                  _DNSEndUsage
                  0x00c6b2                  _DNSIsResolved
                  0x00c622                  _DNSResolve
                  0x0101aa                  _DataRdyUART2
                  0x01061e                  _Delay10us
                  0x010646                  _DelayMs
                  0x00fc2c                  _DiscoveryTask
                  0x00d100                  _DisplayIPValue
                  0x00ec08                  _DoUARTConfig
                  0x00c5cc                  _FormatNetBIOSName
                  0x00c0d6                  _GenerateRandomDWORD
                  0x00fcf2                  _GenericTCPClient
                  0x0103fe                  _GenericTCPServer
                  0x008bf2                  _GetCLKOUT
                  0x000fbc                  _HTML_DOWN_ARROW
                  0x000fbf                  _HTML_UP_ARROW
                  0x0064ca                  _HTTPCheckAuth
                  0x0064ee                  _HTTPExecuteGet
                  0x006776                  _HTTPExecutePost
                  0x0052d0                  _HTTPGetArg
                  0x0054a2                  _HTTPIncFile
                  0x0051b4                  _HTTPInit
                  0x0064a2                  _HTTPNeedsAuth
                  0x005546                  _HTTPPrint
                  0x0072e2                  _HTTPPrintIP
                  0x0051a4                  _HTTPPrint_
                  0x007016                  _HTTPPrint_btn
                  0x006fd2                  _HTTPPrint_builddate
                  0x00733c                  _HTTPPrint_config_dhcpchecked
                  0x0073ac                  _HTTPPrint_config_dns1
                  0x0073ca                  _HTTPPrint_config_dns2
                  0x007370                  _HTTPPrint_config_gw
                  0x00732c                  _HTTPPrint_config_hostname
                  0x007352                  _HTTPPrint_config_ip
                  0x0073e8                  _HTTPPrint_config_mac
                  0x00738e                  _HTTPPrint_config_subnet
                  0x00720e                  _HTTPPrint_cookiename
                  0x00751c                  _HTTPPrint_ddns_host
                  0x0074e2                  _HTTPPrint_ddns_pass
                  0x007556                  _HTTPPrint_ddns_service
                  0x00757c                  _HTTPPrint_ddns_status
                  0x0075ba                  _HTTPPrint_ddns_status_msg
                  0x0074a8                  _HTTPPrint_ddns_user
                  0x0071d8                  _HTTPPrint_hellomsg
                  0x007146                  _HTTPPrint_lcdtext
                  0x007054                  _HTTPPrint_led
                  0x0070b8                  _HTTPPrint_ledSelected
                  0x007128                  _HTTPPrint_pot
                  0x007460                  _HTTPPrint_read_comm
                  0x007494                  _HTTPPrint_reboot
                  0x007498                  _HTTPPrint_rebootaddr
                  0x00764a                  _HTTPPrint_smtps_en
                  0x00765a                  _HTTPPrint_snmp_en
                  0x00768e                  _HTTPPrint_status_fail
                  0x00766a                  _HTTPPrint_status_ok
                  0x00723e                  _HTTPPrint_uploadedmd5
                  0x007006                  _HTTPPrint_version
                  0x00747a                  _HTTPPrint_write_comm
                  0x005430                  _HTTPReadPostName
                  0x005450                  _HTTPReadPostValue
                  0x0056f2                  _HTTPServer
                  0x005262                  _HTTPURLDecode
                  0x00a13c                  _HashAddData
                  0x00f26a                  _ICMPBeginUsage
                  0x00f276                  _ICMPEndUsage
                  0x00f164                  _ICMPGetReply
                  0x00f076                  _ICMPProcess
                  0x00f130                  _ICMPSendPing
                  0x00f14a                  _ICMPSendPingToHost
                  0x00fb40                  _IPGetHeader
                  0x00fab8                  _IPPutHeader
                  0x00fa8c                  _IPSetRxBuffer
                  0x00fa76                  _LCDErase
                  0x00f982                  _LCDInit
                  0x00f9fe                  _LCDUpdate
                  0x008e7c                  _MACCalcRxChecksum
                  0x008a92                  _MACDiscardRx
                  0x008f4c                  _MACFlush
                  0x0087f2                  _MACGet
                  0x008818                  _MACGetArray
                  0x0090fe                  _MACGetFreeRxSize
                  0x009062                  _MACGetHeader
                  0x009196                  _MACInit
                  0x008bb2                  _MACIsLinked
                  0x008c58                  _MACIsMemCopyDone
                  0x009180                  _MACIsTxReady
                  0x008c6e                  _MACMemCopyAsync
                  0x008c2e                  _MACPowerDown
                  0x008c10                  _MACPowerUp
                  0x0088aa                  _MACPut
                  0x0088d8                  _MACPutArray
                  0x008a12                  _MACPutHeader
                  0x008ed8                  _MACSetReadPtr
                  0x0089f0                  _MACSetReadPtrInRx
                  0x008f12                  _MACSetWritePtr
                  0x009d2c                  _MD5AddData
                  0x009d76                  _MD5Calculate
                  0x009bb2                  _MD5Initialize
                  0x00b55c                  _MPFSClose
                  0x00b928                  _MPFSFormat
                  0x00b574                  _MPFSGet
                  0x00b5fa                  _MPFSGetArray
                  0x00b9dc                  _MPFSGetBytesRem
                  0x00b844                  _MPFSGetEndAddr
                  0x00b9fc                  _MPFSGetFilename
                  0x00b9b8                  _MPFSGetFlags
                  0x00ba58                  _MPFSGetID
                  0x00b7e0                  _MPFSGetLong
                  0x00b990                  _MPFSGetMicrotime
                  0x00ba40                  _MPFSGetPosition
                  0x00b7ee                  _MPFSGetSize
                  0x00b816                  _MPFSGetStartAddr
                  0x00b968                  _MPFSGetTimestamp
                  0x00bb1a                  _MPFSInit
                  0x00b6fc                  _MPFSOpen
                  0x00b6a2                  _MPFSOpenID
                  0x00baae                  _MPFSPutArray
                  0x00ba92                  _MPFSPutEnd
                  0x00b876                  _MPFSSeek
                  0x00e27e                  _NBNSTask
                  0x01049e                  _PingDemo
                  0x00d444                  _RSABeginUsage
                  0x00d460                  _RSAEndUsage
                  0x00d404                  _RSAInit
                  0x00d464                  _RSASetData
                  0x00d758                  _RSAStep
                  0x0105ca                  _RandomAdd
                  0x0105f2                  _RandomGet
                  0x0105be                  _RandomInit
                  0x008b54                  _ReadPHYReg
                  0x010246                  _ReadStringUART
                  0x0101b0                  _ReadUART2
                  0x010346                  _RebootTask
                  0x00a0f0                  _SHA1AddData
                  0x00a164                  _SHA1Calculate
                  0x009e70                  _SHA1Initialize
                  0x0092d0                  _SMTPBeginUsage
                  0x010278                  _SMTPDemo
                  0x0092fa                  _SMTPEndUsage
                  0x009ba8                  _SMTPFlush
                  0x009ae6                  _SMTPIsBusy
                  0x009af0                  _SMTPIsPutReady
                  0x009b04                  _SMTPPut
                  0x009b6a                  _SMTPPutArray
                  0x009bae                  _SMTPPutDone
                  0x009b8c                  _SMTPPutString
                  0x009ae2                  _SMTPSendMail
                  0x0093d2                  _SMTPTask
                  0x00aa72                  _SNMPGetNextIndex
                  0x00ad98                  _SNMPGetVar
                  0x003d02                  _SNMPInit
                  0x003d46                  _SNMPIsNotifyReady
                  0x00a96e                  _SNMPIsValidSetLen
                  0x004282                  _SNMPNotify
                  0x003d12                  _SNMPNotifyPrepare
                  0x00ab5e                  _SNMPSendTrap
                  0x00a988                  _SNMPSetVar
                  0x00456a                  _SNMPTask
                  0x00acb4                  _SNMPTrapDemo
                  0x00a90a                  _SNMPValidateCommunity
                  0x00f27a                  _SNTPClient
                  0x00f440                  _SNTPGetUTCSeconds
                  0x0076b2                  _SSLInit
                  0x0087e8                  _SSLMACAdd
                  0x007734                  _SSLMACBegin
                  0x007796                  _SSLMACCalc
                  0x0083fc                  _SSLPeriodic
                  0x007c64                  _SSLRxHandshake
                  0x0081d0                  _SSLRxRecord
                  0x008126                  _SSLStartPartialRecord
                  0x00801a                  _SSLStartSession
                  0x0083ce                  _SSLTerminate
                  0x0084a4                  _SSLTxMessage
                  0x008158                  _SSLTxRecord
                  0x001462                  _SSL_CERT
                  0x001460                  _SSL_CERT_LEN
                  0x0016ee                  _SSL_P
                  0x0016ce                  _SSL_Q
                  0x0016ae                  _SSL_dP
                  0x00168e                  _SSL_dQ
                  0x00166e                  _SSL_qInv
                  0x00d3ea                  _SaveAppConfig
                  0x008b06                  _SetCLKOUT
                  0x00f7c8                  _StackApplications
                  0x00f648                  _StackInit
                  0x00f684                  _StackTask
                  0x00c1ac                  _StringToIPAddress
                  0x0032e6                  _TCPAddSSLListener
                  0x00289e                  _TCPAdjustFIFOSize
                  0x0029ae                  _TCPDiscard
                  0x0029de                  _TCPDisconnect
                  0x002b4c                  _TCPFindArrayEx
                  0x002cbe                  _TCPFindEx
                  0x0029ca                  _TCPFlush
                  0x002d4e                  _TCPGet
                  0x002cd2                  _TCPGetArray
                  0x002506                  _TCPGetRemoteInfo
                  0x002344                  _TCPGetRxFIFOFree
                  0x002312                  _TCPGetTxFIFOFull
                  0x00251a                  _TCPInit
                  0x0022b8                  _TCPIsConnected
                  0x002328                  _TCPIsGetReady
                  0x0022c8                  _TCPIsPutReady
                  0x0023d0                  _TCPIsSSL
                  0x002a56                  _TCPOpen
                  0x00f072                  _TCPPerformanceTask
                  0x00363a                  _TCPProcess
                  0x002e94                  _TCPPut
                  0x002da6                  _TCPPutArray
                  0x002e7a                  _TCPPutString
                  0x00ef9c                  _TCPRXPerformanceTask
                  0x003302                  _TCPRequestSSLMessage
                  0x003332                  _TCPSSLDecryptMAC
                  0x00236e                  _TCPSSLGetPendingTxSize
                  0x003552                  _TCPSSLHandleIncoming
                  0x00332c                  _TCPSSLHandshakeComplete
                  0x003414                  _TCPSSLInPlaceMACEncrypt
                  0x003322                  _TCPSSLIsHandshaking
                  0x0034f0                  _TCPSSLPutRecordHeader
                  0x0021c4                  _TCPSocketInitializer
                  0x002f2a                  _TCPStartSSLServer
                  0x00ee40                  _TCPTXPerformanceTask
                  0x002f7c                  _TCPTick
                  0x0022a8                  _TCPWasReset
                  0x00dc1e                  _TelnetTask
                  0x0100a6                  _TickConvertToMilliseconds
                  0x01003e                  _TickGet
                  0x010046                  _TickGetDiv256
                  0x010076                  _TickGetDiv64K
                  0x00ffe8                  _TickInit
                  0x00f7f8                  _UART2TCPBridgeInit
                  0x00f80a                  _UART2TCPBridgeTask
                  0x00d850                  _UDPClose
                  0x00daa8                  _UDPDiscard
                  0x00d980                  _UDPFlush
                  0x00da5c                  _UDPGet
                  0x00da80                  _UDPGetArray
                  0x00dc08                  _UDPInit
                  0x00da40                  _UDPIsGetReady
                  0x00d8ee                  _UDPIsPutReady
                  0x00d86c                  _UDPOpen
                  0x00dab8                  _UDPProcess
                  0x00d918                  _UDPPut
                  0x00d93e                  _UDPPutArray
                  0x00d96a                  _UDPPutString
                  0x00d8de                  _UDPSetRxBuffer
                  0x00d8cc                  _UDPSetTxBuffer
                  0x00d868                  _UDPTask
                  0x008b1c                  _WritePHYReg
                  0x0101fe                  _WriteUART2
                  0x00e792                  _XEEBeginRead
                  0x00e79c                  _XEEBeginWrite
                  0x00e79a                  _XEEEndRead
                  0x00e986                  _XEEEndWrite
                  0x00e77a                  _XEEInit
                  0x00e870                  _XEEIsBusy
                  0x00e838                  _XEERead
                  0x00e7a4                  _XEEReadArray
                  0x00e98e                  _XEEWrite
                  0x00e9ae                  _XEEWriteArray
                  0x00cf98                  __AddressError
                  0x01066c                  __DefaultInterrupt
                  0x0005a4                  __Geterrno
                  0x00cfa2                  __StackError
                  0x0002e6                  __Stoul
                  0x0100ba                  __T1Interrupt
                  0x00f8f4                  __U2RXInterrupt
                  0x00f928                  __U2TXInterrupt
                  0x0006ba                  ___divdi3
                  0x0006f4                  ___moddi3
                  0x0007f2                  ___muldi3
                  0x0007e6                  ___mulsi3
                  0x0006a4                  ___udivdi3
                  0x0005d6                  ___udivmoddi3
                  0x0007c6                  ___udivsi3
                  0x0006b2                  ___umoddi3
                  0x00084e                  ___umuldi3
                  0x0100ce                  __addBI
                  0x01018c                  __copyBI
                  0x00022e                  __data_init
                  0x01016a                  __masBI
                  0x01011a                  __msbBI
                  0x01012a                  __mulBI
                  0x00021e                  __psv_init
                  0x000200                  __resetPRI
                  0x010160                  __sqrBI
                  0x0100ee                  __subBI
                  0x01010e                  __zeroBI
                  0x00bc4c                  _accept
                  0x00bb90                  _bind
                  0x00c4ce                  _btohexa_high
                  0x00c4e2                  _btohexa_low
                  0x00c090                  _closesocket
                  0x00bcc0                  _connect
                  0x00c058                  _gethostname
                  0x01020e                  _getsUART2
                  0x00c472                  _hexatob
                  0x000572                  _isspace
                  0x00bbca                  _listen
                  0x00cfac                  _main
                  0x000590                  _memchr
                  0x0002a6                  _memcmp
                  0x000522                  _memcpy
                  0x00040e                  _memset
                  0x0101c2                  _putsUART2
                  0x00041c                  _rand
                  0x00bf04                  _recv
                  0x00bfdc                  _recvfrom
                  0x00bd52                  _send
                  0x00be2a                  _sendto
                  0x00bb56                  _socket
                  0x0004c6                  _srand
                  0x000554                  _strcat
                  0x0004e8                  _strchr
                  0x0002c2                  _strcmp
                  0x000296                  _strcpy
                  0x00c4f4                  _stricmppgm2ram
                  0x000288                  _strlen
                  0x000530                  _strncmp
                  0x0004fa                  _strstr
                  0x00c5ae                  _strupr
                  0x00c548                  _swapl
                  0x00c536                  _swaps
                  0x000582                  _tolower
                  0x00c3d8                  _uitoa
                  0x00c414                  _ultoa

Memory Configuration

Name             Origin             Length             Attributes
data             0x000800           0x002000           a !xr
reset            0x000000           0x000004  
ivt              0x000004           0x0000fc  
aivt             0x000104           0x0000fc  
program          0x000200           0x0155fc           xr
config2          0x0157fc           0x000002  
config1          0x0157fe           0x000002  
*default*        0x000000           0xffffffff  

Linker script and memory map

LOAD Objects - TCPIP Demo App-C30\MainDemo.o
LOAD Objects - TCPIP Demo App-C30\CustomHTTPApp.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Tick.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UART2TCPBridge.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UART.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UDP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UDPPerformanceTest.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Announce.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ARP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Delay.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DHCP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DHCPs.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DNS.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DynDNS.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\FTP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Hashes.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Helpers.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\HTTP2.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\HTTP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ICMP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\IP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\LCDBlocking.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\MPFS2.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\MPFS.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\NBNS.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Reboot.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SMTP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SNMP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SNTP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SPIEEPROM.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SPIFlash.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SPIRAM.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\StackTsk.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCP.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCPPerformanceTest.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Telnet.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TFTPc.o
LOAD Objects - TCPIP Demo App-C30\CustomSNMPApp.o
LOAD Objects - TCPIP Demo App-C30\UARTConfig.o
LOAD Objects - TCPIP Demo App-C30\GenericTCPClient.o
LOAD Objects - TCPIP Demo App-C30\GenericTCPServer.o
LOAD Objects - TCPIP Demo App-C30\PingDemo.o
LOAD Objects - TCPIP Demo App-C30\SMTPDemo.o
LOAD Objects - TCPIP Demo App-C30\LegacyHTTPApp.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\BerkeleyAPI.o
LOAD Objects - TCPIP Demo App-C30\BerkeleyUDPClientDemo.o
LOAD Objects - TCPIP Demo App-C30\BerkeleyTCPClientDemo.o
LOAD Objects - TCPIP Demo App-C30\BerkeleyTCPServerDemo.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ENCX24J600.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ENC28J60.o
LOAD Objects - TCPIP Demo App-C30\CustomSSLCert.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SSL.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ARCFOUR.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\BigInt.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Random.o
LOAD ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\RSA.o
LOAD C:\Microchip Solutions\Microchip\TCPIP Stack\BigInt_helper_coff.a
LOAD C:\Microchip Solutions\Microchip\TCPIP Stack\BigInt_helper_elf.a
LOAD c:/program files/microchip/mplab c30/bin/bin/../../lib/PIC24F\libpPIC24Fxxx-coff.a
                    0x157fc                  __CONFIG2 = 0x157fc
                    0x157fe                  __CONFIG1 = 0x157fe
                    0x0004                  __IVT_BASE = 0x4
                    0x0104                  __AIVT_BASE = 0x104
                    0x0800                  __DATA_BASE = 0x800
                    0x0200                  __CODE_BASE = 0x200

.reset            0x000000          0x4
                  0x000000          0x2 SHORT 0x200 <code 337> (__reset)
                  0x000001          0x2 SHORT 0x4
                  0x000002          0x2 SHORT 0x0 ((<code 337> (__reset) >> 0x10) & 0x7f)
                  0x000003          0x2 SHORT 0x0

.text             0x000200        0x692
 *(.init)
 .init            0x000200         0x88 c:/program files/microchip/mplab c30/bin/bin/../../lib\libpic30-coff.a(crt0.o)
                  0x000200                  _resetPRI
                  0x000200                  _reset
                  0x00021e                  _psv_init
                  0x00022e                  _data_init
 *(.user_init)
 *(.handle)
 *(.libc)
 .libc            0x000288          0xe c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strlen.o)
                  0x000288                  strlen
 .libc            0x000296         0x10 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strcpy.o)
                  0x000296                  strcpy
 .libc            0x0002a6         0x1c c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memcmp.o)
                  0x0002a6                  memcmp
 .libc            0x0002c2         0x24 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strcmp.o)
                  0x0002c2                  strcmp
 .libc            0x0002e6        0x128 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xstoul.o)
                  0x0002e6                  _Stoul
 .libc            0x00040e          0xe c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memset.o)
                  0x00040e                  memset
 .libc            0x00041c         0xaa c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(rand.o)
                  0x00041c                  rand
 .libc            0x0004c6         0x22 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(srand.o)
                  0x0004c6                  srand
 .libc            0x0004e8         0x12 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strchr.o)
                  0x0004e8                  strchr
 .libc            0x0004fa         0x28 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strstr.o)
                  0x0004fa                  strstr
 .libc            0x000522          0xe c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memcpy.o)
                  0x000522                  memcpy
 .libc            0x000530         0x24 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strncmp.o)
                  0x000530                  strncmp
 .libc            0x000554         0x1e c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(strcat.o)
                  0x000554                  strcat
 .libc            0x000572         0x10 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(isspace.os)
                  0x000572                  isspace
 .libc            0x000582          0xe c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(tolower.os)
                  0x000582                  tolower
 .libc            0x000590         0x14 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(memchr.o)
                  0x000590                  memchr
 .libc            0x0005a4          0xc c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(errno.o)
                  0x0005a4                  _Geterrno
 *(.libm)
 .libm            0x0005b0        0x216 c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(divmoddi3.o)
                  0x0005d6                  __udivmoddi3
                  0x0006a4                  __udivdi3
                  0x0006b2                  __umoddi3
                  0x0006ba                  __divdi3
                  0x0006f4                  __moddi3
 .libm            0x0007c6         0x20 c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(udivsi3.o)
                  0x0007c6                  __udivsi3
 .libm            0x0007e6          0xc c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(mulsi3.o)
                  0x0007e6                  __mulsi3
 .libm            0x0007f2         0x5c c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(muldi3.o)
                  0x0007f2                  __muldi3
 .libm            0x00084e         0x44 c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a(umuldi3.o)
                  0x00084e                  __umuldi3
 *(.libdsp)
 *(.lib*)

__CONFIG2         0x0157fc          0x2
 *(__CONFIG2.sec)
 __CONFIG2.sec    0x0157fc          0x2 Objects - TCPIP Demo App-C30\MainDemo.o

__CONFIG1         0x0157fe          0x2
 *(__CONFIG1.sec)
 __CONFIG1.sec    0x0157fe          0x2 Objects - TCPIP Demo App-C30\MainDemo.o

.comment
 *(.comment)

.debug_info
 *(.debug_info)
 *(.gnu.linkonce.wi.*)

.debug_abbrev
 *(.debug_abbrev)

.debug_line
 *(.debug_line)

.debug_frame
 *(.debug_frame)

.debug_str
 *(.debug_str)

.debug_loc
 *(.debug_loc)

.debug_macinfo
 *(.debug_macinfo)

.debug_pubnames
 *(.debug_pubnames)

.debug_ranges
 *(.debug_ranges)

.debug_aranges
 *(.debug_aranges)

.ivt              0x000004         0xfc
                  0x000004          0x4 LONG 0x1066c DEFINED (__ReservedTrap0)?<code 337> (__ReservedTrap0):<code 337> (__DefaultInterrupt)
                  0x000006          0x4 LONG 0x1066c DEFINED (__OscillatorFail)?<code 337> (__OscillatorFail):<code 337> (__DefaultInterrupt)
                  0x000008          0x4 LONG 0xcf98 DEFINED (__AddressError)?<code 337> (__AddressError):<code 337> (__DefaultInterrupt)
                  0x00000a          0x4 LONG 0xcfa2 DEFINED (__StackError)?<code 337> (__StackError):<code 337> (__DefaultInterrupt)
                  0x00000c          0x4 LONG 0x1066c DEFINED (__MathError)?<code 337> (__MathError):<code 337> (__DefaultInterrupt)
                  0x00000e          0x4 LONG 0x1066c DEFINED (__ReservedTrap5)?<code 337> (__ReservedTrap5):<code 337> (__DefaultInterrupt)
                  0x000010          0x4 LONG 0x1066c DEFINED (__ReservedTrap6)?<code 337> (__ReservedTrap6):<code 337> (__DefaultInterrupt)
                  0x000012          0x4 LONG 0x1066c DEFINED (__ReservedTrap7)?<code 337> (__ReservedTrap7):<code 337> (__DefaultInterrupt)
                  0x000014          0x4 LONG 0x1066c DEFINED (__INT0Interrupt)?<code 337> (__INT0Interrupt):<code 337> (__DefaultInterrupt)
                  0x000016          0x4 LONG 0x1066c DEFINED (__IC1Interrupt)?<code 337> (__IC1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000018          0x4 LONG 0x1066c DEFINED (__OC1Interrupt)?<code 337> (__OC1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00001a          0x4 LONG 0x100ba DEFINED (__T1Interrupt)?<code 337> (__T1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00001c          0x4 LONG 0x1066c DEFINED (__Interrupt4)?<code 337> (__Interrupt4):<code 337> (__DefaultInterrupt)
                  0x00001e          0x4 LONG 0x1066c DEFINED (__IC2Interrupt)?<code 337> (__IC2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000020          0x4 LONG 0x1066c DEFINED (__OC2Interrupt)?<code 337> (__OC2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000022          0x4 LONG 0x1066c DEFINED (__T2Interrupt)?<code 337> (__T2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000024          0x4 LONG 0x1066c DEFINED (__T3Interrupt)?<code 337> (__T3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000026          0x4 LONG 0x1066c DEFINED (__SPI1ErrInterrupt)?<code 337> (__SPI1ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x000028          0x4 LONG 0x1066c DEFINED (__SPI1Interrupt)?<code 337> (__SPI1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00002a          0x4 LONG 0x1066c DEFINED (__U1RXInterrupt)?<code 337> (__U1RXInterrupt):<code 337> (__DefaultInterrupt)
                  0x00002c          0x4 LONG 0x1066c DEFINED (__U1TXInterrupt)?<code 337> (__U1TXInterrupt):<code 337> (__DefaultInterrupt)
                  0x00002e          0x4 LONG 0x1066c DEFINED (__ADC1Interrupt)?<code 337> (__ADC1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000030          0x4 LONG 0x1066c DEFINED (__Interrupt14)?<code 337> (__Interrupt14):<code 337> (__DefaultInterrupt)
                  0x000032          0x4 LONG 0x1066c DEFINED (__Interrupt15)?<code 337> (__Interrupt15):<code 337> (__DefaultInterrupt)
                  0x000034          0x4 LONG 0x1066c DEFINED (__SI2C1Interrupt)?<code 337> (__SI2C1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000036          0x4 LONG 0x1066c DEFINED (__MI2C1Interrupt)?<code 337> (__MI2C1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000038          0x4 LONG 0x1066c DEFINED (__CompInterrupt)?<code 337> (__CompInterrupt):<code 337> (__DefaultInterrupt)
                  0x00003a          0x4 LONG 0x1066c DEFINED (__CNInterrupt)?<code 337> (__CNInterrupt):<code 337> (__DefaultInterrupt)
                  0x00003c          0x4 LONG 0x1066c DEFINED (__INT1Interrupt)?<code 337> (__INT1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00003e          0x4 LONG 0x1066c DEFINED (__Interrupt21)?<code 337> (__Interrupt21):<code 337> (__DefaultInterrupt)
                  0x000040          0x4 LONG 0x1066c DEFINED (__Interrupt22)?<code 337> (__Interrupt22):<code 337> (__DefaultInterrupt)
                  0x000042          0x4 LONG 0x1066c DEFINED (__Interrupt23)?<code 337> (__Interrupt23):<code 337> (__DefaultInterrupt)
                  0x000044          0x4 LONG 0x1066c DEFINED (__Interrupt24)?<code 337> (__Interrupt24):<code 337> (__DefaultInterrupt)
                  0x000046          0x4 LONG 0x1066c DEFINED (__OC3Interrupt)?<code 337> (__OC3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000048          0x4 LONG 0x1066c DEFINED (__OC4Interrupt)?<code 337> (__OC4Interrupt):<code 337> (__DefaultInterrupt)
                  0x00004a          0x4 LONG 0x1066c DEFINED (__T4Interrupt)?<code 337> (__T4Interrupt):<code 337> (__DefaultInterrupt)
                  0x00004c          0x4 LONG 0x1066c DEFINED (__T5Interrupt)?<code 337> (__T5Interrupt):<code 337> (__DefaultInterrupt)
                  0x00004e          0x4 LONG 0x1066c DEFINED (__INT2Interrupt)?<code 337> (__INT2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000050          0x4 LONG 0xf8f4 DEFINED (__U2RXInterrupt)?<code 337> (__U2RXInterrupt):<code 337> (__DefaultInterrupt)
                  0x000052          0x4 LONG 0xf928 DEFINED (__U2TXInterrupt)?<code 337> (__U2TXInterrupt):<code 337> (__DefaultInterrupt)
                  0x000054          0x4 LONG 0x1066c DEFINED (__SPI2ErrInterrupt)?<code 337> (__SPI2ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x000056          0x4 LONG 0x1066c DEFINED (__SPI2Interrupt)?<code 337> (__SPI2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000058          0x4 LONG 0x1066c DEFINED (__Interrupt34)?<code 337> (__Interrupt34):<code 337> (__DefaultInterrupt)
                  0x00005a          0x4 LONG 0x1066c DEFINED (__Interrupt35)?<code 337> (__Interrupt35):<code 337> (__DefaultInterrupt)
                  0x00005c          0x4 LONG 0x1066c DEFINED (__Interrupt36)?<code 337> (__Interrupt36):<code 337> (__DefaultInterrupt)
                  0x00005e          0x4 LONG 0x1066c DEFINED (__IC3Interrupt)?<code 337> (__IC3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000060          0x4 LONG 0x1066c DEFINED (__IC4Interrupt)?<code 337> (__IC4Interrupt):<code 337> (__DefaultInterrupt)
                  0x000062          0x4 LONG 0x1066c DEFINED (__IC5Interrupt)?<code 337> (__IC5Interrupt):<code 337> (__DefaultInterrupt)
                  0x000064          0x4 LONG 0x1066c DEFINED (__Interrupt40)?<code 337> (__Interrupt40):<code 337> (__DefaultInterrupt)
                  0x000066          0x4 LONG 0x1066c DEFINED (__OC5Interrupt)?<code 337> (__OC5Interrupt):<code 337> (__DefaultInterrupt)
                  0x000068          0x4 LONG 0x1066c DEFINED (__Interrupt42)?<code 337> (__Interrupt42):<code 337> (__DefaultInterrupt)
                  0x00006a          0x4 LONG 0x1066c DEFINED (__Interrupt43)?<code 337> (__Interrupt43):<code 337> (__DefaultInterrupt)
                  0x00006c          0x4 LONG 0x1066c DEFINED (__Interrupt44)?<code 337> (__Interrupt44):<code 337> (__DefaultInterrupt)
                  0x00006e          0x4 LONG 0x1066c DEFINED (__PMPInterrupt)?<code 337> (__PMPInterrupt):<code 337> (__DefaultInterrupt)
                  0x000070          0x4 LONG 0x1066c DEFINED (__Interrupt46)?<code 337> (__Interrupt46):<code 337> (__DefaultInterrupt)
                  0x000072          0x4 LONG 0x1066c DEFINED (__Interrupt47)?<code 337> (__Interrupt47):<code 337> (__DefaultInterrupt)
                  0x000074          0x4 LONG 0x1066c DEFINED (__Interrupt48)?<code 337> (__Interrupt48):<code 337> (__DefaultInterrupt)
                  0x000076          0x4 LONG 0x1066c DEFINED (__SI2C2Interrupt)?<code 337> (__SI2C2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000078          0x4 LONG 0x1066c DEFINED (__MI2C2Interrupt)?<code 337> (__MI2C2Interrupt):<code 337> (__DefaultInterrupt)
                  0x00007a          0x4 LONG 0x1066c DEFINED (__Interrupt51)?<code 337> (__Interrupt51):<code 337> (__DefaultInterrupt)
                  0x00007c          0x4 LONG 0x1066c DEFINED (__Interrupt52)?<code 337> (__Interrupt52):<code 337> (__DefaultInterrupt)
                  0x00007e          0x4 LONG 0x1066c DEFINED (__INT3Interrupt)?<code 337> (__INT3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000080          0x4 LONG 0x1066c DEFINED (__INT4Interrupt)?<code 337> (__INT4Interrupt):<code 337> (__DefaultInterrupt)
                  0x000082          0x4 LONG 0x1066c DEFINED (__Interrupt55)?<code 337> (__Interrupt55):<code 337> (__DefaultInterrupt)
                  0x000084          0x4 LONG 0x1066c DEFINED (__Interrupt56)?<code 337> (__Interrupt56):<code 337> (__DefaultInterrupt)
                  0x000086          0x4 LONG 0x1066c DEFINED (__Interrupt57)?<code 337> (__Interrupt57):<code 337> (__DefaultInterrupt)
                  0x000088          0x4 LONG 0x1066c DEFINED (__Interrupt58)?<code 337> (__Interrupt58):<code 337> (__DefaultInterrupt)
                  0x00008a          0x4 LONG 0x1066c DEFINED (__Interrupt59)?<code 337> (__Interrupt59):<code 337> (__DefaultInterrupt)
                  0x00008c          0x4 LONG 0x1066c DEFINED (__Interrupt60)?<code 337> (__Interrupt60):<code 337> (__DefaultInterrupt)
                  0x00008e          0x4 LONG 0x1066c DEFINED (__Interrupt61)?<code 337> (__Interrupt61):<code 337> (__DefaultInterrupt)
                  0x000090          0x4 LONG 0x1066c DEFINED (__RTCCInterrupt)?<code 337> (__RTCCInterrupt):<code 337> (__DefaultInterrupt)
                  0x000092          0x4 LONG 0x1066c DEFINED (__Interrupt63)?<code 337> (__Interrupt63):<code 337> (__DefaultInterrupt)
                  0x000094          0x4 LONG 0x1066c DEFINED (__Interrupt64)?<code 337> (__Interrupt64):<code 337> (__DefaultInterrupt)
                  0x000096          0x4 LONG 0x1066c DEFINED (__U1ErrInterrupt)?<code 337> (__U1ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x000098          0x4 LONG 0x1066c DEFINED (__U2ErrInterrupt)?<code 337> (__U2ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x00009a          0x4 LONG 0x1066c DEFINED (__CRCInterrupt)?<code 337> (__CRCInterrupt):<code 337> (__DefaultInterrupt)
                  0x00009c          0x4 LONG 0x1066c DEFINED (__Interrupt68)?<code 337> (__Interrupt68):<code 337> (__DefaultInterrupt)
                  0x00009e          0x4 LONG 0x1066c DEFINED (__Interrupt69)?<code 337> (__Interrupt69):<code 337> (__DefaultInterrupt)
                  0x0000a0          0x4 LONG 0x1066c DEFINED (__Interrupt70)?<code 337> (__Interrupt70):<code 337> (__DefaultInterrupt)
                  0x0000a2          0x4 LONG 0x1066c DEFINED (__Interrupt71)?<code 337> (__Interrupt71):<code 337> (__DefaultInterrupt)
                  0x0000a4          0x4 LONG 0x1066c DEFINED (__Interrupt72)?<code 337> (__Interrupt72):<code 337> (__DefaultInterrupt)
                  0x0000a6          0x4 LONG 0x1066c DEFINED (__Interrupt73)?<code 337> (__Interrupt73):<code 337> (__DefaultInterrupt)
                  0x0000a8          0x4 LONG 0x1066c DEFINED (__Interrupt74)?<code 337> (__Interrupt74):<code 337> (__DefaultInterrupt)
                  0x0000aa          0x4 LONG 0x1066c DEFINED (__Interrupt75)?<code 337> (__Interrupt75):<code 337> (__DefaultInterrupt)
                  0x0000ac          0x4 LONG 0x1066c DEFINED (__Interrupt76)?<code 337> (__Interrupt76):<code 337> (__DefaultInterrupt)
                  0x0000ae          0x4 LONG 0x1066c DEFINED (__Interrupt77)?<code 337> (__Interrupt77):<code 337> (__DefaultInterrupt)
                  0x0000b0          0x4 LONG 0x1066c DEFINED (__Interrupt78)?<code 337> (__Interrupt78):<code 337> (__DefaultInterrupt)
                  0x0000b2          0x4 LONG 0x1066c DEFINED (__Interrupt79)?<code 337> (__Interrupt79):<code 337> (__DefaultInterrupt)
                  0x0000b4          0x4 LONG 0x1066c DEFINED (__Interrupt80)?<code 337> (__Interrupt80):<code 337> (__DefaultInterrupt)
                  0x0000b6          0x4 LONG 0x1066c DEFINED (__Interrupt81)?<code 337> (__Interrupt81):<code 337> (__DefaultInterrupt)
                  0x0000b8          0x4 LONG 0x1066c DEFINED (__Interrupt82)?<code 337> (__Interrupt82):<code 337> (__DefaultInterrupt)
                  0x0000ba          0x4 LONG 0x1066c DEFINED (__Interrupt83)?<code 337> (__Interrupt83):<code 337> (__DefaultInterrupt)
                  0x0000bc          0x4 LONG 0x1066c DEFINED (__Interrupt84)?<code 337> (__Interrupt84):<code 337> (__DefaultInterrupt)
                  0x0000be          0x4 LONG 0x1066c DEFINED (__Interrupt85)?<code 337> (__Interrupt85):<code 337> (__DefaultInterrupt)
                  0x0000c0          0x4 LONG 0x1066c DEFINED (__Interrupt86)?<code 337> (__Interrupt86):<code 337> (__DefaultInterrupt)
                  0x0000c2          0x4 LONG 0x1066c DEFINED (__Interrupt87)?<code 337> (__Interrupt87):<code 337> (__DefaultInterrupt)
                  0x0000c4          0x4 LONG 0x1066c DEFINED (__Interrupt88)?<code 337> (__Interrupt88):<code 337> (__DefaultInterrupt)
                  0x0000c6          0x4 LONG 0x1066c DEFINED (__Interrupt89)?<code 337> (__Interrupt89):<code 337> (__DefaultInterrupt)
                  0x0000c8          0x4 LONG 0x1066c DEFINED (__Interrupt90)?<code 337> (__Interrupt90):<code 337> (__DefaultInterrupt)
                  0x0000ca          0x4 LONG 0x1066c DEFINED (__Interrupt91)?<code 337> (__Interrupt91):<code 337> (__DefaultInterrupt)
                  0x0000cc          0x4 LONG 0x1066c DEFINED (__Interrupt92)?<code 337> (__Interrupt92):<code 337> (__DefaultInterrupt)
                  0x0000ce          0x4 LONG 0x1066c DEFINED (__Interrupt93)?<code 337> (__Interrupt93):<code 337> (__DefaultInterrupt)
                  0x0000d0          0x4 LONG 0x1066c DEFINED (__Interrupt94)?<code 337> (__Interrupt94):<code 337> (__DefaultInterrupt)
                  0x0000d2          0x4 LONG 0x1066c DEFINED (__Interrupt95)?<code 337> (__Interrupt95):<code 337> (__DefaultInterrupt)
                  0x0000d4          0x4 LONG 0x1066c DEFINED (__Interrupt96)?<code 337> (__Interrupt96):<code 337> (__DefaultInterrupt)
                  0x0000d6          0x4 LONG 0x1066c DEFINED (__Interrupt97)?<code 337> (__Interrupt97):<code 337> (__DefaultInterrupt)
                  0x0000d8          0x4 LONG 0x1066c DEFINED (__Interrupt98)?<code 337> (__Interrupt98):<code 337> (__DefaultInterrupt)
                  0x0000da          0x4 LONG 0x1066c DEFINED (__Interrupt99)?<code 337> (__Interrupt99):<code 337> (__DefaultInterrupt)
                  0x0000dc          0x4 LONG 0x1066c DEFINED (__Interrupt100)?<code 337> (__Interrupt100):<code 337> (__DefaultInterrupt)
                  0x0000de          0x4 LONG 0x1066c DEFINED (__Interrupt101)?<code 337> (__Interrupt101):<code 337> (__DefaultInterrupt)
                  0x0000e0          0x4 LONG 0x1066c DEFINED (__Interrupt102)?<code 337> (__Interrupt102):<code 337> (__DefaultInterrupt)
                  0x0000e2          0x4 LONG 0x1066c DEFINED (__Interrupt103)?<code 337> (__Interrupt103):<code 337> (__DefaultInterrupt)
                  0x0000e4          0x4 LONG 0x1066c DEFINED (__Interrupt104)?<code 337> (__Interrupt104):<code 337> (__DefaultInterrupt)
                  0x0000e6          0x4 LONG 0x1066c DEFINED (__Interrupt105)?<code 337> (__Interrupt105):<code 337> (__DefaultInterrupt)
                  0x0000e8          0x4 LONG 0x1066c DEFINED (__Interrupt106)?<code 337> (__Interrupt106):<code 337> (__DefaultInterrupt)
                  0x0000ea          0x4 LONG 0x1066c DEFINED (__Interrupt107)?<code 337> (__Interrupt107):<code 337> (__DefaultInterrupt)
                  0x0000ec          0x4 LONG 0x1066c DEFINED (__Interrupt108)?<code 337> (__Interrupt108):<code 337> (__DefaultInterrupt)
                  0x0000ee          0x4 LONG 0x1066c DEFINED (__Interrupt109)?<code 337> (__Interrupt109):<code 337> (__DefaultInterrupt)
                  0x0000f0          0x4 LONG 0x1066c DEFINED (__Interrupt110)?<code 337> (__Interrupt110):<code 337> (__DefaultInterrupt)
                  0x0000f2          0x4 LONG 0x1066c DEFINED (__Interrupt111)?<code 337> (__Interrupt111):<code 337> (__DefaultInterrupt)
                  0x0000f4          0x4 LONG 0x1066c DEFINED (__Interrupt112)?<code 337> (__Interrupt112):<code 337> (__DefaultInterrupt)
                  0x0000f6          0x4 LONG 0x1066c DEFINED (__Interrupt113)?<code 337> (__Interrupt113):<code 337> (__DefaultInterrupt)
                  0x0000f8          0x4 LONG 0x1066c DEFINED (__Interrupt114)?<code 337> (__Interrupt114):<code 337> (__DefaultInterrupt)
                  0x0000fa          0x4 LONG 0x1066c DEFINED (__Interrupt115)?<code 337> (__Interrupt115):<code 337> (__DefaultInterrupt)
                  0x0000fc          0x4 LONG 0x1066c DEFINED (__Interrupt116)?<code 337> (__Interrupt116):<code 337> (__DefaultInterrupt)
                  0x0000fe          0x4 LONG 0x1066c DEFINED (__Interrupt117)?<code 337> (__Interrupt117):<code 337> (__DefaultInterrupt)

.aivt             0x000104         0xfc
                  0x000104          0x4 LONG 0x1066c DEFINED (__AltReservedTrap0)?<code 337> (__AltReservedTrap0):DEFINED (__ReservedTrap0)?<code 337> (__ReservedTrap0):<code 337> (__DefaultInterrupt)
                  0x000106          0x4 LONG 0x1066c DEFINED (__AltOscillatorFail)?<code 337> (__AltOscillatorFail):DEFINED (__OscillatorFail)?<code 337> (__OscillatorFail):<code 337> (__DefaultInterrupt)
                  0x000108          0x4 LONG 0xcf98 DEFINED (__AltAddressError)?<code 337> (__AltAddressError):DEFINED (__AddressError)?<code 337> (__AddressError):<code 337> (__DefaultInterrupt)
                  0x00010a          0x4 LONG 0xcfa2 DEFINED (__AltStackError)?<code 337> (__AltStackError):DEFINED (__StackError)?<code 337> (__StackError):<code 337> (__DefaultInterrupt)
                  0x00010c          0x4 LONG 0x1066c DEFINED (__AltMathError)?<code 337> (__AltMathError):DEFINED (__MathError)?<code 337> (__MathError):<code 337> (__DefaultInterrupt)
                  0x00010e          0x4 LONG 0x1066c DEFINED (__AltReservedTrap5)?<code 337> (__AltReservedTrap5):DEFINED (__ReservedTrap5)?<code 337> (__ReservedTrap5):<code 337> (__DefaultInterrupt)
                  0x000110          0x4 LONG 0x1066c DEFINED (__AltReservedTrap6)?<code 337> (__AltReservedTrap6):DEFINED (__ReservedTrap6)?<code 337> (__ReservedTrap6):<code 337> (__DefaultInterrupt)
                  0x000112          0x4 LONG 0x1066c DEFINED (__AltReservedTrap7)?<code 337> (__AltReservedTrap7):DEFINED (__ReservedTrap7)?<code 337> (__ReservedTrap7):<code 337> (__DefaultInterrupt)
                  0x000114          0x4 LONG 0x1066c DEFINED (__AltINT0Interrupt)?<code 337> (__AltINT0Interrupt):DEFINED (__INT0Interrupt)?<code 337> (__INT0Interrupt):<code 337> (__DefaultInterrupt)
                  0x000116          0x4 LONG 0x1066c DEFINED (__AltIC1Interrupt)?<code 337> (__AltIC1Interrupt):DEFINED (__IC1Interrupt)?<code 337> (__IC1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000118          0x4 LONG 0x1066c DEFINED (__AltOC1Interrupt)?<code 337> (__AltOC1Interrupt):DEFINED (__OC1Interrupt)?<code 337> (__OC1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00011a          0x4 LONG 0x100ba DEFINED (__AltT1Interrupt)?<code 337> (__AltT1Interrupt):DEFINED (__T1Interrupt)?<code 337> (__T1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00011c          0x4 LONG 0x1066c DEFINED (__AltInterrupt4)?<code 337> (__AltInterrupt4):DEFINED (__Interrupt4)?<code 337> (__Interrupt4):<code 337> (__DefaultInterrupt)
                  0x00011e          0x4 LONG 0x1066c DEFINED (__AltIC2Interrupt)?<code 337> (__AltIC2Interrupt):DEFINED (__IC2Interrupt)?<code 337> (__IC2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000120          0x4 LONG 0x1066c DEFINED (__AltOC2Interrupt)?<code 337> (__AltOC2Interrupt):DEFINED (__OC2Interrupt)?<code 337> (__OC2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000122          0x4 LONG 0x1066c DEFINED (__AltT2Interrupt)?<code 337> (__AltT2Interrupt):DEFINED (__T2Interrupt)?<code 337> (__T2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000124          0x4 LONG 0x1066c DEFINED (__AltT3Interrupt)?<code 337> (__AltT3Interrupt):DEFINED (__T3Interrupt)?<code 337> (__T3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000126          0x4 LONG 0x1066c DEFINED (__AltSPI1ErrInterrupt)?<code 337> (__AltSPI1ErrInterrupt):DEFINED (__SPI1ErrInterrupt)?<code 337> (__SPI1ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x000128          0x4 LONG 0x1066c DEFINED (__AltSPI1Interrupt)?<code 337> (__AltSPI1Interrupt):DEFINED (__SPI1Interrupt)?<code 337> (__SPI1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00012a          0x4 LONG 0x1066c DEFINED (__AltU1RXInterrupt)?<code 337> (__AltU1RXInterrupt):DEFINED (__U1RXInterrupt)?<code 337> (__U1RXInterrupt):<code 337> (__DefaultInterrupt)
                  0x00012c          0x4 LONG 0x1066c DEFINED (__AltU1TXInterrupt)?<code 337> (__AltU1TXInterrupt):DEFINED (__U1TXInterrupt)?<code 337> (__U1TXInterrupt):<code 337> (__DefaultInterrupt)
                  0x00012e          0x4 LONG 0x1066c DEFINED (__AltADC1Interrupt)?<code 337> (__AltADC1Interrupt):DEFINED (__ADC1Interrupt)?<code 337> (__ADC1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000130          0x4 LONG 0x1066c DEFINED (__AltInterrupt14)?<code 337> (__AltInterrupt14):DEFINED (__Interrupt14)?<code 337> (__Interrupt14):<code 337> (__DefaultInterrupt)
                  0x000132          0x4 LONG 0x1066c DEFINED (__AltInterrupt15)?<code 337> (__AltInterrupt15):DEFINED (__Interrupt15)?<code 337> (__Interrupt15):<code 337> (__DefaultInterrupt)
                  0x000134          0x4 LONG 0x1066c DEFINED (__AltSI2C1Interrupt)?<code 337> (__AltSI2C1Interrupt):DEFINED (__SI2C1Interrupt)?<code 337> (__SI2C1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000136          0x4 LONG 0x1066c DEFINED (__AltMI2C1Interrupt)?<code 337> (__AltMI2C1Interrupt):DEFINED (__MI2C1Interrupt)?<code 337> (__MI2C1Interrupt):<code 337> (__DefaultInterrupt)
                  0x000138          0x4 LONG 0x1066c DEFINED (__AltCompInterrupt)?<code 337> (__AltCompInterrupt):DEFINED (__CompInterrupt)?<code 337> (__CompInterrupt):<code 337> (__DefaultInterrupt)
                  0x00013a          0x4 LONG 0x1066c DEFINED (__AltCNInterrupt)?<code 337> (__AltCNInterrupt):DEFINED (__CNInterrupt)?<code 337> (__CNInterrupt):<code 337> (__DefaultInterrupt)
                  0x00013c          0x4 LONG 0x1066c DEFINED (__AltINT1Interrupt)?<code 337> (__AltINT1Interrupt):DEFINED (__INT1Interrupt)?<code 337> (__INT1Interrupt):<code 337> (__DefaultInterrupt)
                  0x00013e          0x4 LONG 0x1066c DEFINED (__AltInterrupt21)?<code 337> (__AltInterrupt21):DEFINED (__Interrupt21)?<code 337> (__Interrupt21):<code 337> (__DefaultInterrupt)
                  0x000140          0x4 LONG 0x1066c DEFINED (__AltInterrupt22)?<code 337> (__AltInterrupt22):DEFINED (__Interrupt22)?<code 337> (__Interrupt22):<code 337> (__DefaultInterrupt)
                  0x000142          0x4 LONG 0x1066c DEFINED (__AltInterrupt23)?<code 337> (__AltInterrupt23):DEFINED (__Interrupt23)?<code 337> (__Interrupt23):<code 337> (__DefaultInterrupt)
                  0x000144          0x4 LONG 0x1066c DEFINED (__AltInterrupt24)?<code 337> (__AltInterrupt24):DEFINED (__Interrupt24)?<code 337> (__Interrupt24):<code 337> (__DefaultInterrupt)
                  0x000146          0x4 LONG 0x1066c DEFINED (__AltOC3Interrupt)?<code 337> (__AltOC3Interrupt):DEFINED (__OC3Interrupt)?<code 337> (__OC3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000148          0x4 LONG 0x1066c DEFINED (__AltOC4Interrupt)?<code 337> (__AltOC4Interrupt):DEFINED (__OC4Interrupt)?<code 337> (__OC4Interrupt):<code 337> (__DefaultInterrupt)
                  0x00014a          0x4 LONG 0x1066c DEFINED (__AltT4Interrupt)?<code 337> (__AltT4Interrupt):DEFINED (__T4Interrupt)?<code 337> (__T4Interrupt):<code 337> (__DefaultInterrupt)
                  0x00014c          0x4 LONG 0x1066c DEFINED (__AltT5Interrupt)?<code 337> (__AltT5Interrupt):DEFINED (__T5Interrupt)?<code 337> (__T5Interrupt):<code 337> (__DefaultInterrupt)
                  0x00014e          0x4 LONG 0x1066c DEFINED (__AltINT2Interrupt)?<code 337> (__AltINT2Interrupt):DEFINED (__INT2Interrupt)?<code 337> (__INT2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000150          0x4 LONG 0xf8f4 DEFINED (__AltU2RXInterrupt)?<code 337> (__AltU2RXInterrupt):DEFINED (__U2RXInterrupt)?<code 337> (__U2RXInterrupt):<code 337> (__DefaultInterrupt)
                  0x000152          0x4 LONG 0xf928 DEFINED (__AltU2TXInterrupt)?<code 337> (__AltU2TXInterrupt):DEFINED (__U2TXInterrupt)?<code 337> (__U2TXInterrupt):<code 337> (__DefaultInterrupt)
                  0x000154          0x4 LONG 0x1066c DEFINED (__AltSPI2ErrInterrupt)?<code 337> (__AltSPI2ErrInterrupt):DEFINED (__SPI2ErrInterrupt)?<code 337> (__SPI2ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x000156          0x4 LONG 0x1066c DEFINED (__AltSPI2Interrupt)?<code 337> (__AltSPI2Interrupt):DEFINED (__SPI2Interrupt)?<code 337> (__SPI2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000158          0x4 LONG 0x1066c DEFINED (__AltInterrupt34)?<code 337> (__AltInterrupt34):DEFINED (__Interrupt34)?<code 337> (__Interrupt34):<code 337> (__DefaultInterrupt)
                  0x00015a          0x4 LONG 0x1066c DEFINED (__AltInterrupt35)?<code 337> (__AltInterrupt35):DEFINED (__Interrupt35)?<code 337> (__Interrupt35):<code 337> (__DefaultInterrupt)
                  0x00015c          0x4 LONG 0x1066c DEFINED (__AltInterrupt36)?<code 337> (__AltInterrupt36):DEFINED (__Interrupt36)?<code 337> (__Interrupt36):<code 337> (__DefaultInterrupt)
                  0x00015e          0x4 LONG 0x1066c DEFINED (__AltIC3Interrupt)?<code 337> (__AltIC3Interrupt):DEFINED (__IC3Interrupt)?<code 337> (__IC3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000160          0x4 LONG 0x1066c DEFINED (__AltIC4Interrupt)?<code 337> (__AltIC4Interrupt):DEFINED (__IC4Interrupt)?<code 337> (__IC4Interrupt):<code 337> (__DefaultInterrupt)
                  0x000162          0x4 LONG 0x1066c DEFINED (__AltIC5Interrupt)?<code 337> (__AltIC5Interrupt):DEFINED (__IC5Interrupt)?<code 337> (__IC5Interrupt):<code 337> (__DefaultInterrupt)
                  0x000164          0x4 LONG 0x1066c DEFINED (__AltInterrupt40)?<code 337> (__AltInterrupt40):DEFINED (__Interrupt40)?<code 337> (__Interrupt40):<code 337> (__DefaultInterrupt)
                  0x000166          0x4 LONG 0x1066c DEFINED (__AltOC5Interrupt)?<code 337> (__AltOC5Interrupt):DEFINED (__OC5Interrupt)?<code 337> (__OC5Interrupt):<code 337> (__DefaultInterrupt)
                  0x000168          0x4 LONG 0x1066c DEFINED (__AltInterrupt42)?<code 337> (__AltInterrupt42):DEFINED (__Interrupt42)?<code 337> (__Interrupt42):<code 337> (__DefaultInterrupt)
                  0x00016a          0x4 LONG 0x1066c DEFINED (__AltInterrupt43)?<code 337> (__AltInterrupt43):DEFINED (__Interrupt43)?<code 337> (__Interrupt43):<code 337> (__DefaultInterrupt)
                  0x00016c          0x4 LONG 0x1066c DEFINED (__AltInterrupt44)?<code 337> (__AltInterrupt44):DEFINED (__Interrupt44)?<code 337> (__Interrupt44):<code 337> (__DefaultInterrupt)
                  0x00016e          0x4 LONG 0x1066c DEFINED (__AltPMPInterrupt)?<code 337> (__AltPMPInterrupt):DEFINED (__PMPInterrupt)?<code 337> (__PMPInterrupt):<code 337> (__DefaultInterrupt)
                  0x000170          0x4 LONG 0x1066c DEFINED (__AltInterrupt46)?<code 337> (__AltInterrupt46):DEFINED (__Interrupt46)?<code 337> (__Interrupt46):<code 337> (__DefaultInterrupt)
                  0x000172          0x4 LONG 0x1066c DEFINED (__AltInterrupt47)?<code 337> (__AltInterrupt47):DEFINED (__Interrupt47)?<code 337> (__Interrupt47):<code 337> (__DefaultInterrupt)
                  0x000174          0x4 LONG 0x1066c DEFINED (__AltInterrupt48)?<code 337> (__AltInterrupt48):DEFINED (__Interrupt48)?<code 337> (__Interrupt48):<code 337> (__DefaultInterrupt)
                  0x000176          0x4 LONG 0x1066c DEFINED (__AltSI2C2Interrupt)?<code 337> (__AltSI2C2Interrupt):DEFINED (__SI2C2Interrupt)?<code 337> (__SI2C2Interrupt):<code 337> (__DefaultInterrupt)
                  0x000178          0x4 LONG 0x1066c DEFINED (__AltMI2C2Interrupt)?<code 337> (__AltMI2C2Interrupt):DEFINED (__MI2C2Interrupt)?<code 337> (__MI2C2Interrupt):<code 337> (__DefaultInterrupt)
                  0x00017a          0x4 LONG 0x1066c DEFINED (__AltInterrupt51)?<code 337> (__AltInterrupt51):DEFINED (__Interrupt51)?<code 337> (__Interrupt51):<code 337> (__DefaultInterrupt)
                  0x00017c          0x4 LONG 0x1066c DEFINED (__AltInterrupt52)?<code 337> (__AltInterrupt52):DEFINED (__Interrupt52)?<code 337> (__Interrupt52):<code 337> (__DefaultInterrupt)
                  0x00017e          0x4 LONG 0x1066c DEFINED (__AltINT3Interrupt)?<code 337> (__AltINT3Interrupt):DEFINED (__INT3Interrupt)?<code 337> (__INT3Interrupt):<code 337> (__DefaultInterrupt)
                  0x000180          0x4 LONG 0x1066c DEFINED (__AltINT4Interrupt)?<code 337> (__AltINT4Interrupt):DEFINED (__INT4Interrupt)?<code 337> (__INT4Interrupt):<code 337> (__DefaultInterrupt)
                  0x000182          0x4 LONG 0x1066c DEFINED (__AltInterrupt55)?<code 337> (__AltInterrupt55):DEFINED (__Interrupt55)?<code 337> (__Interrupt55):<code 337> (__DefaultInterrupt)
                  0x000184          0x4 LONG 0x1066c DEFINED (__AltInterrupt56)?<code 337> (__AltInterrupt56):DEFINED (__Interrupt56)?<code 337> (__Interrupt56):<code 337> (__DefaultInterrupt)
                  0x000186          0x4 LONG 0x1066c DEFINED (__AltInterrupt57)?<code 337> (__AltInterrupt57):DEFINED (__Interrupt57)?<code 337> (__Interrupt57):<code 337> (__DefaultInterrupt)
                  0x000188          0x4 LONG 0x1066c DEFINED (__AltInterrupt58)?<code 337> (__AltInterrupt58):DEFINED (__Interrupt58)?<code 337> (__Interrupt58):<code 337> (__DefaultInterrupt)
                  0x00018a          0x4 LONG 0x1066c DEFINED (__AltInterrupt59)?<code 337> (__AltInterrupt59):DEFINED (__Interrupt59)?<code 337> (__Interrupt59):<code 337> (__DefaultInterrupt)
                  0x00018c          0x4 LONG 0x1066c DEFINED (__AltInterrupt60)?<code 337> (__AltInterrupt60):DEFINED (__Interrupt60)?<code 337> (__Interrupt60):<code 337> (__DefaultInterrupt)
                  0x00018e          0x4 LONG 0x1066c DEFINED (__AltInterrupt61)?<code 337> (__AltInterrupt61):DEFINED (__Interrupt61)?<code 337> (__Interrupt61):<code 337> (__DefaultInterrupt)
                  0x000190          0x4 LONG 0x1066c DEFINED (__AltRTCCInterrupt)?<code 337> (__AltRTCCInterrupt):DEFINED (__RTCCInterrupt)?<code 337> (__RTCCInterrupt):<code 337> (__DefaultInterrupt)
                  0x000192          0x4 LONG 0x1066c DEFINED (__AltInterrupt63)?<code 337> (__AltInterrupt63):DEFINED (__Interrupt63)?<code 337> (__Interrupt63):<code 337> (__DefaultInterrupt)
                  0x000194          0x4 LONG 0x1066c DEFINED (__AltInterrupt64)?<code 337> (__AltInterrupt64):DEFINED (__Interrupt64)?<code 337> (__Interrupt64):<code 337> (__DefaultInterrupt)
                  0x000196          0x4 LONG 0x1066c DEFINED (__AltU1ErrInterrupt)?<code 337> (__AltU1ErrInterrupt):DEFINED (__U1ErrInterrupt)?<code 337> (__U1ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x000198          0x4 LONG 0x1066c DEFINED (__AltU2ErrInterrupt)?<code 337> (__AltU2ErrInterrupt):DEFINED (__U2ErrInterrupt)?<code 337> (__U2ErrInterrupt):<code 337> (__DefaultInterrupt)
                  0x00019a          0x4 LONG 0x1066c DEFINED (__AltCRCInterrupt)?<code 337> (__AltCRCInterrupt):DEFINED (__CRCInterrupt)?<code 337> (__CRCInterrupt):<code 337> (__DefaultInterrupt)
                  0x00019c          0x4 LONG 0x1066c DEFINED (__AltInterrupt68)?<code 337> (__AltInterrupt68):DEFINED (__Interrupt68)?<code 337> (__Interrupt68):<code 337> (__DefaultInterrupt)
                  0x00019e          0x4 LONG 0x1066c DEFINED (__AltInterrupt69)?<code 337> (__AltInterrupt69):DEFINED (__Interrupt69)?<code 337> (__Interrupt69):<code 337> (__DefaultInterrupt)
                  0x0001a0          0x4 LONG 0x1066c DEFINED (__AltInterrupt70)?<code 337> (__AltInterrupt70):DEFINED (__Interrupt70)?<code 337> (__Interrupt70):<code 337> (__DefaultInterrupt)
                  0x0001a2          0x4 LONG 0x1066c DEFINED (__AltInterrupt71)?<code 337> (__AltInterrupt71):DEFINED (__Interrupt71)?<code 337> (__Interrupt71):<code 337> (__DefaultInterrupt)
                  0x0001a4          0x4 LONG 0x1066c DEFINED (__AltInterrupt72)?<code 337> (__AltInterrupt72):DEFINED (__Interrupt72)?<code 337> (__Interrupt72):<code 337> (__DefaultInterrupt)
                  0x0001a6          0x4 LONG 0x1066c DEFINED (__AltInterrupt73)?<code 337> (__AltInterrupt73):DEFINED (__Interrupt73)?<code 337> (__Interrupt73):<code 337> (__DefaultInterrupt)
                  0x0001a8          0x4 LONG 0x1066c DEFINED (__AltInterrupt74)?<code 337> (__AltInterrupt74):DEFINED (__Interrupt74)?<code 337> (__Interrupt74):<code 337> (__DefaultInterrupt)
                  0x0001aa          0x4 LONG 0x1066c DEFINED (__AltInterrupt75)?<code 337> (__AltInterrupt75):DEFINED (__Interrupt75)?<code 337> (__Interrupt75):<code 337> (__DefaultInterrupt)
                  0x0001ac          0x4 LONG 0x1066c DEFINED (__AltInterrupt76)?<code 337> (__AltInterrupt76):DEFINED (__Interrupt76)?<code 337> (__Interrupt76):<code 337> (__DefaultInterrupt)
                  0x0001ae          0x4 LONG 0x1066c DEFINED (__AltInterrupt77)?<code 337> (__AltInterrupt77):DEFINED (__Interrupt77)?<code 337> (__Interrupt77):<code 337> (__DefaultInterrupt)
                  0x0001b0          0x4 LONG 0x1066c DEFINED (__AltInterrupt78)?<code 337> (__AltInterrupt78):DEFINED (__Interrupt78)?<code 337> (__Interrupt78):<code 337> (__DefaultInterrupt)
                  0x0001b2          0x4 LONG 0x1066c DEFINED (__AltInterrupt79)?<code 337> (__AltInterrupt79):DEFINED (__Interrupt79)?<code 337> (__Interrupt79):<code 337> (__DefaultInterrupt)
                  0x0001b4          0x4 LONG 0x1066c DEFINED (__AltInterrupt80)?<code 337> (__AltInterrupt80):DEFINED (__Interrupt80)?<code 337> (__Interrupt80):<code 337> (__DefaultInterrupt)
                  0x0001b6          0x4 LONG 0x1066c DEFINED (__AltInterrupt81)?<code 337> (__AltInterrupt81):DEFINED (__Interrupt81)?<code 337> (__Interrupt81):<code 337> (__DefaultInterrupt)
                  0x0001b8          0x4 LONG 0x1066c DEFINED (__AltInterrupt82)?<code 337> (__AltInterrupt82):DEFINED (__Interrupt82)?<code 337> (__Interrupt82):<code 337> (__DefaultInterrupt)
                  0x0001ba          0x4 LONG 0x1066c DEFINED (__AltInterrupt83)?<code 337> (__AltInterrupt83):DEFINED (__Interrupt83)?<code 337> (__Interrupt83):<code 337> (__DefaultInterrupt)
                  0x0001bc          0x4 LONG 0x1066c DEFINED (__AltInterrupt84)?<code 337> (__AltInterrupt84):DEFINED (__Interrupt84)?<code 337> (__Interrupt84):<code 337> (__DefaultInterrupt)
                  0x0001be          0x4 LONG 0x1066c DEFINED (__AltInterrupt85)?<code 337> (__AltInterrupt85):DEFINED (__Interrupt85)?<code 337> (__Interrupt85):<code 337> (__DefaultInterrupt)
                  0x0001c0          0x4 LONG 0x1066c DEFINED (__AltInterrupt86)?<code 337> (__AltInterrupt86):DEFINED (__Interrupt86)?<code 337> (__Interrupt86):<code 337> (__DefaultInterrupt)
                  0x0001c2          0x4 LONG 0x1066c DEFINED (__AltInterrupt87)?<code 337> (__AltInterrupt87):DEFINED (__Interrupt87)?<code 337> (__Interrupt87):<code 337> (__DefaultInterrupt)
                  0x0001c4          0x4 LONG 0x1066c DEFINED (__AltInterrupt88)?<code 337> (__AltInterrupt88):DEFINED (__Interrupt88)?<code 337> (__Interrupt88):<code 337> (__DefaultInterrupt)
                  0x0001c6          0x4 LONG 0x1066c DEFINED (__AltInterrupt89)?<code 337> (__AltInterrupt89):DEFINED (__Interrupt89)?<code 337> (__Interrupt89):<code 337> (__DefaultInterrupt)
                  0x0001c8          0x4 LONG 0x1066c DEFINED (__AltInterrupt90)?<code 337> (__AltInterrupt90):DEFINED (__Interrupt90)?<code 337> (__Interrupt90):<code 337> (__DefaultInterrupt)
                  0x0001ca          0x4 LONG 0x1066c DEFINED (__AltInterrupt91)?<code 337> (__AltInterrupt91):DEFINED (__Interrupt91)?<code 337> (__Interrupt91):<code 337> (__DefaultInterrupt)
                  0x0001cc          0x4 LONG 0x1066c DEFINED (__AltInterrupt92)?<code 337> (__AltInterrupt92):DEFINED (__Interrupt92)?<code 337> (__Interrupt92):<code 337> (__DefaultInterrupt)
                  0x0001ce          0x4 LONG 0x1066c DEFINED (__AltInterrupt93)?<code 337> (__AltInterrupt93):DEFINED (__Interrupt93)?<code 337> (__Interrupt93):<code 337> (__DefaultInterrupt)
                  0x0001d0          0x4 LONG 0x1066c DEFINED (__AltInterrupt94)?<code 337> (__AltInterrupt94):DEFINED (__Interrupt94)?<code 337> (__Interrupt94):<code 337> (__DefaultInterrupt)
                  0x0001d2          0x4 LONG 0x1066c DEFINED (__AltInterrupt95)?<code 337> (__AltInterrupt95):DEFINED (__Interrupt95)?<code 337> (__Interrupt95):<code 337> (__DefaultInterrupt)
                  0x0001d4          0x4 LONG 0x1066c DEFINED (__AltInterrupt96)?<code 337> (__AltInterrupt96):DEFINED (__Interrupt96)?<code 337> (__Interrupt96):<code 337> (__DefaultInterrupt)
                  0x0001d6          0x4 LONG 0x1066c DEFINED (__AltInterrupt97)?<code 337> (__AltInterrupt97):DEFINED (__Interrupt97)?<code 337> (__Interrupt97):<code 337> (__DefaultInterrupt)
                  0x0001d8          0x4 LONG 0x1066c DEFINED (__AltInterrupt98)?<code 337> (__AltInterrupt98):DEFINED (__Interrupt98)?<code 337> (__Interrupt98):<code 337> (__DefaultInterrupt)
                  0x0001da          0x4 LONG 0x1066c DEFINED (__AltInterrupt99)?<code 337> (__AltInterrupt99):DEFINED (__Interrupt99)?<code 337> (__Interrupt99):<code 337> (__DefaultInterrupt)
                  0x0001dc          0x4 LONG 0x1066c DEFINED (__AltInterrupt100)?<code 337> (__AltInterrupt100):DEFINED (__Interrupt100)?<code 337> (__Interrupt100):<code 337> (__DefaultInterrupt)
                  0x0001de          0x4 LONG 0x1066c DEFINED (__AltInterrupt101)?<code 337> (__AltInterrupt101):DEFINED (__Interrupt101)?<code 337> (__Interrupt101):<code 337> (__DefaultInterrupt)
                  0x0001e0          0x4 LONG 0x1066c DEFINED (__AltInterrupt102)?<code 337> (__AltInterrupt102):DEFINED (__Interrupt102)?<code 337> (__Interrupt102):<code 337> (__DefaultInterrupt)
                  0x0001e2          0x4 LONG 0x1066c DEFINED (__AltInterrupt103)?<code 337> (__AltInterrupt103):DEFINED (__Interrupt103)?<code 337> (__Interrupt103):<code 337> (__DefaultInterrupt)
                  0x0001e4          0x4 LONG 0x1066c DEFINED (__AltInterrupt104)?<code 337> (__AltInterrupt104):DEFINED (__Interrupt104)?<code 337> (__Interrupt104):<code 337> (__DefaultInterrupt)
                  0x0001e6          0x4 LONG 0x1066c DEFINED (__AltInterrupt105)?<code 337> (__AltInterrupt105):DEFINED (__Interrupt105)?<code 337> (__Interrupt105):<code 337> (__DefaultInterrupt)
                  0x0001e8          0x4 LONG 0x1066c DEFINED (__AltInterrupt106)?<code 337> (__AltInterrupt106):DEFINED (__Interrupt106)?<code 337> (__Interrupt106):<code 337> (__DefaultInterrupt)
                  0x0001ea          0x4 LONG 0x1066c DEFINED (__AltInterrupt107)?<code 337> (__AltInterrupt107):DEFINED (__Interrupt107)?<code 337> (__Interrupt107):<code 337> (__DefaultInterrupt)
                  0x0001ec          0x4 LONG 0x1066c DEFINED (__AltInterrupt108)?<code 337> (__AltInterrupt108):DEFINED (__Interrupt108)?<code 337> (__Interrupt108):<code 337> (__DefaultInterrupt)
                  0x0001ee          0x4 LONG 0x1066c DEFINED (__AltInterrupt109)?<code 337> (__AltInterrupt109):DEFINED (__Interrupt109)?<code 337> (__Interrupt109):<code 337> (__DefaultInterrupt)
                  0x0001f0          0x4 LONG 0x1066c DEFINED (__AltInterrupt110)?<code 337> (__AltInterrupt110):DEFINED (__Interrupt110)?<code 337> (__Interrupt110):<code 337> (__DefaultInterrupt)
                  0x0001f2          0x4 LONG 0x1066c DEFINED (__AltInterrupt111)?<code 337> (__AltInterrupt111):DEFINED (__Interrupt111)?<code 337> (__Interrupt111):<code 337> (__DefaultInterrupt)
                  0x0001f4          0x4 LONG 0x1066c DEFINED (__AltInterrupt112)?<code 337> (__AltInterrupt112):DEFINED (__Interrupt112)?<code 337> (__Interrupt112):<code 337> (__DefaultInterrupt)
                  0x0001f6          0x4 LONG 0x1066c DEFINED (__AltInterrupt113)?<code 337> (__AltInterrupt113):DEFINED (__Interrupt113)?<code 337> (__Interrupt113):<code 337> (__DefaultInterrupt)
                  0x0001f8          0x4 LONG 0x1066c DEFINED (__AltInterrupt114)?<code 337> (__AltInterrupt114):DEFINED (__Interrupt114)?<code 337> (__Interrupt114):<code 337> (__DefaultInterrupt)
                  0x0001fa          0x4 LONG 0x1066c DEFINED (__AltInterrupt115)?<code 337> (__AltInterrupt115):DEFINED (__Interrupt115)?<code 337> (__Interrupt115):<code 337> (__DefaultInterrupt)
                  0x0001fc          0x4 LONG 0x1066c DEFINED (__AltInterrupt116)?<code 337> (__AltInterrupt116):DEFINED (__Interrupt116)?<code 337> (__Interrupt116):<code 337> (__DefaultInterrupt)
                  0x0001fe          0x4 LONG 0x1066c DEFINED (__AltInterrupt117)?<code 337> (__AltInterrupt117):DEFINED (__Interrupt117)?<code 337> (__Interrupt117):<code 337> (__DefaultInterrupt)
                    0x0000                  WREG0 = 0x0
                    0x0000                  _WREG0 = 0x0
                    0x0002                  WREG1 = 0x2
                    0x0002                  _WREG1 = 0x2
                    0x0004                  WREG2 = 0x4
                    0x0004                  _WREG2 = 0x4
                    0x0006                  WREG3 = 0x6
                    0x0006                  _WREG3 = 0x6
                    0x0008                  WREG4 = 0x8
                    0x0008                  _WREG4 = 0x8
                    0x000a                  WREG5 = 0xa
                    0x000a                  _WREG5 = 0xa
                    0x000c                  WREG6 = 0xc
                    0x000c                  _WREG6 = 0xc
                    0x000e                  WREG7 = 0xe
                    0x000e                  _WREG7 = 0xe
                    0x0010                  WREG8 = 0x10
                    0x0010                  _WREG8 = 0x10
                    0x0012                  WREG9 = 0x12
                    0x0012                  _WREG9 = 0x12
                    0x0014                  WREG10 = 0x14
                    0x0014                  _WREG10 = 0x14
                    0x0016                  WREG11 = 0x16
                    0x0016                  _WREG11 = 0x16
                    0x0018                  WREG12 = 0x18
                    0x0018                  _WREG12 = 0x18
                    0x001a                  WREG13 = 0x1a
                    0x001a                  _WREG13 = 0x1a
                    0x001c                  WREG14 = 0x1c
                    0x001c                  _WREG14 = 0x1c
                    0x001e                  WREG15 = 0x1e
                    0x001e                  _WREG15 = 0x1e
                    0x0020                  SPLIM = 0x20
                    0x0020                  _SPLIM = 0x20
                    0x002e                  PCL = 0x2e
                    0x002e                  _PCL = 0x2e
                    0x0030                  PCH = 0x30
                    0x0030                  _PCH = 0x30
                    0x0032                  TBLPAG = 0x32
                    0x0032                  _TBLPAG = 0x32
                    0x0034                  PSVPAG = 0x34
                    0x0034                  _PSVPAG = 0x34
                    0x0036                  RCOUNT = 0x36
                    0x0036                  _RCOUNT = 0x36
                    0x0042                  SR = 0x42
                    0x0042                  _SR = 0x42
                    0x0042                  _SRbits = 0x42
                    0x0044                  CORCON = 0x44
                    0x0044                  _CORCON = 0x44
                    0x0044                  _CORCONbits = 0x44
                    0x0052                  DISICNT = 0x52
                    0x0052                  _DISICNT = 0x52
                    0x0060                  CNEN1 = 0x60
                    0x0060                  _CNEN1 = 0x60
                    0x0060                  _CNEN1bits = 0x60
                    0x0062                  CNEN2 = 0x62
                    0x0062                  _CNEN2 = 0x62
                    0x0062                  _CNEN2bits = 0x62
                    0x0068                  CNPU1 = 0x68
                    0x0068                  _CNPU1 = 0x68
                    0x0068                  _CNPU1bits = 0x68
                    0x006a                  CNPU2 = 0x6a
                    0x006a                  _CNPU2 = 0x6a
                    0x006a                  _CNPU2bits = 0x6a
                    0x0080                  INTCON1 = 0x80
                    0x0080                  _INTCON1 = 0x80
                    0x0080                  _INTCON1bits = 0x80
                    0x0082                  INTCON2 = 0x82
                    0x0082                  _INTCON2 = 0x82
                    0x0082                  _INTCON2bits = 0x82
                    0x0084                  IFS0 = 0x84
                    0x0084                  _IFS0 = 0x84
                    0x0084                  _IFS0bits = 0x84
                    0x0086                  IFS1 = 0x86
                    0x0086                  _IFS1 = 0x86
                    0x0086                  _IFS1bits = 0x86
                    0x0088                  IFS2 = 0x88
                    0x0088                  _IFS2 = 0x88
                    0x0088                  _IFS2bits = 0x88
                    0x008a                  IFS3 = 0x8a
                    0x008a                  _IFS3 = 0x8a
                    0x008a                  _IFS3bits = 0x8a
                    0x008c                  IFS4 = 0x8c
                    0x008c                  _IFS4 = 0x8c
                    0x008c                  _IFS4bits = 0x8c
                    0x0094                  IEC0 = 0x94
                    0x0094                  _IEC0 = 0x94
                    0x0094                  _IEC0bits = 0x94
                    0x0096                  IEC1 = 0x96
                    0x0096                  _IEC1 = 0x96
                    0x0096                  _IEC1bits = 0x96
                    0x0098                  IEC2 = 0x98
                    0x0098                  _IEC2 = 0x98
                    0x0098                  _IEC2bits = 0x98
                    0x009a                  IEC3 = 0x9a
                    0x009a                  _IEC3 = 0x9a
                    0x009a                  _IEC3bits = 0x9a
                    0x009c                  IEC4 = 0x9c
                    0x009c                  _IEC4 = 0x9c
                    0x009c                  _IEC4bits = 0x9c
                    0x00a4                  IPC0 = 0xa4
                    0x00a4                  _IPC0 = 0xa4
                    0x00a4                  _IPC0bits = 0xa4
                    0x00a6                  IPC1 = 0xa6
                    0x00a6                  _IPC1 = 0xa6
                    0x00a6                  _IPC1bits = 0xa6
                    0x00a8                  IPC2 = 0xa8
                    0x00a8                  _IPC2 = 0xa8
                    0x00a8                  _IPC2bits = 0xa8
                    0x00aa                  IPC3 = 0xaa
                    0x00aa                  _IPC3 = 0xaa
                    0x00aa                  _IPC3bits = 0xaa
                    0x00ac                  IPC4 = 0xac
                    0x00ac                  _IPC4 = 0xac
                    0x00ac                  _IPC4bits = 0xac
                    0x00ae                  IPC5 = 0xae
                    0x00ae                  _IPC5 = 0xae
                    0x00ae                  _IPC5bits = 0xae
                    0x00b0                  IPC6 = 0xb0
                    0x00b0                  _IPC6 = 0xb0
                    0x00b0                  _IPC6bits = 0xb0
                    0x00b2                  IPC7 = 0xb2
                    0x00b2                  _IPC7 = 0xb2
                    0x00b2                  _IPC7bits = 0xb2
                    0x00b4                  IPC8 = 0xb4
                    0x00b4                  _IPC8 = 0xb4
                    0x00b4                  _IPC8bits = 0xb4
                    0x00b6                  IPC9 = 0xb6
                    0x00b6                  _IPC9 = 0xb6
                    0x00b6                  _IPC9bits = 0xb6
                    0x00b8                  IPC10 = 0xb8
                    0x00b8                  _IPC10 = 0xb8
                    0x00b8                  _IPC10bits = 0xb8
                    0x00ba                  IPC11 = 0xba
                    0x00ba                  _IPC11 = 0xba
                    0x00ba                  _IPC11bits = 0xba
                    0x00bc                  IPC12 = 0xbc
                    0x00bc                  _IPC12 = 0xbc
                    0x00bc                  _IPC12bits = 0xbc
                    0x00be                  IPC13 = 0xbe
                    0x00be                  _IPC13 = 0xbe
                    0x00be                  _IPC13bits = 0xbe
                    0x00c2                  IPC15 = 0xc2
                    0x00c2                  _IPC15 = 0xc2
                    0x00c2                  _IPC15bits = 0xc2
                    0x00c4                  IPC16 = 0xc4
                    0x00c4                  _IPC16 = 0xc4
                    0x00c4                  _IPC16bits = 0xc4
                    0x0100                  TMR1 = 0x100
                    0x0100                  _TMR1 = 0x100
                    0x0102                  PR1 = 0x102
                    0x0102                  _PR1 = 0x102
                    0x0104                  T1CON = 0x104
                    0x0104                  _T1CON = 0x104
                    0x0104                  _T1CONbits = 0x104
                    0x0106                  TMR2 = 0x106
                    0x0106                  _TMR2 = 0x106
                    0x0108                  TMR3HLD = 0x108
                    0x0108                  _TMR3HLD = 0x108
                    0x010a                  TMR3 = 0x10a
                    0x010a                  _TMR3 = 0x10a
                    0x010c                  PR2 = 0x10c
                    0x010c                  _PR2 = 0x10c
                    0x010e                  PR3 = 0x10e
                    0x010e                  _PR3 = 0x10e
                    0x0110                  T2CON = 0x110
                    0x0110                  _T2CON = 0x110
                    0x0110                  _T2CONbits = 0x110
                    0x0112                  T3CON = 0x112
                    0x0112                  _T3CON = 0x112
                    0x0112                  _T3CONbits = 0x112
                    0x0114                  TMR4 = 0x114
                    0x0114                  _TMR4 = 0x114
                    0x0116                  TMR5HLD = 0x116
                    0x0116                  _TMR5HLD = 0x116
                    0x0118                  TMR5 = 0x118
                    0x0118                  _TMR5 = 0x118
                    0x011a                  PR4 = 0x11a
                    0x011a                  _PR4 = 0x11a
                    0x011c                  PR5 = 0x11c
                    0x011c                  _PR5 = 0x11c
                    0x011e                  T4CON = 0x11e
                    0x011e                  _T4CON = 0x11e
                    0x011e                  _T4CONbits = 0x11e
                    0x0120                  T5CON = 0x120
                    0x0120                  _T5CON = 0x120
                    0x0120                  _T5CONbits = 0x120
                    0x0140                  IC1BUF = 0x140
                    0x0140                  _IC1BUF = 0x140
                    0x0142                  IC1CON = 0x142
                    0x0142                  _IC1CON = 0x142
                    0x0142                  _IC1CONbits = 0x142
                    0x0144                  IC2BUF = 0x144
                    0x0144                  _IC2BUF = 0x144
                    0x0146                  IC2CON = 0x146
                    0x0146                  _IC2CON = 0x146
                    0x0146                  _IC2CONbits = 0x146
                    0x0148                  IC3BUF = 0x148
                    0x0148                  _IC3BUF = 0x148
                    0x014a                  IC3CON = 0x14a
                    0x014a                  _IC3CON = 0x14a
                    0x014a                  _IC3CONbits = 0x14a
                    0x014c                  IC4BUF = 0x14c
                    0x014c                  _IC4BUF = 0x14c
                    0x014e                  IC4CON = 0x14e
                    0x014e                  _IC4CON = 0x14e
                    0x014e                  _IC4CONbits = 0x14e
                    0x0150                  IC5BUF = 0x150
                    0x0150                  _IC5BUF = 0x150
                    0x0152                  IC5CON = 0x152
                    0x0152                  _IC5CON = 0x152
                    0x0152                  _IC5CONbits = 0x152
                    0x0180                  OC1RS = 0x180
                    0x0180                  _OC1RS = 0x180
                    0x0182                  OC1R = 0x182
                    0x0182                  _OC1R = 0x182
                    0x0184                  OC1CON = 0x184
                    0x0184                  _OC1CON = 0x184
                    0x0184                  _OC1CONbits = 0x184
                    0x0186                  OC2RS = 0x186
                    0x0186                  _OC2RS = 0x186
                    0x0188                  OC2R = 0x188
                    0x0188                  _OC2R = 0x188
                    0x018a                  OC2CON = 0x18a
                    0x018a                  _OC2CON = 0x18a
                    0x018a                  _OC2CONbits = 0x18a
                    0x018c                  OC3RS = 0x18c
                    0x018c                  _OC3RS = 0x18c
                    0x018e                  OC3R = 0x18e
                    0x018e                  _OC3R = 0x18e
                    0x0190                  OC3CON = 0x190
                    0x0190                  _OC3CON = 0x190
                    0x0190                  _OC3CONbits = 0x190
                    0x0192                  OC4RS = 0x192
                    0x0192                  _OC4RS = 0x192
                    0x0194                  OC4R = 0x194
                    0x0194                  _OC4R = 0x194
                    0x0196                  OC4CON = 0x196
                    0x0196                  _OC4CON = 0x196
                    0x0196                  _OC4CONbits = 0x196
                    0x0198                  OC5RS = 0x198
                    0x0198                  _OC5RS = 0x198
                    0x019a                  OC5R = 0x19a
                    0x019a                  _OC5R = 0x19a
                    0x019c                  OC5CON = 0x19c
                    0x019c                  _OC5CON = 0x19c
                    0x019c                  _OC5CONbits = 0x19c
                    0x0200                  I2C1RCV = 0x200
                    0x0200                  _I2C1RCV = 0x200
                    0x0202                  I2C1TRN = 0x202
                    0x0202                  _I2C1TRN = 0x202
                    0x0204                  I2C1BRG = 0x204
                    0x0204                  _I2C1BRG = 0x204
                    0x0206                  I2C1CON = 0x206
                    0x0206                  _I2C1CON = 0x206
                    0x0206                  _I2C1CONbits = 0x206
                    0x0208                  I2C1STAT = 0x208
                    0x0208                  _I2C1STAT = 0x208
                    0x0208                  _I2C1STATbits = 0x208
                    0x020a                  I2C1ADD = 0x20a
                    0x020a                  _I2C1ADD = 0x20a
                    0x020c                  I2C1MSK = 0x20c
                    0x020c                  _I2C1MSK = 0x20c
                    0x0210                  I2C2RCV = 0x210
                    0x0210                  _I2C2RCV = 0x210
                    0x0212                  I2C2TRN = 0x212
                    0x0212                  _I2C2TRN = 0x212
                    0x0214                  I2C2BRG = 0x214
                    0x0214                  _I2C2BRG = 0x214
                    0x0216                  I2C2CON = 0x216
                    0x0216                  _I2C2CON = 0x216
                    0x0216                  _I2C2CONbits = 0x216
                    0x0218                  I2C2STAT = 0x218
                    0x0218                  _I2C2STAT = 0x218
                    0x0218                  _I2C2STATbits = 0x218
                    0x021a                  I2C2ADD = 0x21a
                    0x021a                  _I2C2ADD = 0x21a
                    0x021c                  I2C2MSK = 0x21c
                    0x021c                  _I2C2MSK = 0x21c
                    0x0220                  U1MODE = 0x220
                    0x0220                  _U1MODE = 0x220
                    0x0220                  _U1MODEbits = 0x220
                    0x0222                  U1STA = 0x222
                    0x0222                  _U1STA = 0x222
                    0x0222                  _U1STAbits = 0x222
                    0x0224                  U1TXREG = 0x224
                    0x0224                  _U1TXREG = 0x224
                    0x0226                  U1RXREG = 0x226
                    0x0226                  _U1RXREG = 0x226
                    0x0228                  U1BRG = 0x228
                    0x0228                  _U1BRG = 0x228
                    0x0230                  U2MODE = 0x230
                    0x0230                  _U2MODE = 0x230
                    0x0230                  _U2MODEbits = 0x230
                    0x0232                  U2STA = 0x232
                    0x0232                  _U2STA = 0x232
                    0x0232                  _U2STAbits = 0x232
                    0x0234                  U2TXREG = 0x234
                    0x0234                  _U2TXREG = 0x234
                    0x0236                  U2RXREG = 0x236
                    0x0236                  _U2RXREG = 0x236
                    0x0238                  U2BRG = 0x238
                    0x0238                  _U2BRG = 0x238
                    0x0240                  SPI1STAT = 0x240
                    0x0240                  _SPI1STAT = 0x240
                    0x0240                  _SPI1STATbits = 0x240
                    0x0242                  SPI1CON1 = 0x242
                    0x0242                  _SPI1CON1 = 0x242
                    0x0242                  _SPI1CON1bits = 0x242
                    0x0244                  SPI1CON2 = 0x244
                    0x0244                  _SPI1CON2 = 0x244
                    0x0244                  _SPI1CON2bits = 0x244
                    0x0248                  SPI1BUF = 0x248
                    0x0248                  _SPI1BUF = 0x248
                    0x0260                  SPI2STAT = 0x260
                    0x0260                  _SPI2STAT = 0x260
                    0x0260                  _SPI2STATbits = 0x260
                    0x0262                  SPI2CON1 = 0x262
                    0x0262                  _SPI2CON1 = 0x262
                    0x0262                  _SPI2CON1bits = 0x262
                    0x0264                  SPI2CON2 = 0x264
                    0x0264                  _SPI2CON2 = 0x264
                    0x0264                  _SPI2CON2bits = 0x264
                    0x0268                  SPI2BUF = 0x268
                    0x0268                  _SPI2BUF = 0x268
                    0x02c0                  TRISA = 0x2c0
                    0x02c0                  _TRISA = 0x2c0
                    0x02c0                  _TRISAbits = 0x2c0
                    0x02c2                  PORTA = 0x2c2
                    0x02c2                  _PORTA = 0x2c2
                    0x02c2                  _PORTAbits = 0x2c2
                    0x02c4                  LATA = 0x2c4
                    0x02c4                  _LATA = 0x2c4
                    0x02c4                  _LATAbits = 0x2c4
                    0x02c6                  TRISB = 0x2c6
                    0x02c6                  _TRISB = 0x2c6
                    0x02c6                  _TRISBbits = 0x2c6
                    0x02c8                  PORTB = 0x2c8
                    0x02c8                  _PORTB = 0x2c8
                    0x02c8                  _PORTBbits = 0x2c8
                    0x02ca                  LATB = 0x2ca
                    0x02ca                  _LATB = 0x2ca
                    0x02ca                  _LATBbits = 0x2ca
                    0x02cc                  TRISC = 0x2cc
                    0x02cc                  _TRISC = 0x2cc
                    0x02cc                  _TRISCbits = 0x2cc
                    0x02ce                  PORTC = 0x2ce
                    0x02ce                  _PORTC = 0x2ce
                    0x02ce                  _PORTCbits = 0x2ce
                    0x02d0                  LATC = 0x2d0
                    0x02d0                  _LATC = 0x2d0
                    0x02d0                  _LATCbits = 0x2d0
                    0x02d2                  TRISD = 0x2d2
                    0x02d2                  _TRISD = 0x2d2
                    0x02d2                  _TRISDbits = 0x2d2
                    0x02d4                  PORTD = 0x2d4
                    0x02d4                  _PORTD = 0x2d4
                    0x02d4                  _PORTDbits = 0x2d4
                    0x02d6                  LATD = 0x2d6
                    0x02d6                  _LATD = 0x2d6
                    0x02d6                  _LATDbits = 0x2d6
                    0x02d8                  TRISE = 0x2d8
                    0x02d8                  _TRISE = 0x2d8
                    0x02d8                  _TRISEbits = 0x2d8
                    0x02da                  PORTE = 0x2da
                    0x02da                  _PORTE = 0x2da
                    0x02da                  _PORTEbits = 0x2da
                    0x02dc                  LATE = 0x2dc
                    0x02dc                  _LATE = 0x2dc
                    0x02dc                  _LATEbits = 0x2dc
                    0x02de                  TRISF = 0x2de
                    0x02de                  _TRISF = 0x2de
                    0x02de                  _TRISFbits = 0x2de
                    0x02e0                  PORTF = 0x2e0
                    0x02e0                  _PORTF = 0x2e0
                    0x02e0                  _PORTFbits = 0x2e0
                    0x02e2                  LATF = 0x2e2
                    0x02e2                  _LATF = 0x2e2
                    0x02e2                  _LATFbits = 0x2e2
                    0x02e4                  TRISG = 0x2e4
                    0x02e4                  _TRISG = 0x2e4
                    0x02e4                  _TRISGbits = 0x2e4
                    0x02e6                  PORTG = 0x2e6
                    0x02e6                  _PORTG = 0x2e6
                    0x02e6                  _PORTGbits = 0x2e6
                    0x02e8                  LATG = 0x2e8
                    0x02e8                  _LATG = 0x2e8
                    0x02e8                  _LATGbits = 0x2e8
                    0x02fc                  PADCFG1 = 0x2fc
                    0x02fc                  _PADCFG1 = 0x2fc
                    0x02fc                  _PADCFG1bits = 0x2fc
                    0x0300                  ADC1BUF0 = 0x300
                    0x0300                  _ADC1BUF0 = 0x300
                    0x0302                  ADC1BUF1 = 0x302
                    0x0302                  _ADC1BUF1 = 0x302
                    0x0304                  ADC1BUF2 = 0x304
                    0x0304                  _ADC1BUF2 = 0x304
                    0x0306                  ADC1BUF3 = 0x306
                    0x0306                  _ADC1BUF3 = 0x306
                    0x0308                  ADC1BUF4 = 0x308
                    0x0308                  _ADC1BUF4 = 0x308
                    0x030a                  ADC1BUF5 = 0x30a
                    0x030a                  _ADC1BUF5 = 0x30a
                    0x030c                  ADC1BUF6 = 0x30c
                    0x030c                  _ADC1BUF6 = 0x30c
                    0x030e                  ADC1BUF7 = 0x30e
                    0x030e                  _ADC1BUF7 = 0x30e
                    0x0310                  ADC1BUF8 = 0x310
                    0x0310                  _ADC1BUF8 = 0x310
                    0x0312                  ADC1BUF9 = 0x312
                    0x0312                  _ADC1BUF9 = 0x312
                    0x0314                  ADC1BUFA = 0x314
                    0x0314                  _ADC1BUFA = 0x314
                    0x0316                  ADC1BUFB = 0x316
                    0x0316                  _ADC1BUFB = 0x316
                    0x0318                  ADC1BUFC = 0x318
                    0x0318                  _ADC1BUFC = 0x318
                    0x031a                  ADC1BUFD = 0x31a
                    0x031a                  _ADC1BUFD = 0x31a
                    0x031c                  ADC1BUFE = 0x31c
                    0x031c                  _ADC1BUFE = 0x31c
                    0x031e                  ADC1BUFF = 0x31e
                    0x031e                  _ADC1BUFF = 0x31e
                    0x0320                  AD1CON1 = 0x320
                    0x0320                  _AD1CON1 = 0x320
                    0x0320                  _AD1CON1bits = 0x320
                    0x0322                  AD1CON2 = 0x322
                    0x0322                  _AD1CON2 = 0x322
                    0x0322                  _AD1CON2bits = 0x322
                    0x0324                  AD1CON3 = 0x324
                    0x0324                  _AD1CON3 = 0x324
                    0x0324                  _AD1CON3bits = 0x324
                    0x0328                  AD1CHS = 0x328
                    0x0328                  _AD1CHS = 0x328
                    0x0328                  _AD1CHSbits = 0x328
                    0x032c                  AD1PCFG = 0x32c
                    0x032c                  _AD1PCFG = 0x32c
                    0x032c                  _AD1PCFGbits = 0x32c
                    0x0330                  AD1CSSL = 0x330
                    0x0330                  _AD1CSSL = 0x330
                    0x0330                  _AD1CSSLbits = 0x330
                    0x0600                  PMCON = 0x600
                    0x0600                  _PMCON = 0x600
                    0x0600                  _PMCONbits = 0x600
                    0x0602                  PMMODE = 0x602
                    0x0602                  _PMMODE = 0x602
                    0x0602                  _PMMODEbits = 0x602
                    0x0604                  PMADDR = 0x604
                    0x0604                  _PMADDR = 0x604
                    0x0604                  _PMADDRbits = 0x604
                    0x0604                  PMDOUT1 = 0x604
                    0x0604                  _PMDOUT1 = 0x604
                    0x0604                  _PMDOUT1bits = 0x604
                    0x0606                  PMDOUT2 = 0x606
                    0x0606                  _PMDOUT2 = 0x606
                    0x0608                  PMDIN1 = 0x608
                    0x0608                  _PMDIN1 = 0x608
                    0x060a                  PMDIN2 = 0x60a
                    0x060a                  _PMDIN2 = 0x60a
                    0x060c                  PMAEN = 0x60c
                    0x060c                  _PMAEN = 0x60c
                    0x060c                  _PMAENbits = 0x60c
                    0x060e                  PMSTAT = 0x60e
                    0x060e                  _PMSTAT = 0x60e
                    0x060e                  _PMSTATbits = 0x60e
                    0x0620                  ALRMVAL = 0x620
                    0x0620                  _ALRMVAL = 0x620
                    0x0622                  ALCFGRPT = 0x622
                    0x0622                  _ALCFGRPT = 0x622
                    0x0622                  _ALCFGRPTbits = 0x622
                    0x0624                  RTCVAL = 0x624
                    0x0624                  _RTCVAL = 0x624
                    0x0626                  RCFGCAL = 0x626
                    0x0626                  _RCFGCAL = 0x626
                    0x0626                  _RCFGCALbits = 0x626
                    0x0630                  CMCON = 0x630
                    0x0630                  _CMCON = 0x630
                    0x0630                  _CMCONbits = 0x630
                    0x0632                  CVRCON = 0x632
                    0x0632                  _CVRCON = 0x632
                    0x0632                  _CVRCONbits = 0x632
                    0x0640                  CRCCON = 0x640
                    0x0640                  _CRCCON = 0x640
                    0x0640                  _CRCCONbits = 0x640
                    0x0642                  CRCXOR = 0x642
                    0x0642                  _CRCXOR = 0x642
                    0x0642                  _CRCXORbits = 0x642
                    0x0644                  CRCDAT = 0x644
                    0x0644                  _CRCDAT = 0x644
                    0x0646                  CRCWDAT = 0x646
                    0x0646                  _CRCWDAT = 0x646
                    0x06c0                  ODCA = 0x6c0
                    0x06c0                  _ODCA = 0x6c0
                    0x06c0                  _ODCAbits = 0x6c0
                    0x06c6                  ODCB = 0x6c6
                    0x06c6                  _ODCB = 0x6c6
                    0x06c6                  _ODCBbits = 0x6c6
                    0x06cc                  ODCC = 0x6cc
                    0x06cc                  _ODCC = 0x6cc
                    0x06cc                  _ODCCbits = 0x6cc
                    0x06d2                  ODCD = 0x6d2
                    0x06d2                  _ODCD = 0x6d2
                    0x06d2                  _ODCDbits = 0x6d2
                    0x06d8                  ODCE = 0x6d8
                    0x06d8                  _ODCE = 0x6d8
                    0x06d8                  _ODCEbits = 0x6d8
                    0x06de                  ODCF = 0x6de
                    0x06de                  _ODCF = 0x6de
                    0x06de                  _ODCFbits = 0x6de
                    0x06e4                  ODCG = 0x6e4
                    0x06e4                  _ODCG = 0x6e4
                    0x06e4                  _ODCGbits = 0x6e4
                    0x0740                  RCON = 0x740
                    0x0740                  _RCON = 0x740
                    0x0740                  _RCONbits = 0x740
                    0x0742                  OSCCON = 0x742
                    0x0742                  _OSCCON = 0x742
                    0x0742                  _OSCCONbits = 0x742
                    0x0742                  OSCCONL = 0x742
                    0x0742                  _OSCCONL = 0x742
                    0x0743                  OSCCONH = 0x743
                    0x0743                  _OSCCONH = 0x743
                    0x0744                  CLKDIV = 0x744
                    0x0744                  _CLKDIV = 0x744
                    0x0744                  _CLKDIVbits = 0x744
                    0x0748                  OSCTUN = 0x748
                    0x0748                  _OSCTUN = 0x748
                    0x0748                  _OSCTUNbits = 0x748
                    0x0760                  NVMCON = 0x760
                    0x0760                  _NVMCON = 0x760
                    0x0760                  _NVMCONbits = 0x760
                    0x0766                  NVMKEY = 0x766
                    0x0766                  _NVMKEY = 0x766
                    0x0770                  PMD1 = 0x770
                    0x0770                  _PMD1 = 0x770
                    0x0770                  _PMD1bits = 0x770
                    0x0772                  PMD2 = 0x772
                    0x0772                  _PMD2 = 0x772
                    0x0772                  _PMD2bits = 0x772
                    0x0774                  PMD3 = 0x774
                    0x0774                  _PMD3 = 0x774
                    0x0774                  _PMD3bits = 0x774
                    0x0140                  IC1 = 0x140
                    0x0140                  _IC1 = 0x140
                    0x0144                  IC2 = 0x144
                    0x0144                  _IC2 = 0x144
                    0x0148                  IC3 = 0x148
                    0x0148                  _IC3 = 0x148
                    0x014c                  IC4 = 0x14c
                    0x014c                  _IC4 = 0x14c
                    0x0150                  IC5 = 0x150
                    0x0150                  _IC5 = 0x150
                    0x0180                  OC1 = 0x180
                    0x0180                  _OC1 = 0x180
                    0x0186                  OC2 = 0x186
                    0x0186                  _OC2 = 0x186
                    0x018c                  OC3 = 0x18c
                    0x018c                  _OC3 = 0x18c
                    0x0192                  OC4 = 0x192
                    0x0192                  _OC4 = 0x192
                    0x0198                  OC5 = 0x198
                    0x0198                  _OC5 = 0x198
                    0x0240                  SPI1 = 0x240
                    0x0240                  _SPI1 = 0x240
                    0x0260                  SPI2 = 0x260
                    0x0260                  _SPI2 = 0x260
                    0x0220                  UART1 = 0x220
                    0x0220                  _UART1 = 0x220
                    0x0230                  UART2 = 0x230
                    0x0230                  _UART2 = 0x230
                    0x0001                  __MPLAB_BUILD = 0x1
START GROUP
LOAD c:/program files/microchip/mplab c30/bin/bin/../../lib\libpic30-coff.a
LOAD c:/program files/microchip/mplab c30/bin/bin/../../lib\libm-coff.a
LOAD c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a
END GROUP
OUTPUT(TCPIP Demo App-C30.cof coff-pic30)
LOAD data_init
LOAD default_isr

.nbss               0x0800        0x65a
 .nbss              0x0800        0x220 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SSL.o
                    0x0800                  isBufferUsed
                    0x0802                  isHashUsed
                    0x0804                  isStubUsed
                    0x0806                  ptrHS
                    0x0808                  sslSessionStubs
                    0x0818                  sslSession
                    0x0868                  sslHash
                    0x08c2                  sslBuffer
 .nbss              0x0a20        0x1d8 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCP.o
 .nbss              0x0bf8         0xc8 Objects - TCPIP Demo App-C30\CustomHTTPApp.o
 .nbss              0x0cc0         0x98 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UDP.o
                    0x0cc0                  UDPRxCount
                    0x0cc2                  UDPTxCount
                    0x0cc4                  activeUDPSocket
                    0x0cc6                  UDPSocketInfo
 .nbss              0x0d58         0x8c ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\HTTP2.o
                    0x0d58                  curHTTPID
                    0x0d5a                  httpStubs
                    0x0d62                  curHTTP
 .nbss              0x0de4         0x76 Objects - TCPIP Demo App-C30\MainDemo.o
                    0x0de8                  AppConfig
                    0x0e51                  AN0String

.ndata              0x0e5a         0x72
 .ndata             0x0e5a         0x72 Objects - TCPIP Demo App-C30\BerkeleyTCPClientDemo.o

.nbss               0x0ecc        0x1ee
 .nbss              0x0ecc         0x70 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\MPFS2.o
                    0x0ecc                  lastRead
 .nbss              0x0f3c         0x70 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Random.o
 .nbss              0x0fac         0x66 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\BerkeleyAPI.o
 .nbss              0x1012         0x54 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UART2TCPBridge.o
 .nbss              0x1066         0x54 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\RSA.o
                    0x107c                  qInv
                    0x1084                  dQ
                    0x108c                  dP
                    0x1094                  Q
                    0x109c                  P

.ndata              0x10ba         0x98
 .ndata             0x10ba         0x50 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\HTTP2.o
 .ndata             0x110a         0x48 Objects - TCPIP Demo App-C30\SMTPDemo.o

.nbss               0x1152        0x130
 .nbss              0x1152         0x40 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Hashes.o
                    0x1152                  lastBlock
 .nbss              0x1192         0x3a ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DynDNS.o
                    0x11b0                  DDNSClient
 .nbss              0x11cc         0x3a ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SMTP.o
                    0x11e0                  SMTPClient
 .nbss              0x1206         0x2e ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SNMP.o
                    0x1214                  snmpReqVarErrStatus
 .nbss              0x1234         0x28 Objects - TCPIP Demo App-C30\BerkeleyUDPClientDemo.o
 .nbss              0x125c         0x26 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SPIEEPROM.o

.ndata              0x1282         0x26
 .ndata             0x1282         0x26 Objects - TCPIP Demo App-C30\CustomSNMPApp.o
                    0x1282                  trapInfo
                    0x12a4                  gSpecificTrapNotification
                    0x12a5                  gGenericTrapNotification
                    0x12a6                  gOIDCorrespondingSnmpMibID
                    0x12a7                  gSendTrapFlag

.nbss               0x12a8         0x22
 .nbss              0x12a8         0x22 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DHCP.o

.ndata              0x12ca         0x22
 .ndata             0x12ca         0x22 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DynDNS.o
                    0x12ca                  ddnsServiceHosts

.nbss               0x12ec         0xaa
 .nbss              0x12ec         0x22 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\LCDBlocking.o
                    0x12ec                  LCDText
 .nbss              0x130e         0x20 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCPPerformanceTest.o
 .nbss              0x132e         0x20 Objects - TCPIP Demo App-C30\CustomSNMPApp.o
 .nbss              0x134e         0x1a ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SNTP.o
 .nbss              0x1368         0x18 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DNS.o
 .nbss              0x1380         0x16 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ARP.o

.ndata              0x1396         0x16
 .ndata             0x1396         0x16 Objects - TCPIP Demo App-C30\GenericTCPClient.o

.nbss               0x13ac         0x4e
 .nbss              0x13ac         0x14 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ICMP.o
 .nbss              0x13c0         0x14 Objects - TCPIP Demo App-C30\BerkeleyTCPServerDemo.o
 .nbss              0x13d4         0x10 Objects - TCPIP Demo App-C30\BerkeleyTCPClientDemo.o
 .nbss              0x13e4          0xc ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\StackTsk.o
                    0x13e4                  remoteNode
 .nbss              0x13f0          0xa ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Tick.o

.ndata              0x13fa          0xa
 .ndata             0x13fa          0xa ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UART2TCPBridge.o

.nbss               0x1404         0x18
 .nbss              0x1404          0x8 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DHCPs.o
 .nbss              0x140c          0x8 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Telnet.o
 .nbss              0x1414          0x8 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ENC28J60.o

.ndata              0x141c          0x6
 .ndata             0x141c          0x6 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DHCP.o
                    0x141c                  DHCPBindCount
                    0x141d                  DHCPFlags
                    0x141e                  smDHCPState

.nbss               0x1422          0xc
 .nbss              0x1422          0x6 Objects - TCPIP Demo App-C30\PingDemo.o
 .nbss              0x1428          0x6 Objects - TCPIP Demo App-C30\SMTPDemo.o

.ndata              0x142e          0x4
 .ndata             0x142e          0x4 Objects - TCPIP Demo App-C30\MainDemo.o
                    0x142e                  myDHCPBindCount
                    0x1430                  __C30_UART

.nbss               0x1432          0x4
 .nbss              0x1432          0x4 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Announce.o

.ndata              0x1436          0x4
 .ndata             0x1436          0x4 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DNS.o

.nbss               0x143a         0x10
 .nbss              0x143a          0x4 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\IP.o
 .nbss              0x143e          0x4 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\NBNS.o
 .nbss              0x1442          0x4 Objects - TCPIP Demo App-C30\GenericTCPClient.o
 .nbss              0x1446          0x4 Objects - TCPIP Demo App-C30\GenericTCPServer.o

.ndata              0x144a          0x6
 .ndata             0x144a          0x4 Objects - TCPIP Demo App-C30\BerkeleyTCPServerDemo.o
 .ndata             0x144e          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UDP.o

_018770704a24403d
                    0x1450          0x2
 _018770704a24403d
                    0x1450          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UDP.o

.ndata              0x1452          0x2
 .ndata             0x1452          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DHCPs.o
                    0x1452                  bDHCPServerEnabled

_0188b5404a244046
                    0x1454          0x2
 _0188b5404a244046
                    0x1454          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DNS.o

.ndata              0x1456          0x8
 .ndata             0x1456          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Reboot.o
 .ndata             0x1458          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SMTP.o
 .ndata             0x145a          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SNMP.o
 .ndata             0x145c          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCP.o

_018aebd04a244061
                    0x145e          0x2
 _018aebd04a244061
                    0x145e          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCP.o

.ndata              0x1460          0x6
 .ndata             0x1460          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCPPerformanceTest.o
 .ndata             0x1462          0x2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\BerkeleyAPI.o
 .ndata             0x1464          0x2 Objects - TCPIP Demo App-C30\BerkeleyUDPClientDemo.o

.bss                0x1466         0x88
 .bss               0x1466         0x88 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(rand.o)

.data               0x14ee         0x4a
 .data              0x14ee         0x4a c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(xstoul.o)

.bss                0x1538          0xc
 .bss               0x1538          0xc C:\Microchip Solutions\Microchip\TCPIP Stack\BigInt_helper_coff.a(BigInt_helper.o)
                    0x1538                  _iA
                    0x153a                  _xA
                    0x153c                  _iB
                    0x153e                  _xB
                    0x1540                  _iR
                    0x1542                  _wC

.data               0x1544          0xe
 .data              0x1544          0xa c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(rand.o)
                    0x1544                  _Tls_setup__Randseed
                    0x1546                  _Randseed
                    0x154a                  _Tls_setup__Randinit
                    0x154c                  _Randinit
 .data              0x154e          0x4 c:/program files/microchip/mplab c30/bin/bin/../../lib\libc-coff.a(errno.o)
                    0x154e                  _Tls_setup_errno
                    0x1550                  errno

.const              0x8892       0x19dc load address 0x000892  
 .const             0x8892        0x72a ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\HTTP2.o
 .const             0x8fbc        0x4a4 Objects - TCPIP Demo App-C30\CustomHTTPApp.o
                    0x8fbc                  HTML_DOWN_ARROW
                    0x8fbf                  HTML_UP_ARROW
 .const             0x9460        0x2ae Objects - TCPIP Demo App-C30\CustomSSLCert.o
                    0x9460                  SSL_CERT_LEN
                    0x9462                  SSL_CERT
                    0x966e                  SSL_qInv
                    0x968e                  SSL_dQ
                    0x96ae                  SSL_dP
                    0x96ce                  SSL_Q
                    0x96ee                  SSL_P
 .const             0x970e        0x1fe Objects - TCPIP Demo App-C30\UARTConfig.o
 .const             0x990c        0x1c2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Telnet.o
 .const             0x9ace        0x19a ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DynDNS.o
 .const             0x9c68        0x140 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Hashes.o
 .const             0x9da8        0x12e Objects - TCPIP Demo App-C30\BerkeleyTCPClientDemo.o
 .const             0x9ed6         0xb8 Objects - TCPIP Demo App-C30\MainDemo.o
 .const             0x9f8e         0x8e Objects - TCPIP Demo App-C30\GenericTCPClient.o
 .const             0xa01c         0x86 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SMTP.o
 .const             0xa0a2         0x58 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCPPerformanceTest.o
 .const             0xa0fa         0x4a Objects - TCPIP Demo App-C30\SMTPDemo.o
 .const             0xa144         0x42 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SSL.o
 .const             0xa186         0x3e Objects - TCPIP Demo App-C30\PingDemo.o
 .const             0xa1c4         0x36 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCP.o
                    0xa1c4                  TCPSocketInitializer
 .const             0xa1fa         0x22 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SNMP.o
 .const             0xa21c         0x1c ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Announce.o
 .const             0xa238         0x12 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Reboot.o
 .const             0xa24a          0xe ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SNTP.o
 .const             0xa258          0xe Objects - TCPIP Demo App-C30\BerkeleyUDPClientDemo.o
 .const             0xa266          0x8 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\MPFS2.o

.text             0x00226e       0x1a94
 .text            0x00226e       0x1a94 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCP.o
                  0x0022a8                  TCPWasReset
                  0x0022b8                  TCPIsConnected
                  0x0022c8                  TCPIsPutReady
                  0x002312                  TCPGetTxFIFOFull
                  0x002328                  TCPIsGetReady
                  0x002344                  TCPGetRxFIFOFree
                  0x00236e                  TCPSSLGetPendingTxSize
                  0x0023d0                  TCPIsSSL
                  0x002506                  TCPGetRemoteInfo
                  0x00251a                  TCPInit
                  0x00289e                  TCPAdjustFIFOSize
                  0x0029ae                  TCPDiscard
                  0x0029ca                  TCPFlush
                  0x0029de                  TCPDisconnect
                  0x002a56                  TCPOpen
                  0x002b4c                  TCPFindArrayEx
                  0x002cbe                  TCPFindEx
                  0x002cd2                  TCPGetArray
                  0x002d4e                  TCPGet
                  0x002da6                  TCPPutArray
                  0x002e7a                  TCPPutString
                  0x002e94                  TCPPut
                  0x002f2a                  TCPStartSSLServer
                  0x002f7c                  TCPTick
                  0x0032e6                  TCPAddSSLListener
                  0x003302                  TCPRequestSSLMessage
                  0x003322                  TCPSSLIsHandshaking
                  0x00332c                  TCPSSLHandshakeComplete
                  0x003332                  TCPSSLDecryptMAC
                  0x003414                  TCPSSLInPlaceMACEncrypt
                  0x0034f0                  TCPSSLPutRecordHeader
                  0x003552                  TCPSSLHandleIncoming
                  0x00363a                  TCPProcess

.text             0x003d02       0x14a2
 .text            0x003d02       0x14a2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SNMP.o
                  0x003d02                  SNMPInit
                  0x003d12                  SNMPNotifyPrepare
                  0x003d46                  SNMPIsNotifyReady
                  0x004282                  SNMPNotify
                  0x00456a                  SNMPTask

.text             0x0051a4       0x12fe
 .text            0x0051a4       0x12fe ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\HTTP2.o
                  0x0051a4                  HTTPPrint_
                  0x0051b4                  HTTPInit
                  0x005262                  HTTPURLDecode
                  0x0052d0                  HTTPGetArg
                  0x005430                  HTTPReadPostName
                  0x005450                  HTTPReadPostValue
                  0x0054a2                  HTTPIncFile
                  0x005546                  HTTPPrint
                  0x0056f2                  HTTPServer

.text             0x0064a2       0x1210
 .text            0x0064a2       0x1210 Objects - TCPIP Demo App-C30\CustomHTTPApp.o
                  0x0064a2                  HTTPNeedsAuth
                  0x0064ca                  HTTPCheckAuth
                  0x0064ee                  HTTPExecuteGet
                  0x006776                  HTTPExecutePost
                  0x006fd2                  HTTPPrint_builddate
                  0x007006                  HTTPPrint_version
                  0x007016                  HTTPPrint_btn
                  0x007054                  HTTPPrint_led
                  0x0070b8                  HTTPPrint_ledSelected
                  0x007128                  HTTPPrint_pot
                  0x007146                  HTTPPrint_lcdtext
                  0x0071d8                  HTTPPrint_hellomsg
                  0x00720e                  HTTPPrint_cookiename
                  0x00723e                  HTTPPrint_uploadedmd5
                  0x0072e2                  HTTPPrintIP
                  0x00732c                  HTTPPrint_config_hostname
                  0x00733c                  HTTPPrint_config_dhcpchecked
                  0x007352                  HTTPPrint_config_ip
                  0x007370                  HTTPPrint_config_gw
                  0x00738e                  HTTPPrint_config_subnet
                  0x0073ac                  HTTPPrint_config_dns1
                  0x0073ca                  HTTPPrint_config_dns2
                  0x0073e8                  HTTPPrint_config_mac
                  0x007460                  HTTPPrint_read_comm
                  0x00747a                  HTTPPrint_write_comm
                  0x007494                  HTTPPrint_reboot
                  0x007498                  HTTPPrint_rebootaddr
                  0x0074a8                  HTTPPrint_ddns_user
                  0x0074e2                  HTTPPrint_ddns_pass
                  0x00751c                  HTTPPrint_ddns_host
                  0x007556                  HTTPPrint_ddns_service
                  0x00757c                  HTTPPrint_ddns_status
                  0x0075ba                  HTTPPrint_ddns_status_msg
                  0x00764a                  HTTPPrint_smtps_en
                  0x00765a                  HTTPPrint_snmp_en
                  0x00766a                  HTTPPrint_status_ok
                  0x00768e                  HTTPPrint_status_fail

.text             0x0076b2       0x1140
 .text            0x0076b2       0x1140 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SSL.o
                  0x0076b2                  SSLInit
                  0x007734                  SSLMACBegin
                  0x007796                  SSLMACCalc
                  0x007c64                  SSLRxHandshake
                  0x00801a                  SSLStartSession
                  0x008126                  SSLStartPartialRecord
                  0x008158                  SSLTxRecord
                  0x0081d0                  SSLRxRecord
                  0x0083ce                  SSLTerminate
                  0x0083fc                  SSLPeriodic
                  0x0084a4                  SSLTxMessage
                  0x0087e8                  SSLMACAdd

.text             0x0087f2        0xade
 .text            0x0087f2        0xade ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ENC28J60.o
                  0x0087f2                  MACGet
                  0x008818                  MACGetArray
                  0x0088aa                  MACPut
                  0x0088d8                  MACPutArray
                  0x0089f0                  MACSetReadPtrInRx
                  0x008a12                  MACPutHeader
                  0x008a92                  MACDiscardRx
                  0x008b06                  SetCLKOUT
                  0x008b1c                  WritePHYReg
                  0x008b54                  ReadPHYReg
                  0x008bb2                  MACIsLinked
                  0x008bf2                  GetCLKOUT
                  0x008c10                  MACPowerUp
                  0x008c2e                  MACPowerDown
                  0x008c58                  MACIsMemCopyDone
                  0x008c6e                  MACMemCopyAsync
                  0x008dee                  CalcIPBufferChecksum
                  0x008e7c                  MACCalcRxChecksum
                  0x008ed8                  MACSetReadPtr
                  0x008f12                  MACSetWritePtr
                  0x008f4c                  MACFlush
                  0x009062                  MACGetHeader
                  0x0090fe                  MACGetFreeRxSize
                  0x009180                  MACIsTxReady
                  0x009196                  MACInit

.text             0x0092d0        0x8e2
 .text            0x0092d0        0x8e2 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SMTP.o
                  0x0092d0                  SMTPBeginUsage
                  0x0092fa                  SMTPEndUsage
                  0x0093d2                  SMTPTask
                  0x009ae2                  SMTPSendMail
                  0x009ae6                  SMTPIsBusy
                  0x009af0                  SMTPIsPutReady
                  0x009b04                  SMTPPut
                  0x009b6a                  SMTPPutArray
                  0x009b8c                  SMTPPutString
                  0x009ba8                  SMTPFlush
                  0x009bae                  SMTPPutDone

.text             0x009bb2        0x71c
 .text            0x009bb2        0x71c ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Hashes.o
                  0x009bb2                  MD5Initialize
                  0x009d2c                  MD5AddData
                  0x009d76                  MD5Calculate
                  0x009e70                  SHA1Initialize
                  0x00a0f0                  SHA1AddData
                  0x00a13c                  HashAddData
                  0x00a164                  SHA1Calculate

.text             0x00a2ce        0x63c
 .text            0x00a2ce        0x63c ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DHCP.o
                  0x00a2ce                  DHCPReset
                  0x00a2e8                  DHCPDisable
                  0x00a2fa                  DHCPEnable
                  0x00a6e2                  DHCPTask

.text             0x00a90a        0x632
 .text            0x00a90a        0x632 Objects - TCPIP Demo App-C30\CustomSNMPApp.o
                  0x00a90a                  SNMPValidateCommunity
                  0x00a96e                  SNMPIsValidSetLen
                  0x00a988                  SNMPSetVar
                  0x00aa72                  SNMPGetNextIndex
                  0x00ab5e                  SNMPSendTrap
                  0x00acb4                  SNMPTrapDemo
                  0x00ad98                  SNMPGetVar

.text             0x00af3c        0x620
 .text            0x00af3c        0x620 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DynDNS.o
                  0x00af3c                  DDNSInit
                  0x00af6a                  DDNSTask
                  0x00b52c                  DDNSForceUpdate
                  0x00b53e                  DDNSSetService
                  0x00b550                  DDNSGetLastIP
                  0x00b558                  DDNSGetLastStatus

.text             0x00b55c        0x5da
 .text            0x00b55c        0x5da ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\MPFS2.o
                  0x00b55c                  MPFSClose
                  0x00b574                  MPFSGet
                  0x00b5fa                  MPFSGetArray
                  0x00b6a2                  MPFSOpenID
                  0x00b6fc                  MPFSOpen
                  0x00b7e0                  MPFSGetLong
                  0x00b7ee                  MPFSGetSize
                  0x00b816                  MPFSGetStartAddr
                  0x00b844                  MPFSGetEndAddr
                  0x00b876                  MPFSSeek
                  0x00b928                  MPFSFormat
                  0x00b968                  MPFSGetTimestamp
                  0x00b990                  MPFSGetMicrotime
                  0x00b9b8                  MPFSGetFlags
                  0x00b9dc                  MPFSGetBytesRem
                  0x00b9fc                  MPFSGetFilename
                  0x00ba40                  MPFSGetPosition
                  0x00ba58                  MPFSGetID
                  0x00ba92                  MPFSPutEnd
                  0x00baae                  MPFSPutArray
                  0x00bb1a                  MPFSInit

.text             0x00bb36        0x5a0
 .text            0x00bb36        0x5a0 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\BerkeleyAPI.o
                  0x00bb36                  BerkeleySocketInit
                  0x00bb56                  socket
                  0x00bb90                  bind
                  0x00bbca                  listen
                  0x00bc4c                  accept
                  0x00bcc0                  connect
                  0x00bd52                  send
                  0x00be2a                  sendto
                  0x00bf04                  recv
                  0x00bfdc                  recvfrom
                  0x00c058                  gethostname
                  0x00c090                  closesocket

.text             0x00c0d6        0x526
 .text            0x00c0d6        0x526 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Helpers.o
                  0x00c0d6                  GenerateRandomDWORD
                  0x00c1ac                  StringToIPAddress
                  0x00c252                  Base64Decode
                  0x00c318                  Base64Encode
                  0x00c3d8                  uitoa
                  0x00c414                  ultoa
                  0x00c472                  hexatob
                  0x00c4ce                  btohexa_high
                  0x00c4e2                  btohexa_low
                  0x00c4f4                  stricmppgm2ram
                  0x00c536                  swaps
                  0x00c548                  swapl
                  0x00c576                  CalcIPChecksum
                  0x00c5ae                  strupr
                  0x00c5cc                  FormatNetBIOSName

.text             0x00c5fc        0x524
 .text            0x00c5fc        0x524 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DNS.o
                  0x00c5fc                  DNSBeginUsage
                  0x00c608                  DNSEndUsage
                  0x00c622                  DNSResolve
                  0x00c6b2                  DNSIsResolved

.text             0x00cb20        0x478
 .text            0x00cb20        0x478 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\DHCPs.o
                  0x00cb20                  DHCPServerTask

.text             0x00cf98        0x46c
 .text            0x00cf98        0x46c Objects - TCPIP Demo App-C30\MainDemo.o
                  0x00cf98                  _AddressError
                  0x00cfa2                  _StackError
                  0x00cfac                  main
                  0x00d100                  DisplayIPValue
                  0x00d3ea                  SaveAppConfig

.text             0x00d404        0x44c
 .text            0x00d404        0x44c ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\RSA.o
                  0x00d404                  RSAInit
                  0x00d444                  RSABeginUsage
                  0x00d460                  RSAEndUsage
                  0x00d464                  RSASetData
                  0x00d758                  RSAStep

.text             0x00d850        0x3ce
 .text            0x00d850        0x3ce ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UDP.o
                  0x00d850                  UDPClose
                  0x00d868                  UDPTask
                  0x00d86c                  UDPOpen
                  0x00d8cc                  UDPSetTxBuffer
                  0x00d8de                  UDPSetRxBuffer
                  0x00d8ee                  UDPIsPutReady
                  0x00d918                  UDPPut
                  0x00d93e                  UDPPutArray
                  0x00d96a                  UDPPutString
                  0x00d980                  UDPFlush
                  0x00da40                  UDPIsGetReady
                  0x00da5c                  UDPGet
                  0x00da80                  UDPGetArray
                  0x00daa8                  UDPDiscard
                  0x00dab8                  UDPProcess
                  0x00dc08                  UDPInit

.text             0x00dc1e        0x382
 .text            0x00dc1e        0x382 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Telnet.o
                  0x00dc1e                  TelnetTask

.dinit            0x00dfa0        0x2de
 .dinit           0x00dfa0        0x2de data_init

.text             0x00e27e        0x280
 .text            0x00e27e        0x280 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\NBNS.o
                  0x00e27e                  NBNSTask

.text             0x00e4fe        0x27c
 .text            0x00e4fe        0x27c ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ARP.o
                  0x00e4fe                  ARPInit
                  0x00e518                  ARPIsResolved
                  0x00e63e                  ARPResolve
                  0x00e6c4                  ARPProcess

.text             0x00e77a        0x252
 .text            0x00e77a        0x252 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SPIEEPROM.o
                  0x00e77a                  XEEInit
                  0x00e792                  XEEBeginRead
                  0x00e79a                  XEEEndRead
                  0x00e79c                  XEEBeginWrite
                  0x00e7a4                  XEEReadArray
                  0x00e838                  XEERead
                  0x00e870                  XEEIsBusy
                  0x00e986                  XEEEndWrite
                  0x00e98e                  XEEWrite
                  0x00e9ae                  XEEWriteArray

.text             0x00e9cc        0x23c
 .text            0x00e9cc        0x23c ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\BigInt.o
                  0x00e9cc                  BigInt
                  0x00e9de                  BigIntZero
                  0x00ea2a                  BigIntMagnitude
                  0x00ea38                  BigIntMagnitudeDifference
                  0x00ea4c                  BigIntCompare
                  0x00ea94                  BigIntMod
                  0x00eb38                  BigIntMultiply
                  0x00eb6c                  BigIntSquare
                  0x00eb90                  BigIntAdd
                  0x00ebb2                  BigIntSubtract
                  0x00ebd4                  BigIntCopy
                  0x00ebf4                  BigIntSwapEndianness

.text             0x00ec08        0x238
 .text            0x00ec08        0x238 Objects - TCPIP Demo App-C30\UARTConfig.o
                  0x00ec08                  DoUARTConfig

.text             0x00ee40        0x236
 .text            0x00ee40        0x236 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\TCPPerformanceTest.o
                  0x00ee40                  TCPTXPerformanceTask
                  0x00ef9c                  TCPRXPerformanceTask
                  0x00f072                  TCPPerformanceTask

.text             0x00f076        0x204
 .text            0x00f076        0x204 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ICMP.o
                  0x00f076                  ICMPProcess
                  0x00f130                  ICMPSendPing
                  0x00f14a                  ICMPSendPingToHost
                  0x00f164                  ICMPGetReply
                  0x00f26a                  ICMPBeginUsage
                  0x00f276                  ICMPEndUsage

.text             0x00f27a        0x1fe
 .text            0x00f27a        0x1fe ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\SNTP.o
                  0x00f27a                  SNTPClient
                  0x00f440                  SNTPGetUTCSeconds

.text             0x00f478        0x1d0
 .text            0x00f478        0x1d0 Objects - TCPIP Demo App-C30\BerkeleyUDPClientDemo.o
                  0x00f478                  BerkeleyUDPClientDemo
                  0x00f610                  BerkeleySNTPGetUTCSeconds

.text             0x00f648        0x1b0
 .text            0x00f648        0x1b0 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\StackTsk.o
                  0x00f648                  StackInit
                  0x00f684                  StackTask
                  0x00f7c8                  StackApplications

.text             0x00f7f8        0x154
 .text            0x00f7f8        0x154 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UART2TCPBridge.o
                  0x00f7f8                  UART2TCPBridgeInit
                  0x00f80a                  UART2TCPBridgeTask
                  0x00f8f4                  _U2RXInterrupt
                  0x00f928                  _U2TXInterrupt

.text             0x00f94c        0x140
 .text            0x00f94c        0x140 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\LCDBlocking.o
                  0x00f982                  LCDInit
                  0x00f9fe                  LCDUpdate
                  0x00fa76                  LCDErase

.text             0x00fa8c        0x138
 .text            0x00fa8c        0x138 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\IP.o
                  0x00fa8c                  IPSetRxBuffer
                  0x00fab8                  IPPutHeader
                  0x00fb40                  IPGetHeader

.text             0x00fbc4        0x12e
 .text            0x00fbc4        0x12e ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Announce.o
                  0x00fbc4                  AnnounceIP
                  0x00fc2c                  DiscoveryTask

.text             0x00fcf2        0x122
 .text            0x00fcf2        0x122 Objects - TCPIP Demo App-C30\GenericTCPClient.o
                  0x00fcf2                  GenericTCPClient

.text             0x00fe14         0xec
 .text            0x00fe14         0xec Objects - TCPIP Demo App-C30\BerkeleyTCPServerDemo.o
                  0x00fe14                  BerkeleyTCPServerDemo

.text             0x00ff00         0xe8
 .text            0x00ff00         0xe8 Objects - TCPIP Demo App-C30\BerkeleyTCPClientDemo.o
                  0x00ff00                  BerkeleyTCPClientDemo

.text             0x00ffe8         0xe6
 .text            0x00ffe8         0xe6 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Tick.o
                  0x00ffe8                  TickInit
                  0x01003e                  TickGet
                  0x010046                  TickGetDiv256
                  0x010076                  TickGetDiv64K
                  0x0100a6                  TickConvertToMilliseconds
                  0x0100ba                  _T1Interrupt

.text             0x0100ce         0xdc
 .text            0x0100ce         0xdc C:\Microchip Solutions\Microchip\TCPIP Stack\BigInt_helper_coff.a(BigInt_helper.o)
                  0x0100ce                  _addBI
                  0x0100ee                  _subBI
                  0x01010e                  _zeroBI
                  0x01011a                  _msbBI
                  0x01012a                  _mulBI
                  0x010160                  _sqrBI
                  0x01016a                  _masBI
                  0x01018c                  _copyBI

.text             0x0101aa         0xce
 .text            0x0101aa         0xce ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\UART.o
                  0x0101aa                  DataRdyUART2
                  0x0101b0                  ReadUART2
                  0x0101c2                  putsUART2
                  0x0101f6                  BusyUART2
                  0x0101fe                  WriteUART2
                  0x01020e                  getsUART2
                  0x010246                  ReadStringUART

.text             0x010278         0xce
 .text            0x010278         0xce Objects - TCPIP Demo App-C30\SMTPDemo.o
                  0x010278                  SMTPDemo

.text             0x010346         0xb8
 .text            0x010346         0xb8 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Reboot.o
                  0x010346                  RebootTask

.text             0x0103fe         0xa0
 .text            0x0103fe         0xa0 Objects - TCPIP Demo App-C30\GenericTCPServer.o
                  0x0103fe                  GenericTCPServer

.text             0x01049e         0xa0
 .text            0x01049e         0xa0 Objects - TCPIP Demo App-C30\PingDemo.o
                  0x01049e                  PingDemo

.text             0x01053e         0x80
 .text            0x01053e         0x80 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\ARCFOUR.o
                  0x01053e                  ARCFOURInitialize
                  0x01057c                  ARCFOURCrypt

.text             0x0105be         0x60
 .text            0x0105be         0x60 ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Random.o
                  0x0105be                  RandomInit
                  0x0105ca                  RandomAdd
                  0x0105f2                  RandomGet

.text             0x01061e         0x4e
 .text            0x01061e         0x4e ..\Microchip\TCPIP Stack\Objects - TCPIP Demo App-C30\Delay.o
                  0x01061e                  Delay10us
                  0x010646                  DelayMs

.isr              0x01066c          0x2
 .isr             0x01066c          0x2 default_isr
                  0x01066c                  _DefaultInterrupt
